(module C_0805 (layer F.Cu) (tedit 59C63004)
  (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
  (tags "capacitor 0805")
  (solder_mask_margin 0.1)
  (attr smd)
  (fp_text reference REF** (at 0 -0.3) (layer F.Fab)
    (effects (font (size 0.4 0.4) (thickness 0.075)))
  )
  (fp_text value VAL** (at 0.05 0.35) (layer F.Fab)
    (effects (font (size 0.4 0.4) (thickness 0.075)))
  )
  (fp_text user REF** (at 0 -1.3) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_line (start 0 -0.625) (end 0 0.625) (layer F.SilkS) (width 0.2))
  (fp_line (start -1.05 0.65) (end -1.05 -0.65) (layer F.Fab) (width 0.1))
  (fp_line (start 1.05 0.65) (end -1.05 0.65) (layer F.Fab) (width 0.1))
  (fp_line (start 1.05 -0.65) (end 1.05 0.65) (layer F.Fab) (width 0.1))
  (fp_line (start -1.05 -0.65) (end 1.05 -0.65) (layer F.Fab) (width 0.1))
  (fp_line (start -1.6 -0.85) (end 1.6 -0.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.6 0.85) (end 1.6 0.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.6 -0.85) (end -1.6 0.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.6 -0.85) (end 1.6 0.85) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -0.95 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1))
  (pad 2 smd rect (at 0.95 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1))
  (model ${KIPRJMOD}/models/c_0805_h078.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
