(module L_0603 (layer F.Cu) (tedit 59AE759B)
  (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
  (tags "resistor 0603")
  (solder_mask_margin 0.1)
  (attr smd)
  (fp_text reference REF** (at 0 -0.2) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.02)))
  )
  (fp_text value VAL** (at 0 0.2) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.02)))
  )
  (fp_text user 0603 (at 0 -0.5) (layer Cmts.User)
    (effects (font (size 0.15 0.15) (thickness 0.0275)))
  )
  (fp_line (start -0.8 -0.45) (end -0.8 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start -0.75 0.45) (end -0.75 -0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start -0.7 -0.45) (end -0.7 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start -0.65 0.45) (end -0.65 -0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start -0.6 -0.45) (end -0.6 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0.8 0.45) (end 0.8 -0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0.75 -0.45) (end 0.75 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0.7 0.45) (end 0.7 -0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0.65 -0.45) (end 0.65 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0.6 -0.45) (end 0.6 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0.55 -0.45) (end 0.55 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start -0.55 -0.45) (end -0.55 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start -0.85 0.45) (end -0.85 -0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0.85 0.45) (end -0.85 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0.85 -0.45) (end 0.85 0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start -0.85 -0.45) (end 0.85 -0.45) (layer Dwgs.User) (width 0.05))
  (fp_line (start -1.15 -0.6) (end 1.15 -0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.15 0.6) (end 1.15 0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.15 -0.6) (end -1.15 0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.15 -0.6) (end 1.15 0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 0.45) (end 0 -0.45) (layer F.SilkS) (width 0.2))
  (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.05))
  (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.05))
  (fp_line (start -0.6 0.4) (end -0.6 -0.4) (layer F.Fab) (width 0.05))
  (fp_line (start -0.65 -0.4) (end -0.65 0.4) (layer F.Fab) (width 0.05))
  (fp_line (start -0.7 0.4) (end -0.7 -0.4) (layer F.Fab) (width 0.05))
  (fp_line (start -0.75 -0.4) (end -0.75 0.4) (layer F.Fab) (width 0.05))
  (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.05))
  (fp_line (start -0.5 -0.4) (end -0.5 0.4) (layer F.Fab) (width 0.05))
  (fp_line (start -0.55 -0.4) (end -0.55 0.4) (layer F.Fab) (width 0.05))
  (fp_line (start 0.7 0.4) (end 0.7 -0.4) (layer F.Fab) (width 0.05))
  (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.05))
  (fp_line (start 0.75 -0.4) (end 0.75 0.4) (layer F.Fab) (width 0.05))
  (fp_line (start 0.5 0.4) (end 0.5 -0.4) (layer F.Fab) (width 0.05))
  (fp_line (start 0.6 0.4) (end 0.6 -0.4) (layer F.Fab) (width 0.05))
  (fp_line (start 0.65 -0.4) (end 0.65 0.4) (layer F.Fab) (width 0.05))
  (fp_line (start 0.55 -0.4) (end 0.55 0.4) (layer F.Fab) (width 0.05))
  (pad 1 smd roundrect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.15))
  (pad 2 smd roundrect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.15))
  (model Resistors_SMD.3dshapes/R_0603.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
