(module SiliconLabs_QFN-20-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 5AC77ADD)
  (descr "20-Lead Plastic Quad Flat, No Lead Package - 3x3 mm Body [QFN] with corner pads; see figure 8.2 of https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf")
  (tags "QFN 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SiliconLabs_QFN-20-1EP_3x3mm_Pitch0.5mm (at 0 3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 1.5) (end -1.5 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -0.5) (end -0.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.25 -2.25) (end -2.25 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.25 2.25) (end 2.25 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.25 2.25) (end 2.25 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.25 -2.25) (end -2.25 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.16 -1.66) (end 1.66 -1.66) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.66 -1.66) (end 1.66 -1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.16 1.66) (end -1.66 1.66) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.66 1.66) (end -1.66 1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.16 1.66) (end 1.66 1.66) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.66 1.66) (end 1.66 1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.66 -1.66) (end -1.16 -1.66) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.65 0.65) (thickness 0.125)))
  )
  (pad 1 smd roundrect (at -1.25 -1.25) (size 0.33 0.33) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25)
   (solder_mask_margin 0.07))
  (pad 2 smd oval (at -1.55 -0.75) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 3 smd oval (at -1.55 -0.25) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 4 smd oval (at -1.55 0.25) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 5 smd oval (at -1.55 0.75) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 6 smd roundrect (at -1.25 1.25) (size 0.33 0.33) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25)
   (solder_mask_margin 0.07))
  (pad 7 smd oval (at -0.75 1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 8 smd oval (at -0.25 1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 9 smd oval (at 0.25 1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 10 smd oval (at 0.75 1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 11 smd roundrect (at 1.25 1.25) (size 0.33 0.33) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25)
   (solder_mask_margin 0.07))
  (pad 12 smd oval (at 1.55 0.75) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 13 smd oval (at 1.55 0.25) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 14 smd oval (at 1.55 -0.25) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 15 smd oval (at 1.55 -0.75) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 16 smd roundrect (at 1.25 -1.25) (size 0.33 0.33) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25)
   (solder_mask_margin 0.07))
  (pad 17 smd oval (at 0.75 -1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 18 smd oval (at 0.25 -1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 19 smd oval (at -0.25 -1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 20 smd oval (at -0.75 -1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask)
   (solder_mask_margin 0.07))
  (pad 21 smd rect (at 0 0) (size 1.8 1.8) (layers F.Cu F.Mask)
   (solder_mask_margin 0.001))
  (pad "" smd rect (at -0.45 -0.45) (size 0.54 0.54) (layers F.Paste))
  (pad "" smd rect (at -0.45 0.45) (size 0.54 0.54) (layers F.Paste))
  (pad "" smd rect (at 0.45 -0.45) (size 0.54 0.54) (layers F.Paste))
  (pad "" smd rect (at 0.45 0.45) (size 0.54 0.54) (layers F.Paste))
  (model ${KIPRJMOD}/models/QFN/QFN16_3x3_p0_5mm.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
