From bdb12383a58d6989a0b1c2f925890948146bbc90 Mon Sep 17 00:00:00 2001
From: Pauli Virtanen <pav@iki.fi>
Date: Mon, 26 Jul 2021 21:02:06 +0300
Subject: [PATCH 2/2] Bluetooth: btusb: check conditions before enabling USB
 ALT 3 for WBS
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Some USB BT adapters don't satisfy the MTU requirement mentioned in
commit e848dbd364ac ("Bluetooth: btusb: Add support USB ALT 3 for WBS")
and have ALT 3 setting that produces no/garbled audio. Some adapters
with larger MTU were also reported to have problems with ALT 3.

Add a flag and check it and MTU before selecting ALT 3, falling back to
ALT 1. Enable the flag for Realtek, restoring the previous behavior for
non-Realtek devices.

Tested with USB adapters (mtu<72, no/garbled sound with ALT3, ALT1
works) BCM20702A1 0b05:17cb, CSR8510A10 0a12:0001, and (mtu>=72, ALT3
works) RTL8761BU 0bda:8771, Intel AX200 8087:0029 (after disabling
ALT6). Also got reports for (mtu>=72, ALT 3 reported to produce bad
audio) Intel 8087:0a2b.

Signed-off-by: Pauli Virtanen <pav@iki.fi>
Fixes: e848dbd364ac ("Bluetooth: btusb: Add support USB ALT 3 for WBS")
Tested-by: Michał Kępień <kernel@kempniu.pl>

Fixes: https://bugs.archlinux.org/task/71567
---
 drivers/bluetooth/btusb.c | 22 ++++++++++++++--------
 1 file changed, 14 insertions(+), 8 deletions(-)

diff --git a/drivers/bluetooth/btusb.c b/drivers/bluetooth/btusb.c
index 6d23308119d1..e8062d0b7d4d 100644
--- a/drivers/bluetooth/btusb.c
+++ b/drivers/bluetooth/btusb.c
@@ -516,6 +516,7 @@ static const struct dmi_system_id btusb_needs_reset_resume_table[] = {
 #define BTUSB_HW_RESET_ACTIVE	12
 #define BTUSB_TX_WAIT_VND_EVT	13
 #define BTUSB_WAKEUP_DISABLE	14
+#define BTUSB_USE_ALT3_FOR_WBS	15
 
 struct btusb_data {
 	struct hci_dev       *hdev;
@@ -1748,16 +1749,20 @@ static void btusb_work(struct work_struct *work)
 			/* Bluetooth USB spec recommends alt 6 (63 bytes), but
 			 * many adapters do not support it.  Alt 1 appears to
 			 * work for all adapters that do not have alt 6, and
-			 * which work with WBS at all.
+			 * which work with WBS at all.  Some devices prefer
+			 * alt 3 (HCI payload >= 60 Bytes let air packet
+			 * data satisfy 60 bytes), requiring
+			 * MTU >= 3 (packets) * 25 (size) - 3 (headers) = 72
+			 * see also Core spec 5, vol 4, B 2.1.1 & Table 2.1.
 			 */
-			new_alts = btusb_find_altsetting(data, 6) ? 6 : 1;
-			/* Because mSBC frames do not need to be aligned to the
-			 * SCO packet boundary. If support the Alt 3, use the
-			 * Alt 3 for HCI payload >= 60 Bytes let air packet
-			 * data satisfy 60 bytes.
-			 */
-			if (new_alts == 1 && btusb_find_altsetting(data, 3))
+			if (btusb_find_altsetting(data, 6))
+				new_alts = 6;
+			else if (test_bit(BTUSB_USE_ALT3_FOR_WBS, &data->flags) &&
+					hdev->sco_mtu >= 72 &&
+					btusb_find_altsetting(data, 3))
 				new_alts = 3;
+			else
+				new_alts = 1;
 		}
 
 		if (btusb_switch_alt_setting(hdev, new_alts) < 0)
@@ -4733,6 +4738,7 @@ static int btusb_probe(struct usb_interface *intf,
 		 * (DEVICE_REMOTE_WAKEUP)
 		 */
 		set_bit(BTUSB_WAKEUP_DISABLE, &data->flags);
+		set_bit(BTUSB_USE_ALT3_FOR_WBS, &data->flags);
 	}
 
 	if (!reset)
-- 
2.32.0

