From 4cc924c3e3a0d53306d08b04720c427d1c298ba8 Mon Sep 17 00:00:00 2001
From: Julien Grall <jgrall@amazon.com>
Date: Wed, 5 Jan 2022 18:09:20 +0000
Subject: [PATCH] passthrough/x86: stop pirq iteration immediately in case of
 error

pt_pirq_iterate() will iterate in batch over all the PIRQs. The outer
loop will bail out if 'rc' is non-zero but the inner loop will continue.

This means 'rc' will get clobbered and we may miss any errors (such as
-ERESTART in the case of the callback pci_clean_dpci_irq()).

This is CVE-2022-23035 / XSA-395.

Fixes: c24536b636f2 ("replace d->nr_pirqs sized arrays with radix tree")
Fixes: f6dd295381f4 ("dpci: replace tasklet with softirq")
Signed-off-by: Julien Grall <jgrall@amazon.com>
Signed-off-by: Jan Beulich <jbeulich@suse.com>
Reviewed-by: Roger Pau Monné <roger.pau@citrix.com>
---
 xen/drivers/passthrough/x86/hvm.c | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/xen/drivers/passthrough/x86/hvm.c b/xen/drivers/passthrough/x86/hvm.c
index 351daafdc9bf..0b37cd145b60 100644
--- a/xen/drivers/passthrough/x86/hvm.c
+++ b/xen/drivers/passthrough/x86/hvm.c
@@ -732,7 +732,11 @@ int pt_pirq_iterate(struct domain *d,
 
             pirq = pirqs[i]->pirq;
             if ( (pirq_dpci->flags & HVM_IRQ_DPCI_MAPPED) )
+            {
                 rc = cb(d, pirq_dpci, arg);
+                if ( rc )
+                    break;
+            }
         }
     } while ( !rc && ++pirq < d->nr_pirqs && n == ARRAY_SIZE(pirqs) );
 
-- 
2.32.0

