From 7ff58ab770157a03c92604155a0c745bcab834c2 Mon Sep 17 00:00:00 2001
From: Julien Grall <jgrall@amazon.com>
Date: Tue, 14 Dec 2021 09:53:44 +0000
Subject: [PATCH] xen/arm: p2m: Always clear the P2M entry when the mapping is
 removed

Commit 2148a125b73b ("xen/arm: Track page accessed between batch of
Set/Way operations") allowed an entry to be invalid from the CPU PoV
(lpae_is_valid()) but valid for Xen (p2m_is_valid()). This is useful
to track which page is accessed and only perform an action on them
(e.g. clean & invalidate the cache after a set/way instruction).

Unfortunately, __p2m_set_entry() is only zeroing the P2M entry when
lpae_is_valid() returns true. This means the entry will not be zeroed
if the entry was valid from Xen PoV but invalid from the CPU PoV for
tracking purpose.

As a consequence, this will allow a domain to continue to access the
page after it was removed.

Resolve the issue by always zeroing the entry if it the LPAE bit is
set or the entry is about to be removed.

This is CVE-2022-23033 / XSA-393.

Reported-by: Dmytro Firsov <Dmytro_Firsov@epam.com>
Fixes: 2148a125b73b ("xen/arm: Track page accessed between batch of Set/Way operations")
Reviewed-by: Stefano Stabellini <sstabellini@kernel.org>
Signed-off-by: Julien Grall <jgrall@amazon.com>
---
 xen/arch/arm/p2m.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/xen/arch/arm/p2m.c b/xen/arch/arm/p2m.c
index 8b20b430777e..fb71fa4c1c90 100644
--- a/xen/arch/arm/p2m.c
+++ b/xen/arch/arm/p2m.c
@@ -1016,7 +1016,7 @@ static int __p2m_set_entry(struct p2m_domain *p2m,
      * sequence when updating the translation table (D4.7.1 in ARM DDI
      * 0487A.j).
      */
-    if ( lpae_is_valid(orig_pte) )
+    if ( lpae_is_valid(orig_pte) || removing_mapping )
         p2m_remove_pte(entry, p2m->clean_pte);
 
     if ( removing_mapping )
-- 
2.32.0

