From 52422e37bb199fa5c62881cdf26c687aa692d063 Mon Sep 17 00:00:00 2001
From: Jeroen Hofstee <jeroen@myspectrum.nl>
Date: Wed, 8 Oct 2014 22:57:53 +0200
Subject: [PATCH] leds: missing include

Signed-off-by: Jeroen Hofstee <jeroen@myspectrum.nl>
---
 arch/arm/cpu/arm926ejs/at91/led.c | 1 +
 arch/arm/lib/board.c              | 1 +
 board/atmel/at91rm9200ek/led.c    | 1 +
 board/atmel/at91sam9260ek/led.c   | 1 +
 4 files changed, 4 insertions(+)

diff --git a/arch/arm/cpu/arm926ejs/at91/led.c b/arch/arm/cpu/arm926ejs/at91/led.c
index 46ed055..b8d5c78 100644
--- a/arch/arm/cpu/arm926ejs/at91/led.c
+++ b/arch/arm/cpu/arm926ejs/at91/led.c
@@ -9,6 +9,7 @@
 #include <common.h>
 #include <asm/gpio.h>
 #include <asm/arch/gpio.h>
+#include <status_led.h>
 
 #ifdef CONFIG_RED_LED
 void red_led_on(void)
diff --git a/arch/arm/lib/board.c b/arch/arm/lib/board.c
index 98782ca..f606255 100644
--- a/arch/arm/lib/board.c
+++ b/arch/arm/lib/board.c
@@ -34,6 +34,7 @@
 #include <nand.h>
 #include <onenand_uboot.h>
 #include <mmc.h>
+#include <status_led.h>
 #include <libfdt.h>
 #include <fdtdec.h>
 #include <post.h>
diff --git a/board/atmel/at91rm9200ek/led.c b/board/atmel/at91rm9200ek/led.c
index 2298e36..6761b14 100644
--- a/board/atmel/at91rm9200ek/led.c
+++ b/board/atmel/at91rm9200ek/led.c
@@ -14,6 +14,7 @@
 #include <asm/arch/hardware.h>
 #include <asm/arch/at91_pmc.h>
 #include <asm/arch/at91_pio.h>
+#include <status_led.h>
 
 /* bit mask in PIO port B */
 #define	GREEN_LED	(1<<0)
diff --git a/board/atmel/at91sam9260ek/led.c b/board/atmel/at91sam9260ek/led.c
index 56d811c..fbe15af 100644
--- a/board/atmel/at91sam9260ek/led.c
+++ b/board/atmel/at91sam9260ek/led.c
@@ -9,6 +9,7 @@
 #include <common.h>
 #include <asm/io.h>
 #include <asm/arch/gpio.h>
+#include <status_led.h>
 
 void coloured_LED_init(void)
 {
