diff --git a/u-boot-2014.07.orig/include/configs/chiliboard.h b/u-boot-2014.07/include/configs/chiliboard.h
index eacc9af..137ce89 100644
--- a/u-boot-2014.07.orig/include/configs/chiliboard.h
+++ b/u-boot-2014.07/include/configs/chiliboard.h
@@ -124,7 +124,6 @@
  * as that will normally be within the kernel lowmem and thus visible via
  * bootm_size and we only run on platforms with 256MB or more of memory.
  */
-#ifdef CONFIG_RAM128MB
 #define DEFAULT_LINUX_BOOT_ENV \
 	"loadaddr=0x82000000\0" \
 	"kernel_addr_r=0x82000000\0" \
@@ -133,16 +132,6 @@
 	"rdaddr=0x84080000\0" \
 	"ramdisk_addr_r=0x84080000\0" \
 	"bootm_size=0x8000000\0"
-#else
-#define DEFAULT_LINUX_BOOT_ENV \
-	"loadaddr=0x82000000\0" \
-	"kernel_addr_r=0x82000000\0" \
-	"fdtaddr=0x88000000\0" \
-	"fdt_addr_r=0x88000000\0" \
-	"rdaddr=0x88080000\0" \
-	"ramdisk_addr_r=0x88080000\0" \
-	"bootm_size=0x10000000\0"
-#endif
 
 /*
  * Default to a quick boot delay.
@@ -258,6 +247,7 @@
 #define CONFIG_CMD_ASKENV
 #define CONFIG_CMD_ECHO
 #define CONFIG_CMD_BOOTZ
+#define CONFIG_SUPPORT_RAW_INITRD
 
 /*
  * Common filesystems support.  When we have removable storage we
@@ -398,6 +388,9 @@
 #define CONFIG_EFI_PARTITION
 #define CONFIG_PARTITION_UUIDS
 #define CONFIG_CMD_PART
+#define CONFIG_CMD_SETEXPR
+
+#define CONFIG_IDENT_STRING 	" Parabola GNU/Linux-libre"
 
 #ifdef CONFIG_NAND
 #ifndef CONFIG_NAND512MB
@@ -441,18 +434,16 @@
 #define CONFIG_EXTRA_ENV_SETTINGS \
 	DEFAULT_LINUX_BOOT_ENV \
 	"boot_fdt=try\0" \
-	"bootpart=0:2\0" \
+	"bootpart=0:1\0" \
 	"bootdir=/boot\0" \
-	"bootfile=zImage\0" \
-	"fdtfile=undefined\0" \
+	"fdtdir=/boot/dtbs/linux-libre\0" \
+	"bootfile=vmlinuz-linux-libre\0" \
+	"fdtfile=\0" \
 	"console=ttyO0,115200n8\0" \
 	"partitions=" \
 		"uuid_disk=${uuid_gpt_disk};" \
 		"name=rootfs,start=2MiB,size=-,uuid=${uuid_gpt_rootfs}\0" \
 	"optargs=\0" \
-	"mmcdev=0\0" \
-	"mmcroot=/dev/mmcblk0p2 rw\0" \
-	"mmcrootfstype=ext4 rootwait\0" \
 	"rootpath=/export/rootfs\0" \
 	"nfsopts=nolock\0" \
 	"static_ip=${ipaddr}:${serverip}:${gatewayip}:${netmask}:${hostname}" \
@@ -461,8 +452,7 @@
 	"ramrootfstype=ext2\0" \
 	"mmcargs=setenv bootargs console=${console} " \
 		"${optargs} " \
-		"root=${mmcroot} " \
-		"rootfstype=${mmcrootfstype}\0" \
+		"root=${root}\0" \
 	"spiroot=/dev/mtdblock4 rw\0" \
 	"spirootfstype=jffs2\0" \
 	"spisrcaddr=0xe0000\0" \
@@ -477,46 +467,47 @@
 		"root=/dev/nfs " \
 		"nfsroot=${serverip}:${rootpath},${nfsopts} rw " \
 		"ip=dhcp\0" \
-	"bootenv=uEnv.txt\0" \
-	"loadbootenv=load mmc ${mmcdev} ${loadaddr} ${bootenv}\0" \
-	"importbootenv=echo Importing environment from mmc ...; " \
-		"env import -t $loadaddr $filesize\0" \
 	"ramargs=setenv bootargs console=${console} " \
 		"${optargs} " \
 		"root=${ramroot} " \
 		"rootfstype=${ramrootfstype}\0" \
-	"loadramdisk=load mmc ${mmcdev} ${rdaddr} ramdisk.gz\0" \
-	"loadimage=load mmc ${bootpart} ${loadaddr} ${bootdir}/${bootfile}\0" \
-	"loadfdt=load mmc ${bootpart} ${fdtaddr} ${bootdir}/${fdtfile}\0" \
-	"mmcloados=run mmcargs; " \
-		"if test ${boot_fdt} = yes || test ${boot_fdt} = try; then " \
-			"if run loadfdt; then " \
-				"bootz ${loadaddr} - ${fdtaddr}; " \
-			"else " \
-				"if test ${boot_fdt} = try; then " \
-					"bootz; " \
-				"else " \
-					"echo WARN: Cannot load the DT; " \
-				"fi; " \
-			"fi; " \
-		"else " \
-			"bootz; " \
-		"fi;\0" \
-	"mmcboot=mmc dev ${mmcdev}; " \
-		"if mmc rescan; then " \
-			"echo SD/MMC found on device ${mmcdev};" \
-			"if run loadbootenv; then " \
-				"echo Loaded environment from ${bootenv};" \
-				"run importbootenv;" \
-			"fi;" \
-			"if test -n $uenvcmd; then " \
-				"echo Running uenvcmd ...;" \
-				"run uenvcmd;" \
-			"fi;" \
-			"if run loadimage; then " \
-				"run mmcloados;" \
-			"fi;" \
-		"fi;\0" \
+	"loadimage=load ${devtype} ${bootpart} ${loadaddr} ${bootdir}/${bootfile}\0" \
+	"loadrd=load ${devtype} ${bootpart} ${rdaddr} ${bootdir}/${rdfile}\0" \
+	"loadfdt=echo loading ${fdtdir}/${fdtfile} ...; load ${devtype} ${bootpart} ${fdtaddr} ${fdtdir}/${fdtfile}\0" \
+	"mmcboot=for devtype in mmc; do " \
+			"for devnum in 0 1; do " \
+				"if ${devtype} dev ${devnum}; then " \
+					"echo ${devtype} found on device ${devnum};" \
+					"setenv bootpart ${devnum}:1;" \
+					"part uuid ${devtype} ${bootpart} uuid;" \
+					"setenv root PARTUUID=${uuid} rw rootwait;" \
+					"echo Checking for: ${bootdir}/uEnv.txt ...;" \
+					"if test -e ${devtype} ${bootpart} ${bootdir}/uEnv.txt; then " \
+						"load ${devtype} ${bootpart} ${loadaddr} ${bootdir}/uEnv.txt;" \
+						"env import -t ${loadaddr} ${filesize};" \
+						"echo Loaded environment from ${bootdir}/uEnv.txt;" \
+						"echo Checking if uenvcmd is set ...;" \
+						"if test -n ${uenvcmd}; then " \
+							"echo Running uenvcmd ...;" \
+							"run uenvcmd;" \
+						"fi;" \
+					"fi;" \
+					"if run loadimage; then " \
+						"run mmcargs;" \
+						"if run loadfdt; then " \
+							"if run loadrd; then " \
+								"bootz ${loadaddr} ${rdaddr}:${filesize} ${fdtaddr};" \
+							"else " \
+								"bootz ${loadaddr} - ${fdtaddr};" \
+							"fi;" \
+						"fi;" \
+					"else " \
+						"echo No kernel found;" \
+					"fi;" \
+					"setexpr devnum ${devnum} + 1;" \
+				"fi;" \
+			"done;" \
+		"done;\0" \
 	"spiboot=echo Booting from spi ...; " \
 		"run spiargs; " \
 		"sf probe ${spibusno}:0; " \
@@ -541,9 +532,6 @@
 #define CONFIG_BOOTCOMMAND \
 	"run findfdt; " \
 	"run mmcboot;" \
-	"setenv mmcdev 1; " \
-	"setenv bootpart 1:2; " \
-	"run mmcboot;" \
 	"run nandboot;"
 
 /* NS16550 Configuration */
