From d020dc63065a58f4be4817cba4a36da8334ddafb Mon Sep 17 00:00:00 2001
From: Kevin Mihelich <kevin@archlinuxarm.org>
Date: Thu, 11 Aug 2016 00:42:37 -0600
Subject: [PATCH 7/9] exynos4412-odroid: set higher minimum buck2 regulator
 voltage

Set a higher minimum voltage to help reboot issue.
http://www.spinics.net/lists/linux-samsung-soc/msg54434.html

Signed-off-by: Kevin Mihelich <kevin@archlinuxarm.org>
---
 arch/arm/boot/dts/exynos4412-odroid-common.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/exynos4412-odroid-common.dtsi b/arch/arm/boot/dts/exynos4412-odroid-common.dtsi
index 2983e91bc7dd..fbf6c172becf 100644
--- a/arch/arm/boot/dts/exynos4412-odroid-common.dtsi
+++ b/arch/arm/boot/dts/exynos4412-odroid-common.dtsi
@@ -435,7 +435,7 @@ buck1_reg: BUCK1 {
 
 			buck2_reg: BUCK2 {
 				regulator-name = "VDD_ARM";
-				regulator-min-microvolt = <900000>;
+				regulator-min-microvolt = <1100000>;
 				regulator-max-microvolt = <1350000>;
 				regulator-always-on;
 				regulator-boot-on;
-- 
2.30.0

