From c22b09283934f39b059b42e3c29985ba81bc8af7 Mon Sep 17 00:00:00 2001
From: Kevin Mihelich <kevin@archlinuxarm.org>
Date: Sat, 14 Feb 2015 12:32:27 +0100
Subject: [PATCH 6/9] set default cubietruck led triggers

Signed-off-by: Kevin Mihelich <kevin@archlinuxarm.org>
---
 arch/arm/boot/dts/sun7i-a20-cubietruck.dts | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
index 9109ca0919ad..43460add4609 100644
--- a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
@@ -78,6 +78,7 @@ leds {
 		blue {
 			label = "cubietruck:blue:usr";
 			gpios = <&pio 7 21 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "heartbeat";
 		};
 
 		orange {
@@ -93,6 +94,7 @@ white {
 		green {
 			label = "cubietruck:green:usr";
 			gpios = <&pio 7 7 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "mmc0";
 		};
 	};
 
-- 
2.30.0

