# Config file for /etc/init.d/busybox-watchdog

# run "/sbin/watchdog --help" to see all possible options.

# Periodically write to watchdog device
WATCHDOG_OPTS="/dev/watchdog"

# optionally set the nice-level
#SSD_NICELEVEL="-20"
