# Hotplug device map for GPSD
#
# This file is Copyright 2010 by the GPSD project
# SPDX-License-Identifier: BSD-2-clause
#
# GPSes don't have their own USB device class.  They're serial-over-USB
# devices, so what you see is actually the ID of the serial-over-USB chip.
# Fortunately, just two of these account for over 80% of consumer-grade
# GPS sensors.  The gpsdplug script will tell a running gpsd that it should
# look at the device that just went active, because it might be a GPS.
#
# The Prolific Technology 2303 (commonly in tandem with SiRF chips)
gpsd.hotplug 0x0003 0x067b 0x2303 0x0000 0x0000 0x00 0x00 0x00 0x00 0x00 0x00 0x00000000
# FTDI 8U232AM
gpsd.hotplug 0x0003 0x0403 0x6001 0x0000 0x0000 0x00 0x00 0x00 0x00 0x00 0x00 0x00000000
# Cypress M8/CY7C64013 (DeLorme uses these)
gpsd.hotplug 0x0003 0x1163 0x0100 0x0000 0x0000 0x00 0x00 0x00 0x00 0x00 0x00 0x00000000
# PS-360 OEM (Microsoft GPS sold with Street and Trips 2005)
gpsd.hotplug 0x0003 0x067b 0xaaa0 0x0000 0x0000 0x00 0x00 0x00 0x00 0x00 0x00 0x00000000

# vim: set expandtab shiftwidth=4
