

For f2a85 BIOS rev 5103 (an older version):

# dmidecode 2.11
SMBIOS 2.7 present.
66 structures occupying 2602 bytes.
Table at 0x000EB330.

Handle 0x0000, DMI type 0, 24 bytes
BIOS Information
    Vendor: American Megatrends Inc.
    Version: 5103
    Release Date: 09/19/2012
    Address: 0xF0000
    Runtime Size: 64 kB
    ROM Size: 8192 kB
    Characteristics:
        PCI is supported
        BIOS is upgradeable
        BIOS shadowing is allowed
        Boot from CD is supported
        Selectable boot is supported
        BIOS ROM is socketed
        EDD is supported
        5.25"/1.2 MB floppy services are supported (int 13h)
        3.5"/720 kB floppy services are supported (int 13h)
        3.5"/2.88 MB floppy services are supported (int 13h)
        Print screen service is supported (int 5h)
        8042 keyboard services are supported (int 9h)
        Serial services are supported (int 14h)
        Printer services are supported (int 17h)
        ACPI is supported
        USB legacy is supported
        BIOS boot specification is supported
        Targeted content distribution is supported
        UEFI is supported
    BIOS Revision: 4.6

Handle 0x0001, DMI type 1, 27 bytes
System Information
    Manufacturer: System manufacturer
    Product Name: System Product Name
    Version: System Version
    Serial Number: System Serial Number
    UUID: 4E5BFAA0-1609-11E0-B25A-50465D90D676
    Wake-up Type: Power Switch
    SKU Number: SKU
    Family: To be filled by O.E.M.

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
    Manufacturer: ASUSTeK COMPUTER INC.
    Product Name: F2A85-M
    Version: Rev X.0x
    Serial Number: 121002909202970
    Asset Tag: To be filled by O.E.M.
    Features:
        Board is a hosting board
        Board is replaceable
    Location In Chassis: To be filled by O.E.M.
    Chassis Handle: 0x0003
    Type: Motherboard
    Contained Object Handles: 0

Handle 0x0003, DMI type 3, 22 bytes
Chassis Information
    Manufacturer: Chassis Manufacture
    Type: Desktop
    Lock: Not Present
    Version: Chassis Version
    Serial Number: Chassis Serial Number
    Asset Tag: Asset-1234567890
    Boot-up State: Safe
    Power Supply State: Safe
    Thermal State: Safe
    Security Status: None
    OEM Information: 0x00000000
    Height: Unspecified
    Number Of Power Cords: 1
    Contained Elements: 0
    SKU Number: To be filled by O.E.M.

Handle 0x0004, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: PS/2 Keyboard/Mouse
    Internal Connector Type: None
    External Reference Designator: PS/2 Keyboard/Mouse
    External Connector Type: PS/2
    Port Type: Keyboard Port

Handle 0x0005, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: USB34
    Internal Connector Type: None
    External Reference Designator: USB34
    External Connector Type: Access Bus (USB)
    Port Type: USB

Handle 0x0006, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SPDIFO
    Internal Connector Type: None
    External Reference Designator: SPDIFO
    External Connector Type: Other
    Port Type: Other

Handle 0x0007, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: HDMI
    Internal Connector Type: None
    External Reference Designator: HDMI port
    External Connector Type: Other
    Port Type: Other

Handle 0x0008, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: D-SUB
    Internal Connector Type: None
    External Reference Designator: D-SUB port
    External Connector Type: Other
    Port Type: Other

Handle 0x0009, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: DVI
    Internal Connector Type: None
    External Reference Designator: DVI port
    External Connector Type: Other
    Port Type: Other

Handle 0x000A, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: ESATA
    Internal Connector Type: None
    External Reference Designator: ESATA
    External Connector Type: SAS/SATA Plug Receptacle
    Port Type: SATA

Handle 0x000B, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: USB3_12
    Internal Connector Type: None
    External Reference Designator: USB3_12
    External Connector Type: Access Bus (USB)
    Port Type: USB

Handle 0x000C, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: LAN
    Internal Connector Type: None
    External Reference Designator: LAN
    External Connector Type: RJ-45
    Port Type: Network Port

Handle 0x000D, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: USB12
    Internal Connector Type: None
    External Reference Designator: USB12
    External Connector Type: Access Bus (USB)
    Port Type: USB

Handle 0x000E, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: Audio_Line_In
    Internal Connector Type: None
    External Reference Designator: Audio_Line_In
    External Connector Type: Mini Jack (headphones)
    Port Type: Audio Port

Handle 0x000F, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: Audio_Line_Out
    Internal Connector Type: None
    External Reference Designator: Audio_Line_Out
    External Connector Type: Mini Jack (headphones)
    Port Type: Audio Port

Handle 0x0010, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: Audio_Mic_In
    Internal Connector Type: None
    External Reference Designator: Audio_Mic_In
    External Connector Type: Mini Jack (headphones)
    Port Type: Audio Port

Handle 0x0011, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: Audio_Center/Sub
    Internal Connector Type: None
    External Reference Designator: Audio_Center/Sub
    External Connector Type: Mini Jack (headphones)
    Port Type: Audio Port

Handle 0x0012, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: Audio_Rear
    Internal Connector Type: None
    External Reference Designator: Audio_Rear
    External Connector Type: Mini Jack (headphones)
    Port Type: Audio Port

Handle 0x0013, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: Audio_Side
    Internal Connector Type: None
    External Reference Designator: Audio_Side
    External Connector Type: Mini Jack (headphones)
    Port Type: Audio Port

Handle 0x0014, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SATA6G_1
    Internal Connector Type: SAS/SATA Plug Receptacle
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: SATA

Handle 0x0015, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SATA6G_2
    Internal Connector Type: SAS/SATA Plug Receptacle
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: SATA

Handle 0x0016, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SATA6G_3
    Internal Connector Type: SAS/SATA Plug Receptacle
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: SATA

Handle 0x0017, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SATA6G_4
    Internal Connector Type: SAS/SATA Plug Receptacle
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: SATA

Handle 0x0018, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SATA6G_5
    Internal Connector Type: SAS/SATA Plug Receptacle
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: SATA

Handle 0x0019, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SATA6G_6
    Internal Connector Type: SAS/SATA Plug Receptacle
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: SATA

Handle 0x001A, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SATA6G_7
    Internal Connector Type: SAS/SATA Plug Receptacle
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: SATA

Handle 0x001B, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: ESATA6G
    Internal Connector Type: SAS/SATA Plug Receptacle
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: SATA

Handle 0x001C, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: USB3_34
    Internal Connector Type: Access Bus (USB)
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: USB

Handle 0x001D, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: USB78
    Internal Connector Type: Access Bus (USB)
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: USB

Handle 0x001E, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: USB910
    Internal Connector Type: Access Bus (USB)
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: USB

Handle 0x001F, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: USB34
    Internal Connector Type: Access Bus (USB)
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: USB

Handle 0x0020, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: USB56
    Internal Connector Type: Access Bus (USB)
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: USB

Handle 0x0021, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: PANEL
    Internal Connector Type: Other
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: Other

Handle 0x0022, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: COM1
    Internal Connector Type: 9 Pin Dual Inline (pin 10 cut)
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: Other

Handle 0x0023, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: SPDIF_OUT
    Internal Connector Type: Other
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: Other

Handle 0x0024, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: AAFP
    Internal Connector Type: Mini Jack (headphones)
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: Audio Port

Handle 0x0025, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: CPU_FAN
    Internal Connector Type: Other
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: Other

Handle 0x0026, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: CHA_FAN
    Internal Connector Type: Other
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: Other

Handle 0x0027, DMI type 8, 9 bytes
Port Connector Information
    Internal Reference Designator: PWR_FAN
    Internal Connector Type: Other
    External Reference Designator: Not Specified
    External Connector Type: None
    Port Type: Other

Handle 0x0028, DMI type 9, 17 bytes
System Slot Information
    Designation: PCIEX16_1
    Type: 32-bit PCI Express
    Current Usage: In Use
    Length: Short
    ID: 1
    Characteristics:
        3.3 V is provided
        Opening is shared
        PME signal is supported
    Bus Address: 0000:00:01.0

Handle 0x0029, DMI type 9, 17 bytes
System Slot Information
    Designation: PCIEX1_2
    Type: 32-bit PCI Express
    Current Usage: In Use
    Length: Short
    ID: 2
    Characteristics:
        3.3 V is provided
        Opening is shared
        PME signal is supported
    Bus Address: 0000:00:1c.4

Handle 0x002A, DMI type 9, 17 bytes
System Slot Information
    Designation: PCI1
    Type: 32-bit PCI
    Current Usage: In Use
    Length: Short
    ID: 3
    Characteristics:
        3.3 V is provided
        Opening is shared
        PME signal is supported
    Bus Address: 0000:00:1c.6

Handle 0x002B, DMI type 9, 17 bytes
System Slot Information
    Designation: PCIEX16_2
    Type: 32-bit PCI Express
    Current Usage: In Use
    Length: Short
    ID: 4
    Characteristics:
        3.3 V is provided
        Opening is shared
        PME signal is supported
    Bus Address: 0000:00:01.0

Handle 0x002C, DMI type 10, 10 bytes
On Board Device 1 Information
    Type: Video
    Status: Enabled
    Description:    To Be Filled By O.E.M.
On Board Device 2 Information
    Type: Ethernet
    Status: Enabled
    Description: To Be Filled By O.E.M.
On Board Device 3 Information
    Type: Sound
    Status: Enabled
    Description:    To Be Filled By O.E.M.

Handle 0x002D, DMI type 11, 5 bytes
OEM Strings
    String 1: To Be Filled By O.E.M.

Handle 0x002E, DMI type 12, 5 bytes
System Configuration Options
    Option 1: To Be Filled By O.E.M.

Handle 0x002F, DMI type 16, 23 bytes
Physical Memory Array
    Location: System Board Or Motherboard
    Use: System Memory
    Error Correction Type: None
    Maximum Capacity: 8 GB
    Error Information Handle: Not Provided
    Number Of Devices: 4

Handle 0x0030, DMI type 19, 31 bytes
Memory Array Mapped Address
    Starting Address: 0x00000000000
    Ending Address: 0x003FFFFFFFF
    Range Size: 16 GB
    Physical Array Handle: 0x002F
    Partition Width: 255

Handle 0x0031, DMI type 17, 34 bytes
Memory Device
    Array Handle: 0x002F
    Error Information Handle: Not Provided
    Total Width: 64 bits
    Data Width: 64 bits
    Size: 4096 MB
    Form Factor: DIMM
    Set: None
    Locator: DIMM_A1
    Bank Locator: A1_BANK0
    Type: DDR3
    Type Detail: Synchronous Unbuffered (Unregistered)
    Speed: 800 MHz
    Manufacturer: Undefined
    Serial Number: 00000000
    Asset Tag: A1_AssetTagNum1
    Part Number: F3-17000CL11-4GBXL
    Rank: 2
    Configured Clock Speed: Unknown

Handle 0x0032, DMI type 20, 35 bytes
Memory Device Mapped Address
    Starting Address: 0x00000000000
    Ending Address: 0x000FFFFFFFF
    Range Size: 4 GB
    Physical Device Handle: 0x0031
    Memory Array Mapped Address Handle: 0x0030
    Partition Row Position: 1

Handle 0x0033, DMI type 17, 34 bytes
Memory Device
    Array Handle: 0x002F
    Error Information Handle: Not Provided
    Total Width: 64 bits
    Data Width: 64 bits
    Size: 4096 MB
    Form Factor: DIMM
    Set: None
    Locator: DIMM_A2
    Bank Locator: A1_BANK1
    Type: DDR3
    Type Detail: Synchronous Unbuffered (Unregistered)
    Speed: 800 MHz
    Manufacturer: Undefined
    Serial Number: 00000000
    Asset Tag: A1_AssetTagNum0
    Part Number: F3-17000CL11-4GBXL
    Rank: 2
    Configured Clock Speed: 39335 MHz

Handle 0x0034, DMI type 20, 35 bytes
Memory Device Mapped Address
    Starting Address: 0x00100000000
    Ending Address: 0x001FFFFFFFF
    Range Size: 4 GB
    Physical Device Handle: 0x0033
    Memory Array Mapped Address Handle: 0x0030
    Partition Row Position: 1

Handle 0x0035, DMI type 17, 34 bytes
Memory Device
    Array Handle: 0x002F
    Error Information Handle: Not Provided
    Total Width: 64 bits
    Data Width: 64 bits
    Size: 4096 MB
    Form Factor: DIMM
    Set: None
    Locator: DIMM_B1
    Bank Locator: A1_BANK2
    Type: DDR3
    Type Detail: Synchronous Unbuffered (Unregistered)
    Speed: 800 MHz
    Manufacturer: Undefined
    Serial Number: 00000000
    Asset Tag: A1_AssetTagNum2
    Part Number: F3-17000CL11-4GBXL
    Rank: 2
    Configured Clock Speed: Unknown

Handle 0x0036, DMI type 20, 35 bytes
Memory Device Mapped Address
    Starting Address: 0x00200000000
    Ending Address: 0x002FFFFFFFF
    Range Size: 4 GB
    Physical Device Handle: 0x0035
    Memory Array Mapped Address Handle: 0x0030
    Partition Row Position: 1

Handle 0x0037, DMI type 17, 34 bytes
Memory Device
    Array Handle: 0x002F
    Error Information Handle: Not Provided
    Total Width: 64 bits
    Data Width: 64 bits
    Size: 4096 MB
    Form Factor: DIMM
    Set: None
    Locator: DIMM_B2
    Bank Locator: A1_BANK3
    Type: DDR3
    Type Detail: Synchronous Unbuffered (Unregistered)
    Speed: 800 MHz
    Manufacturer: Undefined
    Serial Number: 00000000
    Asset Tag: A1_AssetTagNum3
    Part Number: F3-17000CL11-4GBXL
    Rank: 2
    Configured Clock Speed: 1 MHz

Handle 0x0038, DMI type 20, 35 bytes
Memory Device Mapped Address
    Starting Address: 0x00300000000
    Ending Address: 0x003FFFFFFFF
    Range Size: 4 GB
    Physical Device Handle: 0x0037
    Memory Array Mapped Address Handle: 0x0030
    Partition Row Position: 1

Handle 0x0039, DMI type 32, 20 bytes
System Boot Information
    Status: No errors detected

Handle 0x003A, DMI type 41, 11 bytes
Onboard Device
    Reference Designation:  Onboard IGD
    Type: Video
    Status: Enabled
    Type Instance: 1
    Bus Address: 0000:00:02.0

Handle 0x003B, DMI type 41, 11 bytes
Onboard Device
    Reference Designation:  Onboard LAN
    Type: Ethernet
    Status: Enabled
    Type Instance: 1
    Bus Address: 0000:00:19.0

Handle 0x003C, DMI type 41, 11 bytes
Onboard Device
    Reference Designation:  Onboard 1394
    Type: Other
    Status: Enabled
    Type Instance: 1
    Bus Address: 0000:03:1c.2

Handle 0x003D, DMI type 7, 19 bytes
Cache Information
    Socket Designation: L1 CACHE
    Configuration: Enabled, Not Socketed, Level 1
    Operational Mode: Write Back
    Location: Internal
    Installed Size: 192 kB
    Maximum Size: 192 kB
    Supported SRAM Types:
        Pipeline Burst
    Installed SRAM Type: Pipeline Burst
    Speed: 1 ns
    Error Correction Type: Multi-bit ECC
    System Type: Unified
    Associativity: 2-way Set-associative

Handle 0x003E, DMI type 7, 19 bytes
Cache Information
    Socket Designation: L2 CACHE
    Configuration: Enabled, Not Socketed, Level 2
    Operational Mode: Write Back
    Location: Internal
    Installed Size: 4096 kB
    Maximum Size: 4096 kB
    Supported SRAM Types:
        Pipeline Burst
    Installed SRAM Type: Pipeline Burst
    Speed: 1 ns
    Error Correction Type: Multi-bit ECC
    System Type: Unified
    Associativity: 16-way Set-associative

Handle 0x0047, DMI type 4, 42 bytes
Processor Information
    Socket Designation: FM2
    Type: Central Processor
    Family: <OUT OF SPEC>
    Manufacturer: AuthenticAMD
    ID: 31 0F 61 00 FF FB 8B 17
    Version: AMD A10-6800K APU with Radeon(tm) HD Graphics
    Voltage: 1.3 V
    External Clock: 100 MHz
    Max Speed: 4100 MHz
    Current Speed: 4100 MHz
    Status: Populated, Enabled
    Upgrade: <OUT OF SPEC>
    L1 Cache Handle: 0x003D
    L2 Cache Handle: 0x003E
    L3 Cache Handle: Not Provided
    Serial Number: Not Specified
    Asset Tag: Not Specified
    Part Number: Not Specified
    Core Count: 4
    Core Enabled: 4
    Thread Count: 4
    Characteristics:
        64-bit capable

Handle 0x0048, DMI type 13, 22 bytes
BIOS Language Information
    Language Description Format: Long
    Installable Languages: 8
        en|US|iso8859-1
        fr|FR|iso8859-1
        es|ES|iso8859-1
        de|DE|iso8859-1
        ru|RU|iso8859-5
        ja|JP|unicode
        zh|TW|unicode
        zh|CN|unicode
    Currently Installed Language: en|US|iso8859-1

Handle 0x0049, DMI type 127, 4 bytes
End Of Table


