From 12ee4022f67f8854061b46e5c0a7ad6258ab66c2 Mon Sep 17 00:00:00 2001
From: "Subhransu S. Prusty" <subhransu.s.prusty@intel.com>
Date: Wed, 12 Apr 2017 09:54:00 +0530
Subject: [PATCH] ALSA: hda: Add Geminilake id to SKL_PLUS

Geminilake is Skylake family platform. So add it's id to skl_plus check.

Fixes: 126cfa2f5e15 ("ALSA: hda: Add Geminilake HDMI codec ID")
Signed-off-by: Subhransu S. Prusty <subhransu.s.prusty@intel.com>
Cc: Senthilnathan Veppur <senthilnathanx.veppur@intel.com>
Cc: Vinod Koul <vinod.koul@intel.com>
Cc: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
---
 sound/pci/hda/hda_intel.c | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

diff --git a/sound/pci/hda/hda_intel.c b/sound/pci/hda/hda_intel.c
index 59ab34fa0bc8..b786fbab029f 100644
--- a/sound/pci/hda/hda_intel.c
+++ b/sound/pci/hda/hda_intel.c
@@ -370,8 +370,10 @@ enum {
 #define IS_KBL_LP(pci) ((pci)->vendor == 0x8086 && (pci)->device == 0x9d71)
 #define IS_KBL_H(pci) ((pci)->vendor == 0x8086 && (pci)->device == 0xa2f0)
 #define IS_BXT(pci) ((pci)->vendor == 0x8086 && (pci)->device == 0x5a98)
+#define IS_GLK(pci) ((pci)->vendor == 0x8086 && (pci)->device == 0x3198)
 #define IS_SKL_PLUS(pci) (IS_SKL(pci) || IS_SKL_LP(pci) || IS_BXT(pci)) || \
-			IS_KBL(pci) || IS_KBL_LP(pci) || IS_KBL_H(pci)
+			IS_KBL(pci) || IS_KBL_LP(pci) || IS_KBL_H(pci)	|| \
+			IS_GLK(pci)
 
 static char *driver_short_names[] = {
 	[AZX_DRIVER_ICH] = "HDA Intel",
-- 
2.13.1

