$OpenBSD: patch-nspr_pr_include_md__openbsd_cfg,v 1.2 2017/05/03 07:10:37 sthen Exp $

Index: nspr/pr/include/md/_openbsd.cfg
--- nspr/pr/include/md/_openbsd.cfg.orig
+++ nspr/pr/include/md/_openbsd.cfg
@@ -161,7 +161,7 @@
 #define PR_BYTES_PER_WORD_LOG2  3
 #define PR_BYTES_PER_DWORD_LOG2 3
 
-#elif defined(__sparc__)
+#elif defined(__sparc__) || defined(__hppa__)
 
 #undef IS_LITTLE_ENDIAN
 #define  IS_BIG_ENDIAN 1
@@ -206,7 +206,7 @@
 #define PR_ALIGN_OF_DOUBLE  8
 #define PR_ALIGN_OF_POINTER 4
 
-#elif defined(__alpha__)
+#elif defined(__alpha__) || defined(__aarch64__)
 #define IS_LITTLE_ENDIAN 1
 #undef  IS_BIG_ENDIAN
 #define	HAVE_ALIGNED_DOUBLES
@@ -294,6 +294,58 @@
 #define PR_ALIGN_OF_FLOAT   4
 #define PR_ALIGN_OF_DOUBLE  4
 #define PR_ALIGN_OF_POINTER 4
+
+#define PR_BYTES_PER_WORD_LOG2   2
+#define PR_BYTES_PER_DWORD_LOG2  3
+
+#elif defined(__mips__)
+
+#ifdef __MIPSEB__
+#define IS_BIG_ENDIAN 1
+#undef  IS_LITTLE_ENDIAN
+#elif defined(__MIPSEL__)
+#define IS_LITTLE_ENDIAN 1
+#undef  IS_BIG_ENDIAN
+#else
+#error "Unknown MIPS endianness."
+#endif
+
+#define PR_BYTES_PER_BYTE   1
+#define PR_BYTES_PER_SHORT  2
+#define PR_BYTES_PER_INT    4
+#define PR_BYTES_PER_INT64  8
+#define PR_BYTES_PER_LONG   8
+#define PR_BYTES_PER_FLOAT  4
+#define PR_BYTES_PER_DOUBLE 8
+#define PR_BYTES_PER_WORD   4
+#define PR_BYTES_PER_DWORD  8
+
+#define PR_BITS_PER_BYTE    8
+#define PR_BITS_PER_SHORT   16
+#define PR_BITS_PER_INT     32
+#define PR_BITS_PER_INT64   64
+#define PR_BITS_PER_LONG    64
+#define PR_BITS_PER_FLOAT   32
+#define PR_BITS_PER_DOUBLE  64
+#define PR_BITS_PER_WORD    64
+
+#define PR_BITS_PER_BYTE_LOG2   3
+#define PR_BITS_PER_SHORT_LOG2  4
+#define PR_BITS_PER_INT_LOG2    5
+#define PR_BITS_PER_INT64_LOG2  6
+#define PR_BITS_PER_LONG_LOG2   5
+#define PR_BITS_PER_FLOAT_LOG2  5
+#define PR_BITS_PER_DOUBLE_LOG2 6
+#define PR_BITS_PER_WORD_LOG2   5
+
+#define PR_ALIGN_OF_SHORT   2
+#define PR_ALIGN_OF_INT     4
+#define PR_ALIGN_OF_LONG    4
+#define PR_ALIGN_OF_INT64   8
+#define PR_ALIGN_OF_FLOAT   4
+#define PR_ALIGN_OF_DOUBLE  8
+#define PR_ALIGN_OF_POINTER 4
+#define PR_ALIGN_OF_WORD    4
 
 #define PR_BYTES_PER_WORD_LOG2   2
 #define PR_BYTES_PER_DWORD_LOG2  3
