#!/bin/sh
#Barry Kauler 2007 LGPL
#called from /usr/sbin/modemprobe, pupdial
#v405 overhauled.
#v408 rerwin: bugfix.
#v465 rerwin: v413 move init string to Init3
#v477 rerwin: v413 wait longer for modem response; add splash message during sleep
#v424 rerwin: reset skip-PIN flag
#101203 bk: message modification.
#101220 bk: info box if get empty string.
#120201 rodin.s: internationalized.
#120329 Xdialog bug --yesno supposed to "yes" "No" buttons, but they are "OK" "Cancel".

export TEXTDOMAIN=modemtest
export TEXTDOMAINDIR=/usr/share/locale
export OUTPUT_CHARSET=UTF-8
eval_gettext () {
  local myMESSAGE=$(gettext "$1")
  eval echo \"$myMESSAGE\"
}
export LANGORG=$LANG

Yes_lbl="$(gettext 'Yes')"
No_lbl="$(gettext 'No')"

#[ ! $1 ] && exit
DEVM=$1
PARAM2=$2

MODEMDEV=""
if [ -h /dev/modem ];then
 MODEMDEV="`readlink /dev/modem`"
fi

#a fallback if user runs this script directly...
[ "$DEVM" = "" ] && [ "$MODEMDEV" = "" ] && exit
[ "$DEVM" = "" ] && [ "$MODEMDEV" != "" ] && DEVM="$MODEMDEV"

if [ "$PARAM2" = "initonly" ];then
 MSGSUCCESS="`gettext \"Okay, the modem was probed and it responded, confirming that it does exist,\n
now the probe can be done to determine a suitable initialization string.\n
Click the 'Yes' button to do this (recommended), or\n
'No' if you already have a suitable initialization string for this modem in\n
/etc/wvdial.conf (the configuration file for PupDial) ...that would probably\n
be the case if you had used this modem the last time that you ran PupDial.\n
\n
Note: For some modern modems, the default 'ATZ' initialization string is\n
sufficient and you do not have to do this probe, however it does not do any\n
harm to do so (and gives further confirmation the modem works)...\"`"
else
 MSGSUCCESS="`eval_gettext \"Success, the modem responds as \\\$DEVM! (The modem is there; getting it to dial out is another matter!)\n
Click the 'yes' button if you would like /dev/modem to be a link to \\\${DEVM} and the Wvdial\n
configuration file /etc/wvdial.conf set with entry 'Modem = /dev/\\\${DEVM}. An attempt will\n
also be made to determine appropriate modem initialization strings.\"`"
fi


#return the IRQ that respond to a given device...
irq_from_device_func() { #device passed in, ex: /dev/ttyS0
 #v1.0.2 it seems that setserial may be more trouble than its worth...
 #in the case of linmodems it often doesn't work...
 case ${1} in
  /dev/ttyS[0-9])
   set -- `setserial -v -b ${1} auto_irq skip_test autoconfig session_lockout`
   [ "$6" ] && echo $6 | tr -d \)
  ;;
  esac
}

#talk to modem, wait for response...
chat_with_func() { #device passed in.
 rm -f /tmp/answer.txt
 #TODO maybe send +++ to return modem to command-mode.
 #hangs if modem unplugged or turned off (contrary to what docs say)...
 modem-stats -c "ATZ" $1 > /tmp/answer.txt &
 sleep 5 #v413
 killall modem-stats
 if [ -e /tmp/answer.txt ];then
  if [ -s /tmp/answer.txt ];then #nonzero size.
   grep "^OK" /tmp/answer.txt > /dev/null 2>&1
   [ $? -eq 0 ] && return 0 #success
  fi
 fi
 return 1
}

#v433 Set config file Modem line(s), including possible alternate USB modem device.
modem_device_to_conf_func() {
 #Argument is modem device for config file - current or tested
 DEVMCONF="$1"
 DEVMALT="`get_modem_alternate_device $DEVM`"
 if [ "$DEVMALT" = "" ];then
  if [ "$DEVM" = "$MODEMDEV" -a "$PARAM2" = "" ];then
   grep -q '^#Modem =' /etc/wvdial.conf \
    || return 1
  fi
  aPATTERN="s%^Modem = .*%Modem = /dev/${DEVMCONF}%"
 else
  aPATTERN="s%^Modem = .*%Modem = /dev/${DEVMCONF}\n#Modem = /dev/${DEVMALT}%"
 fi
 sed -i \
  -e '/#Modem =/d' \
  -e "$aPATTERN" /etc/wvdial.conf
 return 0
} #v433 end

modem_test_func() {
 [ "$DEVM" = "" ] && DEVM='invalid'
 #case $DEVM in
 #tty*)
yaf-splash -outline 0 -margin 4 -bg orange -text "$(gettext 'Verifying modem is present...')" &
# /usr/X11R7/bin/yaf-splash -font "8x16" -outline 0 -margin 4 -bg orange -text "Verifying modem is present..." &
  X8PID=$! #v413
  IRQM=$(irq_from_device_func /dev/${DEVM})
  fuser -k /dev/${DEVM} 2>/dev/null #kill processing attached to device.
  chat_with_func /dev/$DEVM
  if [ $? -eq 0 ];then
   kill $X8PID #v413
   modem_device_to_conf_func $DEVM #v433 set tested dev
   if [ "$DEVM" = "$MODEMDEV" -a "$PARAM2" = "" ];then
    Xdialog --left --wmclass "pupdial" --title "$(gettext 'PupDial: modem test')" --no-cancel --msgbox "`eval_gettext \"Success, the modem responds as \\\$DEVM! (The modem is there; getting it to dial out is another matter!)\"`" 0 0
   else 
    Xdialog --left --wmclass "pupdial" --title "$(gettext 'PupDial: modem test')" --ok-label "$Yes_lbl" --cancel-label "$No_lbl" --yesno "${MSGSUCCESS}" 0 0
    if [ $? -eq 0 ];then
     yaf-splash -outline 0 -margin 4 -bg orange -text "$(gettext 'Please wait, updating settings...')" &
#     /usr/X11R7/bin/yaf-splash -font "8x16" -outline 0 -margin 4 -bg orange -text "Please wait, updating settings..." &
     X9PID=$!
     ln -snf $DEVM /dev/modem

     waitmax 29 gen_modem_init_string > /dev/null #writes to /tmp/mymodeminitstring
     FLAGBADINITSTRING='no' #101220
     if [ -s /tmp/mymodeminitstring ];then
      INITSTRING="`cat /tmp/mymodeminitstring | sed 's/\&/\\\&/g' | tr -s ' '`" #v433 sed problem with &
      if [ "$INITSTRING" = "" -o "$INITSTRING" = " " ];then #101220
       FLAGBADINITSTRING='yes' #101220
      else
       bPATTERN="s/^Init3.*/Init3 = ${INITSTRING}/" #v413
       sed -i -e "$bPATTERN" /etc/wvdial.conf #v433
      fi
     else
      FLAGBADINITSTRING='yes' #101220
     fi
     kill $X9PID
     if [ "$FLAGBADINITSTRING" = "yes"  ];then #101220
      Xdialog --left --wmclass "pupdial" --title "$(gettext 'PupDial: Initialization string')" --msgbox "$(gettext 'There is a problem, probing did not generate an initialization string. You could try\n
unplugging the modem, reboot Puppy then plug-in the modem and try again with PupDial.\n
Alternatively, in the PupDial main GUI window, try one of these strings in the second\n
initialization-string entry box (write them down!)'):\n\n
      AT &FE0 V1 X1 &D2 &C1 s0=0\n
      AT Q0 V1 E1 S0=0 &C1 &D2" 0 0
     fi
    else
     #101203...
     INIT3="`cat /etc/wvdial.conf | grep '^Init3' | tr -d ' ' | cut -f 2-9 -d '='`"
     if [ "$INIT3" ];then
      Xdialog --left --wmclass "pupdial" --title "$(gettext 'PupDial: Initialization string')" --ok-label "$Yes_lbl" --cancel-label "$No_lbl" --yesno "`gettext \"The PupDial configuration file /etc/wvdial.conf does have initialization\n
strings in it from previous usage of PupDial. Would you like to reset\n
them to the default ('ATZ' only)?\n
Note, you might want to do this if you have changed modems and you know\n
that the defaults are sufficient. If in doubt, click 'No'...\"`" 0 0
      if [ $? -eq 0 ];then
       #modify [Dialer Defaults] only...
       echo -n "" > /tmp/wvdial.conf-modemtest
       cat /etc/wvdial.conf |
       while read ONELINE
       do
        if [ "`echo -n "$ONELINE" | cut -c 1`" = "[" ];then
         WVSECTION=0
         [ "$ONELINE" = "[Dialer Defaults]" ] && WVSECTION=1
        fi
        if [ $WVSECTION -eq 1 ];then
         NEWONE="`echo -n "$ONELINE" | sed -e 's%^Init3 =.*%Init3 = %'  -e 's%^Init2 =.*%Init2 = ATZ%' -e 's%^Init1 =.*%Init1 = %'`"
         echo "$NEWONE" >> /tmp/wvdial.conf-modemtest
        else
         echo "$ONELINE" >> /tmp/wvdial.conf-modemtest
        fi
       done
       cp -f /tmp/wvdial.conf-modemtest /etc/wvdial.conf
      fi
     fi
    fi
    rm -f /tmp/.pupdial_pin_sent #v433
   fi
   touch /tmp/.pupdial-modem_detected #v433
  else
   kill $X8PID #v413
   modem_device_to_conf_func $MODEMDEV #v433 set current dev
   Xdialog --left --wmclass "pupdial" --title "$(gettext 'PupDial: modem test')" --no-cancel --msgbox "$(gettext 'Sorry, the modem was not detected as') $DEVM." 0 0
   rm -f /tmp/.pupdial_pin_sent #v433
   rm -f /tmp/.pupdial-modem_detected #v433
  fi
 # ;;
 #*)
 #  Xdialog --center --wmclass "pupdial" --title "PupDial: modem test" --no-cancel --msgbox "There is no modem to test." 0 0
 # ;;
 #esac
}

modem_test_func

###END###
