#!/bin/sh
#
# scsi 1.30 1997/05/13 02:18:00 (David Hinds)
#
# Initialize or shutdown a PCMCIA SCSI adapter
#
# The first argument should be either 'start' or 'stop'.  The second
# argument is the base name for the device.
#
# The script passes an extended device address to 'scsi.opts' in the
# ADDRESS variable, to retrieve device-specific configuration options.
# The address format is "scheme,device,socket,channel,id,lun[,part]"
# where "scheme" is the PCMCIA configuration scheme; "device" is the
# SCSI device type (sd, sr, st, sg); "socket" is the socket number;
# "channel", "id", and "lun" are the SCSI device ID's; and "part" is,
# optionally, the partition number.
#
# The script first calls scsi.opts for the entire device.  If
# scsi.opts returns with the PARTS variable set, then this variable
# contains a list of partitions for which options should be read.
#

if [ -r ./shared ] ; then . ./shared ; else . /etc/pcmcia/shared ; fi

# Get device attributes
get_info $DEVICE

case "$DEVICE" in
scsi*) exit 0    ;;
sd*)   TYPE="sd" ;;
st*)   TYPE="st" ;;
scd*)  TYPE="sr" ;;
sg*)   TYPE="sg" ;;
esac
eval `/sbin/scsi_info /dev/$DEVICE` || usage

# Load site-specific settings
ADDRESS="$SCHEME,$TYPE,$SOCKET,$SCSI_ID"
. $0.opts

case "$ACTION" in

'start')
    [ -n "$VERBOSE" -a -n "$INFO" ] && echo "$INFO"
    add_parts $ADDRESS "$PARTS" || exit 1
    ;;

'stop')
    if [ -b /dev/$DEVICE ] ; then
	rm_parts $ADDRESS "$PARTS"
    else
	do_fuser -k /dev/$DEVICE > /dev/null
    fi
    exit $?
    ;;

'check')
    is_true $NO_CHECK && exit 0
    if [ -b /dev/$DEVICE ] ; then
	do_fuser -s -m /dev/${DEVICE}* && exit 1
    elif [ -c /dev/$DEVICE ] ; then
	do_fuser -s /dev/${DEVICE}* && exit 1
    fi
    ;;

'cksum')
    chk_parts "$NEW_SCHEME,$TYPE,$SOCKET,$SCSI_ID" || exit 1
    ;;
    
'suspend'|'resume')
    ;;

*)
    usage
    ;;

esac

exit 0
