# File generated by xf86config.
# and additional hand edited by Rene Rebe - T2 Project
#
# YOU MUST ONLY MODIFY THE CARD SECTION AND SOME MONITOR SETTINGS
# TO GET A WORKING X CONFIGURATION.
#

# **********************************************************************
# Refer to the XF86Config(4/5) man page for details about the format of 
# this file.
# **********************************************************************

# **********************************************************************
# Module section -- this  section  is used to specify
# which dynamically loadable modules to load.
# **********************************************************************

Section "Module"

    Load        "dbe"  	# DBE (double buffer extension)
    Load	"ddc"   # Display Data Channel extension

# This loads the miscellaneous extensions module
    SubSection  "extmod"
      # Option    "omit xfree86-dga" # don't initialise the DGA extension
      # Option    "omit XFree86-VidModeExtension" # disable mode-switching-supoprt
    EndSubSection

# This loads the Type1 and FreeType font modules
    Load        "type1"
    Load        "freetype"

#    Load	"glx"  # GLX extension (OpenGL visuals)
#    Load	"dri"  # Direct Rendering Interface extension (OpenGL)

#    Load	"v4l"  # Video 4 Linux extension (provides a xv adapter)
EndSection

# **********************************************************************
# Extensions section -- this  section  is used to specify
# which extensions to enable.
# **********************************************************************

Section "Extensions"
#    Option  "XEVIE"         "Disable"
    Option  "Composite"     "Enable"
EndSection


# this enabled normal users to use DRI - the Direct Rendering Extension.
# it is also possible to use a group to control access.
#
Section "DRI"
    Mode 0666
EndSection

# **********************************************************************
# Files section.  This allows default font and rgb paths to be set
# **********************************************************************

Section "Files"

# The location of the RGB database.  Note, this is the name of the
# file minus the extension (like ".txt" or ".db").  There is normally
# no need to change the default.

    RgbPath    "/usr/X11/share/X11/rgb"

# Multiple FontPath entries are allowed (which are concatenated together),
# as well as specifying multiple comma-separated entries in one FontPath
# command (or a combination of both methods)
# 
# If you don't have a floating point coprocessor and emacs, Mosaic or other
# programs take long to start up, try moving the Type1 and Speedo directory
# to the end of this list (or comment them out).
# 

    FontPath   "/usr/X11/lib/X11/fonts/75dpi/:unscaled"
    FontPath   "/usr/X11/lib/X11/fonts/100dpi/:unscaled"
    FontPath   "/usr/X11/lib/X11/fonts/CID/"
    FontPath   "/usr/X11/lib/X11/fonts/PEX/"
    FontPath   "/usr/X11/lib/X11/fonts/Speedo/"
    FontPath   "/usr/X11/lib/X11/fonts/Type1/"
    FontPath   "/usr/X11/lib/X11/fonts/cyrillic/"
    FontPath   "/usr/X11/lib/X11/fonts/encodings/"
    FontPath   "/usr/X11/lib/X11/fonts/freefont/"
    FontPath   "/usr/X11/lib/X11/fonts/latin2/"
    FontPath   "/usr/X11/lib/X11/fonts/local/"
    FontPath   "/usr/X11/lib/X11/fonts/misc/"
    FontPath   "/usr/X11/lib/X11/fonts/sharefont/"
    FontPath   "/usr/X11/lib/X11/fonts/TTF/"

# The module search path.  The default path is shown here.

#    ModulePath "/usr/X11/lib/modules"

EndSection

# **********************************************************************
# Server flags section.
# **********************************************************************

Section "ServerFlags"

# Uncomment this to cause a core dump at the spot where a signal is 
# received.  This may leave the console in an unusable state, but may
# provide a better stack trace in the core dump to aid in debugging

#    Option "NoTrapSignals"

# Uncomment this to disable the <Crtl><Alt><BS> server abort sequence
# This allows clients to receive this key event.

#    Option "DontZap"

# Uncomment this to disable the <Crtl><Alt><KP_+>/<KP_-> mode switching
# sequences.  This allows clients to receive these key events.

#    Option "Dont Zoom"

# Uncomment this to disable tuning with the xvidtune client. With
# it the client can still run and fetch card and monitor attributes,
# but it will not be allowed to change them. If it tries it will
# receive a protocol error.

#    Option "DisableVidModeExtension"

# Uncomment this to enable the use of a non-local xvidtune client. 

#    Option "AllowNonLocalXvidtune"

# Uncomment this to disable dynamically modifying the input device
# (mouse and keyboard) settings. 

#    Option "DisableModInDev"

# Uncomment this to enable the use of a non-local client to
# change the keyboard or mouse settings (currently only xset).

#    Option "AllowNonLocalModInDev"

# Uncomment this to enable multi-head Xinerama support

#    Option "Xinerama" "true"

EndSection

# **********************************************************************
# Input devices
# **********************************************************************

# **********************************************************************
# Core keyboard's InputDevice section
# **********************************************************************

Section "InputDevice"

    Identifier	"Keyboard1"
    Driver	"kbd"

# For most OSs the protocol can be omitted (it defaults to "Standard").
# When using XQUEUE (only for SVR3 and SVR4, but not Solaris),
# uncomment the following line.

#    Option     "Protocol"      "Xqueue"

    Option "AutoRepeat" "250 30"

# Specify which keyboard LEDs can be user-controlled (eg, with xset(1))
#    Option "Xleds" "1 2 3"

#    Option "LeftAlt"     "Meta"
#    Option "RightAlt"    "ModeShift"

# To customise the XKB settings to suit your keyboard, modify the
# lines below (which are the defaults).  For example, for a non-U.S.
# keyboard, you will probably want to use:
#    Option "XkbModel"    "pc102"
# If you have a US Microsoft Natural keyboard, you can use:
#    Option "XkbModel"    "microsoft"
#
# Then to change the language, change the Layout setting.
# For example, a german layout can be obtained with:
#    Option "XkbLayout"   "de"
# or:
#    Option "XkbLayout"   "de"
#    Option "XkbVariant"  "nodeadkeys"
#
# If you'd like to switch the positions of your capslock and
# control keys, use:
#    Option "XkbOptions"  "ctrl:swapcaps"

# These are the default XKB settings for XFree86
#    Option "XkbRules"    "xorg"
#    Option "XkbModel"    "pc101"
#    Option "XkbLayout"   "us"
#    Option "XkbVariant"  ""
#    Option "XkbOptions"  ""

#    Option "XkbDisable"

    Option "XkbRules"	"xorg"
    Option "XkbModel"	"pc105"
#    Option "XkbLayout"	"de"  # german keyboard layout
#    Option "XkbVariant" "nodeadkeys"  # normally not wanted

EndSection


# **********************************************************************
# Core Pointer's InputDevice section
# **********************************************************************

# normal wheel mouse ...
#
Section "InputDevice"

    Identifier	"Mouse1"
    Driver	"mouse"

    Option "Protocol"    "IMPS/2"
    Option "Device"      "/dev/input/mice"

#    Option "Protocol"    "Auto"
#    Option "Protocol"    "Microsoft"
#    Option "Protocol"    "PS/2"
#    Option "Device"      "/dev/tts/0"
#    Option "Device"      "/dev/misc/psaux"

    Option "Buttons"	 "5"
    Option "ZaxisMapping" "4 5"

EndSection


# **********************************************************************
# Other input device sections 
# this is optional and is required only if you
# are using extended input devices.  This is for example only.  Refer
# to the XF86Config man page for a description of the options.
# **********************************************************************
#
# Section "InputDevice" 
#    Identifier  "Mouse2"
#    Driver      "mouse"
#    Option      "Protocol"      "MouseMan"
#    Option      "Device"        "/dev/mouse2"
# EndSection
#
# Section "InputDevice"
#    Identifier "Spaceball"
#    Driver     "magellan"
#    Option     "Device"        "/dev/cua0"
# EndSection
#
# Section "InputDevice"
#    Identifier "Spaceball2"
#    Driver     "spaceorb"
#    Option     "Device"        "/dev/cua0"
# EndSection
#
# Section "InputDevice"
#    Identifier  	"Synaptics1"
#    Driver  	"synaptics"
#    Option	"ZaxisMapping"	"4 5 6 7"
#    Option 	"Device"  	"/dev/input/mouse0"
#    Option	"Protocol"	"auto-dev"
#  #  Option	"LeftEdge"      "1700"
#  #  Option	"RightEdge"     "5300"
#  #  Option	"TopEdge"       "1700"
#  #  Option	"BottomEdge"    "4200"
#    Option	"FingerLow"	"25"
#    Option	"FingerHigh"	"30"
#    Option	"MaxTapTime"	"180"
#    Option	"MaxTapMove"	"220"
#    Option	"TapButton2"	"3"
#    Option	"TapButton3"	"2"
#    Option	"VertTwoFingerScroll"	"true"
#    Option	"HorizTwoFingerScroll"	"true"
#    Option	"VertScrollDelta" "5"
#    Option	"HorizScrollDelta" "5"
#    Option	"MinSpeed"	"0.40"
#    Option	"MaxSpeed"	"1.00"
#    Option	"AccelFactor"	"0.05"
#    Option	"SHMConfig"	"on"
# EndSection
#
# Section "InputDevice"
#    Identifier "Touchscreen0"
#    Driver     "microtouch"
#    Option     "Device"        "/dev/ttyS0"
#    Option     "MinX"          "1412"
#    Option     "MaxX"          "15184"
#    Option     "MinY"          "15372"
#    Option     "MaxY"          "1230"
#    Option     "ScreenNumber"  "0"
#    Option     "ReportingMode" "Scaled"
#    Option     "ButtonNumber"  "1"
#    Option     "SendCoreEvents"
# EndSection
#
# Section "InputDevice"
#    Identifier "Touchscreen1"
#    Driver     "elo2300"
#    Option     "Device"        "/dev/ttyS0"
#    Option     "MinX"          "231"
#    Option     "MaxX"          "3868"
#    Option     "MinY"          "3858"
#    Option     "MaxY"          "272"
#    Option     "ScreenNumber"  "0"
#    Option     "ReportingMode" "Scaled"
#    Option     "ButtonThreshold"       "17"
#    Option     "ButtonNumber"  "1"
#    Option     "SendCoreEvents"
# EndSection

# Section "InputDevice"
#   Identifier "Tablet1"
#   Driver     "summa"
#   Option     "Device"        "/dev/ttyS0"
#   Option     "MinX"          "231"
#   Option     "MaxX"          "3868"
#   Option     "MinY"          "3858"
#   Option     "MaxY"          "272"
#   Option     "ScreenNumber"  "0"
#   Option     "ReportingMode" "Scaled"
#   Option     "ButtonThreshold"       "17"
#   Option     "ButtonNumber"  "1"
#   Option     "SendCoreEvents"
#   Option	"BaudRate"    "19200"
#   Option	"DataBits"    "8"
#   Option	"StopBits"    "1"
#   Option	"Parity"      "Odd"
#   Option	"FlowControl" "Xoff"
#   Option	"VTime"       "10"
#   Option	"VMin"        "1"
# EndSection


# **********************************************************************
# Monitor section
# **********************************************************************

# Any number of monitor sections may be present

Section "Monitor"

    Identifier  "Monitor1"

# NOTE: THE VALUES HERE ARE EXAMPLES ONLY.  REFER TO YOUR MONITOR'S
# USER MANUAL FOR THE CORRECT NUMBERS !!

# normally uncomment this lines
#    HorizSync   24.0 - 80.0
#    VertRefresh 50-100

# overwrite the screen dimensions (in mm) e.g. to get another virtual dpi
# value
#    DisplaySize 345 260

# HorizSync is in kHz unless units are specified.
# HorizSync may be a comma separated list of discrete values, or a
# comma separated list of ranges of values.
#    HorizSync	30-64         # multisync
#    HorizSync	31.5, 35.2    # multiple fixed sync frequencies
#    HorizSync	15-25, 30-50  # multiple ranges of sync frequencies

# VertRefresh is in Hz unless units are specified.
# VertRefresh may be a comma separated list of discrete values, or a
# comma separated list of ranges of values.
#    VertRefresh 50-100

# some mode examples 1,2 selfmade - 3 from fbset
# (only needed for low-level tricks, exotic Laptops or other LCD's)
#
#    Mode "1152x900"
#        DotClock        120  
#        HTimings        1152 1200 1312 1528 
#        VTimings        900  910  946  985
#    EndMode
#    Mode "1152x900-2"
#        DotClock        100
#        HTimings        1152 1200 1312 1528
#        VTimings        900  910  946  985
#    EndMode
#    Mode "1152x864"
#	DotClock 105.810
#	HTimings 1152 1184 1312 1504
#	VTimings 864 868 872 902
#	Flags    "-HSync" "-VSync"
#    EndMode

# for framebuffer devices you might want to simply add
# the 'fbset -x' output here.

EndSection


# **********************************************************************
# Graphics device section
# **********************************************************************

# Any number of graphics device sections may be present

Section "Device"
    Identifier	"Card1"

    # Use this for framebuffer devices - should work on most systems.
    Driver       "fbdev"
    Option       "fbdev" "/dev/fb/0"

#    Driver	"vga" # mga, ati, nv, sis, vesa ...
#    # Option     "BackingStore"

#    # Some driver accept an UseFBDev option (e.g. radeon) to switch the
#    # mode via the Linux framebuffer layer. Needed e.g. as workaround for
#    # iBooks.
#    # Option	"UseFBDev"

#    # The BuID is only required for multi-monitor configs or some fbdev drivers
#    # BusID	"PCI:1:5:0"
#    # Screen	0 # Screen of a dual-head mga card

#    # Option	"NoHal" # do not use the binary-only Matrox HAL library
#    # Option	"AGPMode2x"

#    # Option   "MergedFB" "true" # lightweight multi-head
#    # Option   "CRT2Position" "RightOf"

EndSection

# Matrox Millenium 4xx, Ati or NVidia second-head
#Section "Device"
#    Identifier	"Card2"
#    Driver	"mga" # or other dual-able cards like ati, nv
#    # Option	"BackingStore"

#    BusID	"PCI:1:5:0"
#    Screen	1
#
#    # Option	"NoHal" # do not use the binary-only Matrox HAL library
#    # Option	"AGPMode2x"

#    # Option	"Tv" "yes"
#    # Option	"TVStandard" "PAL"
#    # Option	"CableType" "SCART_COMPOSITE"
#EndSection

# **********************************************************************
# Screen sections
# **********************************************************************

# Any number of screen sections may be present.  Each describes
# the configuration of a single screen.  A single specific screen section
# may be specified from the X server command line with the "-screen"
# option.
Section "Screen"
    Identifier  "Screen1"
    Device      "Card1"
    Monitor     "Monitor1"
    DefaultDepth 24

    Subsection "Display"
        Modes       "1024x768" "800x600" "640x480"
    EndSubsection
EndSection

#Section "Screen"
#    Identifier  "Screen2"
#    Device      "Card2"
#    Monitor     "Monitor1"
#    DefaultDepth 16
#
#    Subsection "Display"
#        Modes       "1024x768" "800x600" "640x480" 
#    EndSubsection
#EndSection

#Section "Screen"
#    Identifier  "ScreenTV"
#    Device      "CardTV"
#    Monitor     "Monitor1"
#    DefaultDepth 16
#
#    Subsection "Display"
#        Depth       16
#        Modes       "640x480"
#        ViewPort    0 0
#    EndSubsection
#EndSection


# **********************************************************************
# ServerLayout sections.
# **********************************************************************

# Any number of ServerLayout sections may be present.  Each describes
# the way multiple screens are organised.  A specific ServerLayout
# section may be specified from the X server command line with the
# "-layout" option.  In the absence of this, the first section is used.
# When now ServerLayout section is present, the first Screen section
# is used alone.

Section "ServerLayout"

# The Identifier line must be present
    Identifier  "Simple Layout"

# Each Screen line specifies a Screen section name, and optionally
# the relative position of other screens.  The four names after
# primary screen name are the screens to the top, bottom, left and right
# of the primary screen.  In this example, screen 2 is located to the
# right of screen 1.

    Screen "Screen1"  # LeftOf "Screen2"
    # Screen "Screen2"
    # Screen "ScreenTV" 

# Each InputDevice line specifies an InputDevice section name and
# optionally some options to specify the way the device is to be
# used.  Those options include "CorePointer", "CoreKeyboard" and
# "SendCoreEvents".

    InputDevice "Mouse1" "CorePointer"
    InputDevice "Keyboard1" "CoreKeyboard"

# It is possible to specify secondary input devices which might not
# be pressend on X startup. Nice for laptops with temporary external
# mices ;-)!

#    InputDevice "Mouse2" "SendCoreEvents"
#    InputDevice "Tablet1"

EndSection

