##############################################################################
# Copyright (c) 1998-2002,2006 Free Software Foundation, Inc.                #
#                                                                            #
# Permission is hereby granted, free of charge, to any person obtaining a    #
# copy of this software and associated documentation files (the "Software"), #
# to deal in the Software without restriction, including without limitation  #
# the rights to use, copy, modify, merge, publish, distribute, distribute    #
# with modifications, sublicense, and/or sell copies of the Software, and to #
# permit persons to whom the Software is furnished to do so, subject to the  #
# following conditions:                                                      #
#                                                                            #
# The above copyright notice and this permission notice shall be included in #
# all copies or substantial portions of the Software.                        #
#                                                                            #
# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR #
# IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,   #
# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL    #
# THE ABOVE COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER      #
# LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING    #
# FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER        #
# DEALINGS IN THE SOFTWARE.                                                  #
#                                                                            #
# Except as contained in this notice, the name(s) of the above copyright     #
# holders shall not be used in advertising or otherwise to promote the sale, #
# use or other dealings in this Software without prior written               #
# authorization.                                                             #
##############################################################################
#
# Author: Zeyd M. Ben-Halim <zmbenhal@netcom.com> 1992,1995
#    and: Eric S. Raymond <esr@snark.thyrsus.com>
#
# $Id: Caps,v 1.36 2006/05/27 15:33:04 tom Exp $
#
# This is the master termcap/terminfo capability table.
#
# This table is used to generate initializers for tables that drive tic,
# infocmp, and the library compilation code used to support the termcap 
# compatibility hack.  It is also used to generate the tabular portion of the
# terminfo(5) man page; lines beginning with `#%' are passed through to become
# the terminfo table.
#
# This file has three major sections; a standard-capabilities table, two
# extension-capability tables, and a section of aliases declarations.
# The first two have the same format, as follows:
#
# FILE FORMAT
#
# Column 1: terminfo variable name
# Column 2: terminfo capability name
# Column 3: capability type (boolean, numeric, or string)
# Column 4: termcap capability name
# Column 5: KEY_xxx name, if any, `-' otherwise
# Column 6: value for KEY_xxx name, if any, `-' otherwise
# Column 7: Lead with `Y' if capability should be emitted in termcap
#           translations, `-' otherwise
# Column 8: capability description
#
# The codes following [Y-] in column 7 describe the versions of termcap which
# use the given capability.  This information is not used by the curses library
# proper; rather, it's there to help the terminfo maintainer avoid emitting
# termcap entry translations that are more than 1023 bytes long (and tank a
# lot of old termcap-using programs).  The codes read as follows:
#	B = mentioned in the BSD man page for 4.4BSD curses
#	C = used by the 4.4BSD curses library
#	G = mentioned in the documentation for GNU termcap
#	E = used by GNU Emacs
#	K = remove this terminfo capability when translating to standard format
# The important codes are C and E.  A cap with C or E should be preserved in
# translation if possible.  The problem is that preserving all such caps may
# lead to some termcap translations being too long.  The termcap maintainer
# has a bit of a juggling act to do...potential problem cases are marked with
# an asterisk (*).
#
# The aliases section has the following format:
#
# Column 1: either `capalias' or `infoalias'
# Column 2: name to be aliased
# Column 3: what name it should translate to.  The name IGNORE means it
#           should be discarded with a warning message.
# Column 4: name of the extension set (used for compiler warning messages)
# Column 5: capability description (usually an associated terminfo variable)
#
# HANDLING TERMCAP AND TERMINFO EXTENSIONS
#
# There are basically five different ways to handle termcap and terminfo
# extensions:
#
# 1. Don't list the capname here, or list it but comment it out (the latter
# is preferable; someone might want to handle it in the future).  If you do
# this, the capability will be treated as unknown and raise a warning from
# the compiler.
#
# 2. Alias it.  This is appropriate if the capability has the same meaning
# as an already-supported one.  The compiler will handle aliasing, emitting
# an appropriate informational message whenever an alias fires.
#
# 3. List it in the standard table.  You almost certainly do *not* want
# to do this -- the capabilities in that one, and their order, have been
# carefully chosen to be SVr4-binary-compatible when they're written out
# as a terminfo object, and breaking this would be bad.  It's up the ncurses
# library what to do with the terminfo data after it's read in.
#
# 4. List it in the aliases table with an IGNORE target field.  If you
# do this, the capability will be ignored on input (though the user will
# get a warning message about it).
#
# 5. List it in the extensions table. If you do this, the compiler will
# silently accept the capability, but the curses library proper will never
# see it (because it won't be written out as part of the terminfo object
# format).  It's up to you what you have the compiler do with it.
#
# There are two opposite reasons to choose option 5.  One is when you want
# to eat the capability silently and discard it when doing translations
# to terminfo with tic -I.  Some very old obsolete BSD caps like :kn: are
# in this class.  Nothing will ever use them again.
#
# More usually, you want the compiler to try to deduce something from the
# capability value that it can use to translate it into your output format.
# You'll need to write custom code, probably in postprocess_termcap() or
# postprocess_terminfo(), to handle the translation.
#
# CONTROLLING ENTRY LENGTH 
#
# Notes on specific elisions made to fit translations within 1023 bytes:
#
# Machines with IBM PC-like keyboards want to be able to define the following
# keys: key_npage, key_ppage, key_home, key_ll (which is used for in termcap-
# only environments for End or Home-Down), key_dc, and key_ic.  This is also
# the set of keys the `joe' editor will be upset if it can't see.  So don't 
# trim those out of the set to be translated to termcap, or various users of
# the termcap file will become irate.
#
# It might look tempting to leave those long init strings out of translations.
# We can't do it (yet); 4.4BSD tput and tset use them.
#
# We retain the sgr capability in translation in spite of the fact that neither
# 4.4BSD nor GNU Emacs uses it, because (a) some entry naming distinctions are
# hard to understand without it, and (b) the entries in which it is long tend
# to be older types that don't use up a lot of string space on function keys.
# The tic(1) translation code will complain and elide it if it makes a critical
# difference (there is special code in tic to recognize this situation).
#
# Yes, BSD tset(1) uses hpa.  We elide hpa/vpa anyway because the motion
# optimizer in BSD curses didn't use them.  This omission seems to be the
# single most effective one, it shortened the resolved length of all thirteen
# problem entries in the 9.9.0 version of the terminfo master below critical.
#
# It would be nice to keep f11 and f12 for Emacs use, but a couple of termcap
# translations go back over critical if we do this.  As 4.4BSD curses fades
# into history and GNU termcap's application base shrinks towards being GNU 
# Emacs only, we'll probably elide out some BSD-only capabilities in order
# to buy space for non-essentials Emacs is still using.  Capabilities high
# on that hit list: rc, sc, uc.
#
#############################################################################
#
# STANDARD CAPABILITIES
#
#%The following is a complete table of the capabilities included in a
#%terminfo description block and available to terminfo-using code.  In each
#%line of the table,
#%
#%The \fBvariable\fR is the name by which the programmer (at the terminfo level)
#%accesses the capability.
#%
#%The \fBcapname\fR is the short name used in the text of the database,
#%and is used by a person updating the database.
#%Whenever possible, capnames are chosen to be the same as or similar to
#%the ANSI X3.64-1979 standard (now superseded by ECMA-48, which uses 
#%identical or very similar names).  Semantics are also intended to match
#%those of the specification.
#%
#%The termcap code is the old
#%.B termcap
#%capability name (some capabilities are new, and have names which termcap
#%did not originate).
#%.P
#%Capability names have no hard length limit, but an informal limit of 5
#%characters has been adopted to keep them short and to allow the tabs in
#%the source file
#%.B Caps
#%to line up nicely.
#%
#%Finally, the description field attempts to convey the semantics of the
#%capability.  You may find some codes in the description field:
#%.TP
#%(P)
#%indicates that padding may be specified
#%.TP
#%#[1-9]
#%in the description field indicates that the string is passed through tparm with
#%parms as given (#\fIi\fP).
#%.TP
#%(P*)
#%indicates that padding may vary in proportion to the number of
#%lines affected
#%.TP
#%(#\d\fIi\fP\u)
#%indicates the \fIi\fP\uth\d parameter.
#%
#%.PP
#% These are the boolean capabilities:
#%
#%.na
#%.TS H
#%center expand;
#%c l l c
#%c l l c
#%lw25 lw6 lw2 lw20.
#%\fBVariable	Cap-	TCap	Description\fR
#%\fBBooleans	name	Code\fR
auto_left_margin		bw	bool	bw	-	-	YB-G-	cub1 wraps from column 0 to last column
auto_right_margin		am	bool	am	-	-	YBCGE	terminal has automatic margins
no_esc_ctlc			xsb	bool	xb	-	-	YBCG-	beehive (f1=escape, f2=ctrl C)
ceol_standout_glitch		xhp	bool	xs	-	-	YBCGE	standout not erased by overwriting (hp)
eat_newline_glitch		xenl	bool	xn	-	-	YBCGE	newline ignored after 80 cols (concept)
erase_overstrike		eo	bool	eo	-	-	YBCG-	can erase overstrikes with a blank
generic_type			gn	bool	gn	-	-	YB-G-	generic line type
hard_copy			hc	bool	hc	-	-	YBCG-	hardcopy terminal
has_meta_key			km	bool	km	-	-	YB-GE	Has a meta key (i.e., sets 8th-bit)
has_status_line			hs	bool	hs	-	-	YB-G-	has extra status line
insert_null_glitch		in	bool	in	-	-	YBCGE	insert mode distinguishes nulls
memory_above			da	bool	da	-	-	YBCG-	display may be retained above the screen
memory_below			db	bool	db	-	-	YB-GE	display may be retained below the screen
move_insert_mode		mir	bool	mi	-	-	YBCGE	safe to move while in insert mode
move_standout_mode		msgr	bool	ms	-	-	YBCGE	safe to move while in standout mode
over_strike			os	bool	os	-	-	YBCG-	terminal can overstrike
status_line_esc_ok		eslok	bool	es	-	-	YB-G-	escape can be used on the status line
dest_tabs_magic_smso		xt	bool	xt	-	-	YBCGE	tabs destructive, magic so char (t1061)
tilde_glitch			hz	bool	hz	-	-	YB-GE	cannot print ~'s (hazeltine)
transparent_underline		ul	bool	ul	-	-	YBCGE	underline character overstrikes
xon_xoff			xon	bool	xo	-	-	YB---	terminal uses xon/xoff handshaking
needs_xon_xoff			nxon	bool	nx	-	-	-----	padding will not work, xon/xoff required
prtr_silent			mc5i	bool	5i	-	-	-----	printer will not echo on screen
hard_cursor			chts	bool	HC	-	-	-----	cursor is hard to see
non_rev_rmcup			nrrmc	bool	NR	-	-	-----	smcup does not reverse rmcup
no_pad_char			npc	bool	NP	-	-	-----	pad character does not exist
non_dest_scroll_region		ndscr	bool	ND	-	-	-----	scrolling region is non-destructive
can_change			ccc	bool	cc	-	-	-----	terminal can re-define existing colors
back_color_erase		bce	bool	ut	-	-	-----	screen erased with background color
hue_lightness_saturation	hls	bool	hl	-	-	-----	terminal uses only HLS color notation (Tektronix)
col_addr_glitch			xhpa	bool	YA	-	-	-----	only positive motion for hpa/mhpa caps
cr_cancels_micro_mode		crxm	bool	YB	-	-	-----	using cr turns off micro mode
has_print_wheel			daisy	bool	YC	-	-	-----	printer needs operator to change character set
row_addr_glitch			xvpa	bool	YD	-	-	-----	only positive motion for vpa/mvpa caps
semi_auto_right_margin		sam	bool	YE	-	-	-----	printing in last column causes cr
cpi_changes_res			cpix	bool	YF	-	-	-----	changing character pitch changes resolution
lpi_changes_res			lpix	bool	YG	-	-	-----	changing line pitch changes resolution
#%.TE
#%.ad
#%
#%These are the numeric capabilities:
#%
#%.na
#%.TS H
#%center expand;
#%c l l c
#%c l l c
#%lw25 lw6 lw2 lw20.
#%\fBVariable	Cap-	TCap	Description\fR
#%\fBNumeric	name	Code\fR
columns				cols	num	co	-	-	YBCGE	number of columns in a line
init_tabs			it	num	it	-	-	YB-G-	tabs initially every # spaces
lines				lines	num	li	-	-	YBCGE	number of lines on screen or page
lines_of_memory			lm	num	lm	-	-	YB-G-	lines of memory if > line. 0 means varies
magic_cookie_glitch		xmc	num	sg	-	-	YBCGE	number of blank characters left by smso or rmso
padding_baud_rate		pb	num	pb	-	-	YB-GE	lowest baud rate where padding needed
virtual_terminal		vt	num	vt	-	-	YB---	virtual terminal number (CB/unix)
width_status_line		wsl	num	ws	-	-	YB-G-	number of columns in status line
num_labels			nlab	num	Nl	-	-	-----	number of labels on screen
label_height			lh	num	lh	-	-	-----	rows in each label
label_width			lw	num	lw	-	-	-----	columns in each label
max_attributes			ma	num	ma	-	-	YBC--	maximum combined attributes terminal can handle
maximum_windows			wnum	num	MW	-	-	-----	maximum number of defineable windows
# These came in with SVr4's color support
max_colors			colors	num	Co	-	-	-----	maximum number of colors on screen
max_pairs			pairs	num	pa	-	-	-----	maximum number of color-pairs on the screen
no_color_video			ncv	num	NC	-	-	-----	video attributes that cannot be used with colors
#%.TE
#%.ad
#%
#%The following numeric capabilities are present in the SVr4.0 term structure,
#%but are not yet documented in the man page.  They came in with SVr4's
#%printer support.
#%
#%.na
#%.TS H
#%center expand;
#%c l l c
#%c l l c
#%lw25 lw6 lw2 lw20.
#%\fBVariable	Cap-	TCap	Description\fR
#%\fBNumeric	name	Code\fR
buffer_capacity			bufsz	num	Ya	-	-	-----	numbers of bytes buffered before printing
dot_vert_spacing		spinv	num	Yb	-	-	-----	spacing of pins vertically in pins per inch
dot_horz_spacing		spinh	num	Yc	-	-	-----	spacing of dots horizontally in dots per inch
max_micro_address		maddr	num	Yd	-	-	-----	maximum value in micro_..._address
max_micro_jump			mjump	num	Ye	-	-	-----	maximum value in parm_..._micro
micro_col_size			mcs	num	Yf	-	-	-----	character step size when in micro mode
micro_line_size			mls	num	Yg	-	-	-----	line step size when in micro mode
number_of_pins			npins	num	Yh	-	-	-----	numbers of pins in print-head
output_res_char			orc	num	Yi	-	-	-----	horizontal resolution in units per line
output_res_line			orl	num	Yj	-	-	-----	vertical resolution in units per line
output_res_horz_inch		orhi	num	Yk	-	-	-----	horizontal resolution in units per inch
output_res_vert_inch		orvi	num	Yl	-	-	-----	vertical resolution in units per inch
print_rate			cps	num	Ym	-	-	-----	print rate in characters per second
wide_char_size			widcs	num	Yn	-	-	-----	character step size when in double wide mode
buttons				btns	num	BT	-	-	-----	number of buttons on mouse
bit_image_entwining		bitwin	num	Yo	-	-	-----	number of passes for each bit-image row
bit_image_type			bitype	num	Yp	-	-	-----	type of bit-image device
#%.TE
#%.ad
#%
#%These are the string capabilities:
#%
#%.na
#%.TS H
#%center expand;
#%c l l c
#%c l l c
#%lw25 lw6 lw2 lw20.
#%\fBVariable	Cap-	TCap	Description\fR
#%\fBString	name	Code\fR
back_tab			cbt	str	bt	-		-	YBCGE	back tab (P)
bell				bel	str	bl	-		-	YB-GE	audible signal (bell) (P)
carriage_return			cr	str	cr	-		-	YBCGE	carriage return (P*) (P*)
change_scroll_region		csr	str	cs	-		-	YBCGE	change region to line #1 to line #2 (P)
clear_all_tabs			tbc	str	ct	-		-	YB-G-	clear all tab stops (P)
clear_screen			clear	str	cl	-		-	YBCGE	clear screen and home cursor (P*)
clr_eol				el	str	ce	-		-	YBCGE	clear to end of line (P)
clr_eos				ed	str	cd	-		-	YBCGE	clear to end of screen (P*)
column_address			hpa	str	ch	-		-	-B-GE*	horizontal position #1, absolute (P)
command_character		cmdch	str	CC	-		-	YB-G-	terminal settable cmd character in prototype !?
cursor_address			cup	str	cm	-		-	YBCGE	move to row #1 columns #2
cursor_down			cud1	str	do	-		-	YBCGE	down one line
cursor_home			home	str	ho	-		-	YBCGE	home cursor (if no cup)
cursor_invisible		civis	str	vi	-		-	YB-G-	make cursor invisible
cursor_left			cub1	str	le	-		-	YBCGE	move left one space
cursor_mem_address		mrcup	str	CM	-		-	YB-G-	memory relative cursor addressing, move to row #1 columns #2
cursor_normal			cnorm	str	ve	-		-	YBCGE	make cursor appear normal (undo civis/cvvis)
cursor_right			cuf1	str	nd	-		-	YBCGE	non-destructive space (move right one space)
cursor_to_ll			ll	str	ll	-		-	YBCGE	last line, first column (if no cup)
cursor_up			cuu1	str	up	-		-	YBCGE	up one line
cursor_visible			cvvis	str	vs	-		-	YBCGE	make cursor very visible
delete_character		dch1	str	dc	-		-	YBCGE	delete character (P*)
delete_line			dl1	str	dl	-		-	YBCGE	delete line (P*)
dis_status_line			dsl	str	ds	-		-	YB-G-	disable status line
down_half_line			hd	str	hd	-		-	YB-G-	half a line down
enter_alt_charset_mode		smacs	str	as	-		-	YB-G-	start alternate character set (P)
enter_blink_mode		blink	str	mb	-		-	YB-G-	turn on blinking
enter_bold_mode			bold	str	md	-		-	YB-G-	turn on bold (extra bright) mode
enter_ca_mode			smcup	str	ti	-		-	YBCGE	string to start programs using cup
enter_delete_mode		smdc	str	dm	-		-	YBCGE	enter delete mode
enter_dim_mode			dim	str	mh	-		-	YB-G-	turn on half-bright mode
enter_insert_mode		smir	str	im	-		-	YBCGE	enter insert mode
enter_secure_mode		invis	str	mk	-		-	-B-G-*	turn on blank mode (characters invisible)
enter_protected_mode		prot	str	mp	-		-	-B-G-*	turn on protected mode
enter_reverse_mode		rev	str	mr	-		-	YB-G-	turn on reverse video mode
enter_standout_mode		smso	str	so	-		-	YBCGE	begin standout mode
enter_underline_mode		smul	str	us	-		-	YBCGE	begin underline mode
erase_chars			ech	str	ec	-		-	YB-G-	erase #1 characters (P)
exit_alt_charset_mode		rmacs	str	ae	-		-	YB-G-	end alternate character set (P)
exit_attribute_mode		sgr0	str	me	-		-	YB-GE	turn off all attributes
exit_ca_mode			rmcup	str	te	-		-	YBCGE	strings to end programs using cup
exit_delete_mode		rmdc	str	ed	-		-	YBCGE	end delete mode
exit_insert_mode		rmir	str	ei	-		-	YBCGE	exit insert mode
exit_standout_mode		rmso	str	se	-		-	YBCGE	exit standout mode
exit_underline_mode		rmul	str	ue	-		-	YBCGE	exit underline mode
flash_screen			flash	str	vb	-		-	YBCGE	visible bell (may not move cursor)
form_feed			ff	str	ff	-		-	YB-G-	hardcopy terminal page eject (P*)
from_status_line		fsl	str	fs	-		-	YB-G-	return from status line
init_1string			is1	str	i1	-		-	YB-G-	initialization string
init_2string			is2	str	is	-		-	YB-G-	initialization string
init_3string			is3	str	i3	-		-	YB-G-	initialization string
init_file			if	str	if	-		-	YB-G-	name of initialization file
insert_character		ich1	str	ic	-		-	YBCGE	insert character (P)
insert_line			il1	str	al	-		-	YBCGE	insert line (P*)
insert_padding			ip	str	ip	-		-	YBCGE	insert padding after inserted character
key_backspace			kbs	str	kb	KEY_BACKSPACE	0407	YB-G-	backspace key
key_catab			ktbc	str	ka	KEY_CATAB	0526	-B-G-*	clear-all-tabs key
key_clear			kclr	str	kC	KEY_CLEAR	0515	-B-G-*	clear-screen or erase key
key_ctab			kctab	str	kt	KEY_CTAB	0525	-B-G-*	clear-tab key
key_dc				kdch1	str	kD	KEY_DC		0512	YB-G-	delete-character key
key_dl				kdl1	str	kL	KEY_DL		0510	-B-G-*	delete-line key
key_down			kcud1	str	kd	KEY_DOWN	0402	YBCGE	down-arrow key
key_eic				krmir	str	kM	KEY_EIC		0514	-B-G-*	sent by rmir or smir in insert mode
key_eol				kel	str	kE	KEY_EOL		0517	-B-G-*	clear-to-end-of-line key
key_eos				ked	str	kS	KEY_EOS		0516	-B-G-*	clear-to-end-of-screen key
key_f0				kf0	str	k0	KEY_F(0)	0410	YBCGE	F0 function key
key_f1				kf1	str	k1	KEY_F(1)	-	YBCGE	F1 function key
key_f10				kf10	str	k;	KEY_F(10)	-	----E	F10 function key
key_f2				kf2	str	k2	KEY_F(2)	-	YBCGE	F2 function key
key_f3				kf3	str	k3	KEY_F(3)	-	YBCGE	F3 function key
key_f4				kf4	str	k4	KEY_F(4)	-	YBCGE	F4 function key
key_f5				kf5	str	k5	KEY_F(5)	-	YBCGE	F5 function key
key_f6				kf6	str	k6	KEY_F(6)	-	YBCGE	F6 function key
key_f7				kf7	str	k7	KEY_F(7)	-	YBCGE	F7 function key
key_f8				kf8	str	k8	KEY_F(8)	-	YBCGE	F8 function key
key_f9				kf9	str	k9	KEY_F(9)	-	YBCGE	F9 function key
key_home			khome	str	kh	KEY_HOME	0406	YBCGE	home key
key_ic				kich1	str	kI	KEY_IC		0513	YB-GE	insert-character key
key_il				kil1	str	kA	KEY_IL		0511	-B-G-*	insert-line key
key_left			kcub1	str	kl	KEY_LEFT	0404	YBCGE	left-arrow key
key_ll				kll	str	kH	KEY_LL		0533	YB-G-	lower-left key (home down)
key_npage			knp	str	kN	KEY_NPAGE	0522	YB-GE	next-page key
key_ppage			kpp	str	kP	KEY_PPAGE	0523	YB-GE	previous-page key
key_right			kcuf1	str	kr	KEY_RIGHT	0405	YBCGE	right-arrow key
key_sf				kind	str	kF	KEY_SF		0520	-B-G-*	scroll-forward key
key_sr				kri	str	kR	KEY_SR		0521	-B-G-*	scroll-backward key
key_stab			khts	str	kT	KEY_STAB	0524	-B-G-*	set-tab key
key_up				kcuu1	str	ku	KEY_UP		0403	YBCGE	up-arrow key
keypad_local			rmkx	str	ke	-		-	YBCGE	leave 'keyboard_transmit' mode
keypad_xmit			smkx	str	ks	-		-	YBCGE	enter 'keyboard_transmit' mode
lab_f0				lf0	str	l0	-		-	-B-G-*	label on function key f0 if not f0
lab_f1				lf1	str	l1	-		-	-B-G-*	label on function key f1 if not f1
lab_f10				lf10	str	la	-		-	-----	label on function key f10 if not f10
lab_f2				lf2	str	l2	-		-	-B-G-*	label on function key f2 if not f2
lab_f3				lf3	str	l3	-		-	-B-G-*	label on function key f3 if not f3
lab_f4				lf4	str	l4	-		-	-B-G-*	label on function key f4 if not f4
lab_f5				lf5	str	l5	-		-	-B-G-*	label on function key f5 if not f5
lab_f6				lf6	str	l6	-		-	-B-G-*	label on function key f6 if not f6
lab_f7				lf7	str	l7	-		-	-B-G-*	label on function key f7 if not f7
lab_f8				lf8	str	l8	-		-	-B-G-*	label on function key f8 if not f8
lab_f9				lf9	str	l9	-		-	-B-G-*	label on function key f9 if not f9
meta_off			rmm	str	mo	-		-	YB-G-*	turn off meta mode
meta_on				smm	str	mm	-		-	YB-G-*	turn on meta mode (8th-bit on)
newline				nel	str	nw	-		-	YB-G-*	newline (behave like cr followed by lf)
pad_char			pad	str	pc	-		-	YBCGE	padding char (instead of null)
parm_dch			dch	str	DC	-		-	YB-GE	delete #1 characters (P*)
parm_delete_line		dl	str	DL	-		-	YBCGE	delete #1 lines (P*)
parm_down_cursor		cud	str	DO	-		-	YBCGE	down #1 lines (P*)
parm_ich			ich	str	IC	-		-	YB-GE	insert #1 characters (P*)
parm_index			indn	str	SF	-		-	YBCG-	scroll forward #1 lines (P)
parm_insert_line		il	str	AL	-		-	YBCGE	insert #1 lines (P*)
parm_left_cursor		cub	str	LE	-		-	YBCGE	move #1 characters to the left (P)
parm_right_cursor		cuf	str	RI	-		-	YBCGE	move #1 characters to the right (P*)
parm_rindex			rin	str	SR	-		-	YBCG-	scroll back #1 lines (P)
parm_up_cursor			cuu	str	UP	-		-	YBCGE	up #1 lines (P*)
pkey_key			pfkey	str	pk	-		-	-B---	program function key #1 to type string #2
pkey_local			pfloc	str	pl	-		-	-B---	program function key #1 to execute string #2
pkey_xmit			pfx	str	px	-		-	-B---	program function key #1 to transmit string #2
print_screen			mc0	str	ps	-		-	-B-G-*	print contents of screen
prtr_off			mc4	str	pf	-		-	-B-G-*	turn off printer
prtr_on				mc5	str	po	-		-	-B-G-*	turn on printer
repeat_char			rep	str	rp	-		-	YB-GE	repeat char #1 #2 times (P*)
reset_1string			rs1	str	r1	-		-	-B---	reset string
reset_2string			rs2	str	r2	-		-	-B---	reset string
reset_3string			rs3	str	r3	-		-	-B---	reset string
reset_file			rf	str	rf	-		-	-B---	name of reset file
restore_cursor			rc	str	rc	-		-	YBCG-	restore cursor to position of last save_cursor
row_address			vpa	str	cv	-		-	-B-GE*	vertical position #1 absolute (P)
save_cursor			sc	str	sc	-		-	YBCG-	save current cursor position (P)
scroll_forward			ind	str	sf	-		-	YBCGE	scroll text up (P)
scroll_reverse			ri	str	sr	-		-	YBCGE	scroll text down (P)
set_attributes			sgr	str	sa	-		-	YB-G-	define video attributes #1-#9 (PG9)
set_tab				hts	str	st	-		-	YB-G-	set a tab in every row, current columns
set_window			wind	str	wi	-		-	-B-GE	current window is lines #1-#2 cols #3-#4
tab				ht	str	ta	-		-	YBCGE	tab to next 8-space hardware tab stop
to_status_line			tsl	str	ts	-		-	YB-G-	move to status line, column #1
underline_char			uc	str	uc	-		-	YBCG-	underline char and move past it
up_half_line			hu	str	hu	-		-	YB-G-	half a line up
init_prog			iprog	str	iP	-		-	-B---	path name of program for initialization
key_a1				ka1	str	K1	KEY_A1		0534	YB-GE	upper left of keypad
key_a3				ka3	str	K3	KEY_A3		0535	YB-GE	upper right of keypad
key_b2				kb2	str	K2	KEY_B2		0536	YB-GE	center of keypad
key_c1				kc1	str	K4	KEY_C1		0537	YB-GE	lower left of keypad
key_c3				kc3	str	K5	KEY_C3		0540	YB-GE	lower right of keypad
prtr_non			mc5p	str	pO	-		-	-B-G-*	turn on printer for #1 bytes
#
# SVr1 capabilities stop here.	IBM's version of terminfo is the same as
# SVr4 up to this point, but has a different set afterwards.
#
char_padding			rmp	str	rP	-		-	-----	like ip but when in insert mode
acs_chars			acsc	str	ac	-		-	-----	graphics charset pairs, based on vt100
plab_norm			pln	str	pn	-		-	-----	program label #1 to show string #2
key_btab			kcbt	str	kB	KEY_BTAB	0541	-----	back-tab key
enter_xon_mode			smxon	str	SX	-		-	-----	turn on xon/xoff handshaking
exit_xon_mode			rmxon	str	RX	-		-	-----	turn off xon/xoff handshaking
enter_am_mode			smam	str	SA	-		-	-----	turn on automatic margins
exit_am_mode			rmam	str	RA	-		-	-----	turn off automatic margins
xon_character			xonc	str	XN	-		-	-----	XON character
xoff_character			xoffc	str	XF	-		-	-----	XOFF character
ena_acs				enacs	str	eA	-		-	-----	enable alternate char set
label_on			smln	str	LO	-		-	-----	turn on soft labels
label_off			rmln	str	LF	-		-	-----	turn off soft labels
key_beg				kbeg	str	@1	KEY_BEG		0542	-----	begin key
key_cancel			kcan	str	@2	KEY_CANCEL	0543	-----	cancel key
key_close			kclo	str	@3	KEY_CLOSE	0544	-----	close key
key_command			kcmd	str	@4	KEY_COMMAND	0545	-----	command key
key_copy			kcpy	str	@5	KEY_COPY	0546	-----	copy key
key_create			kcrt	str	@6	KEY_CREATE	0547	-----	create key
key_end				kend	str	@7	KEY_END		0550	-----	end key
key_enter			kent	str	@8	KEY_ENTER	0527	-----	enter/send key
key_exit			kext	str	@9	KEY_EXIT	0551	-----	exit key
key_find			kfnd	str	@0	KEY_FIND	0552	-----	find key
key_help			khlp	str	%1	KEY_HELP	0553	-----	help key
key_mark			kmrk	str	%2	KEY_MARK	0554	-----	mark key
key_message			kmsg	str	%3	KEY_MESSAGE	0555	-----	message key
key_move			kmov	str	%4	KEY_MOVE	0556	-----	move key
key_next			knxt	str	%5	KEY_NEXT	0557	-----	next key
key_open			kopn	str	%6	KEY_OPEN	0560	-----	open key
key_options			kopt	str	%7	KEY_OPTIONS	0561	-----	options key
key_previous			kprv	str	%8	KEY_PREVIOUS	0562	-----	previous key
key_print			kprt	str	%9	KEY_PRINT	0532	-----	print key
key_redo			krdo	str	%0	KEY_REDO	0563	-----	redo key
key_reference			kref	str	&1	KEY_REFERENCE	0564	-----	reference key
key_refresh			krfr	str	&2	KEY_REFRESH	0565	-----	refresh key
key_replace			krpl	str	&3	KEY_REPLACE	0566	-----	replace key
key_restart			krst	str	&4	KEY_RESTART	0567	-----	restart key
key_resume			kres	str	&5	KEY_RESUME	0570	-----	resume key
key_save			ksav	str	&6	KEY_SAVE	0571	-----	save key
key_suspend			kspd	str	&7	KEY_SUSPEND	0627	-----	suspend key
key_undo			kund	str	&8	KEY_UNDO	0630	-----	undo key
key_sbeg			kBEG	str	&9	KEY_SBEG	0572	-----	shifted begin key
key_scancel			kCAN	str	&0	KEY_SCANCEL	0573	-----	shifted cancel key
key_scommand			kCMD	str	*1	KEY_SCOMMAND	0574	-----	shifted command key
key_scopy			kCPY	str	*2	KEY_SCOPY	0575	-----	shifted copy key
key_screate			kCRT	str	*3	KEY_SCREATE	0576	-----	shifted create key
key_sdc				kDC	str	*4	KEY_SDC		0577	-----	shifted delete-character key
key_sdl				kDL	str	*5	KEY_SDL		0600	-----	shifted delete-line key
key_select			kslt	str	*6	KEY_SELECT	0601	-----	select key
key_send			kEND	str	*7	KEY_SEND	0602	-----	shifted end key
key_seol			kEOL	str	*8	KEY_SEOL	0603	-----	shifted clear-to-end-of-line key
key_sexit			kEXT	str	*9	KEY_SEXIT	0604	-----	shifted exit key
key_sfind			kFND	str	*0	KEY_SFIND	0605	-----	shifted find key
key_shelp			kHLP	str	#1	KEY_SHELP	0606	-----	shifted help key
key_shome			kHOM	str	#2	KEY_SHOME	0607	-----	shifted home key
key_sic				kIC	str	#3	KEY_SIC		0610	-----	shifted insert-character key
key_sleft			kLFT	str	#4	KEY_SLEFT	0611	-----	shifted left-arrow key
key_smessage			kMSG	str	%a	KEY_SMESSAGE	0612	-----	shifted message key
key_smove			kMOV	str	%b	KEY_SMOVE	0613	-----	shifted move key
key_snext			kNXT	str	%c	KEY_SNEXT	0614	-----	shifted next key
key_soptions			kOPT	str	%d	KEY_SOPTIONS	0615	-----	shifted options key
key_sprevious			kPRV	str	%e	KEY_SPREVIOUS	0616	-----	shifted previous key
key_sprint			kPRT	str	%f	KEY_SPRINT	0617	-----	shifted print key
key_sredo			kRDO	str	%g	KEY_SREDO	0620	-----	shifted redo key
key_sreplace			kRPL	str	%h	KEY_SREPLACE	0621	-----	shifted replace key
key_sright			kRIT	str	%i	KEY_SRIGHT	0622	-----	shifted right-arrow key
key_srsume			kRES	str	%j	KEY_SRSUME	0623	-----	shifted resume key
key_ssave			kSAV	str	!1	KEY_SSAVE	0624	-----	shifted save key
key_ssuspend			kSPD	str	!2	KEY_SSUSPEND	0625	-----	shifted suspend key
key_sundo			kUND	str	!3	KEY_SUNDO	0626	-----	shifted undo key
req_for_input			rfi	str	RF	-		-	-----	send next input char (for ptys)
key_f11				kf11	str	F1	KEY_F(11)	-	----E	F11 function key
key_f12				kf12	str	F2	KEY_F(12)	-	----E	F12 function key
key_f13				kf13	str	F3	KEY_F(13)	-	----E	F13 function key
key_f14				kf14	str	F4	KEY_F(14)	-	----E	F14 function key
key_f15				kf15	str	F5	KEY_F(15)	-	----E	F15 function key
key_f16				kf16	str	F6	KEY_F(16)	-	----E	F16 function key
key_f17				kf17	str	F7	KEY_F(17)	-	----E	F17 function key
key_f18				kf18	str	F8	KEY_F(18)	-	----E	F18 function key
key_f19				kf19	str	F9	KEY_F(19)	-	----E	F19 function key
key_f20				kf20	str	FA	KEY_F(20)	-	----E	F20 function key
key_f21				kf21	str	FB	KEY_F(21)	-	----E	F21 function key
key_f22				kf22	str	FC	KEY_F(22)	-	----E	F22 function key
key_f23				kf23	str	FD	KEY_F(23)	-	----E	F23 function key
key_f24				kf24	str	FE	KEY_F(24)	-	----E	F24 function key
key_f25				kf25	str	FF	KEY_F(25)	-	----E	F25 function key
key_f26				kf26	str	FG	KEY_F(26)	-	----E	F26 function key
key_f27				kf27	str	FH	KEY_F(27)	-	----E	F27 function key
key_f28				kf28	str	FI	KEY_F(28)	-	----E	F28 function key
key_f29				kf29	str	FJ	KEY_F(29)	-	----E	F29 function key
key_f30				kf30	str	FK	KEY_F(30)	-	----E	F30 function key
key_f31				kf31	str	FL	KEY_F(31)	-	----E	F31 function key
key_f32				kf32	str	FM	KEY_F(32)	-	----E	F32 function key
key_f33				kf33	str	FN	KEY_F(33)	-	----E	F33 function key
key_f34				kf34	str	FO	KEY_F(34)	-	----E	F34 function key
key_f35				kf35	str	FP	KEY_F(35)	-	----E	F35 function key
key_f36				kf36	str	FQ	KEY_F(36)	-	----E	F36 function key
key_f37				kf37	str	FR	KEY_F(37)	-	----E	F37 function key
key_f38				kf38	str	FS	KEY_F(38)	-	----E	F38 function key
key_f39				kf39	str	FT	KEY_F(39)	-	----E	F39 function key
key_f40				kf40	str	FU	KEY_F(40)	-	----E	F40 function key
key_f41				kf41	str	FV	KEY_F(41)	-	----E	F41 function key
key_f42				kf42	str	FW	KEY_F(42)	-	----E	F42 function key
key_f43				kf43	str	FX	KEY_F(43)	-	----E	F43 function key
key_f44				kf44	str	FY	KEY_F(44)	-	----E	F44 function key
key_f45				kf45	str	FZ	KEY_F(45)	-	----E	F45 function key
key_f46				kf46	str	Fa	KEY_F(46)	-	----E	F46 function key
key_f47				kf47	str	Fb	KEY_F(47)	-	----E	F47 function key
key_f48				kf48	str	Fc	KEY_F(48)	-	----E	F48 function key
key_f49				kf49	str	Fd	KEY_F(49)	-	----E	F49 function key
key_f50				kf50	str	Fe	KEY_F(50)	-	----E	F50 function key
key_f51				kf51	str	Ff	KEY_F(51)	-	----E	F51 function key
key_f52				kf52	str	Fg	KEY_F(52)	-	----E	F52 function key
key_f53				kf53	str	Fh	KEY_F(53)	-	----E	F53 function key
key_f54				kf54	str	Fi	KEY_F(54)	-	----E	F54 function key
key_f55				kf55	str	Fj	KEY_F(55)	-	----E	F55 function key
key_f56				kf56	str	Fk	KEY_F(56)	-	----E	F56 function key
key_f57				kf57	str	Fl	KEY_F(57)	-	----E	F57 function key
key_f58				kf58	str	Fm	KEY_F(58)	-	----E	F58 function key
key_f59				kf59	str	Fn	KEY_F(59)	-	----E	F59 function key
key_f60				kf60	str	Fo	KEY_F(60)	-	----E	F60 function key
key_f61				kf61	str	Fp	KEY_F(61)	-	----E	F61 function key
key_f62				kf62	str	Fq	KEY_F(62)	-	----E	F62 function key
key_f63				kf63	str	Fr	KEY_F(63)	-	----E	F63 function key
clr_bol				el1	str	cb	-		-	-----	Clear to beginning of line
clear_margins			mgc	str	MC	-		-	-----	clear right and left soft margins
set_left_margin			smgl	str	ML	-		-	-----	set left soft margin at current column.	 See smgl. (ML is not in BSD termcap).
set_right_margin		smgr	str	MR	-		-	-----	set right soft margin at current column
label_format			fln	str	Lf	-		-	-----	label format
set_clock			sclk	str	SC	-		-	-----	set clock, #1 hrs #2 mins #3 secs
display_clock			dclk	str	DK	-		-	-----	display clock
remove_clock			rmclk	str	RC	-		-	-----	remove clock
create_window			cwin	str	CW	-		-	-----	define a window #1 from #2,#3 to #4,#5
goto_window			wingo	str	WG	-		-	-----	go to window #1
hangup				hup	str	HU	-		-	-----	hang-up phone
dial_phone			dial	str	DI	-		-	-----	dial number #1
quick_dial			qdial	str	QD	-		-	-----	dial number #1 without checking
tone				tone	str	TO	-		-	-----	select touch tone dialing
pulse				pulse	str	PU	-		-	-----	select pulse dialing
flash_hook			hook	str	fh	-		-	-----	flash switch hook
fixed_pause			pause	str	PA	-		-	-----	pause for 2-3 seconds
wait_tone			wait	str	WA	-		-	-----	wait for dial-tone
user0				u0	str	u0	-		-	-----	User string #0
user1				u1	str	u1	-		-	-----	User string #1
user2				u2	str	u2	-		-	-----	User string #2
user3				u3	str	u3	-		-	-----	User string #3
user4				u4	str	u4	-		-	-----	User string #4
user5				u5	str	u5	-		-	-----	User string #5
user6				u6	str	u6	-		-	-----	User string #6
user7				u7	str	u7	-		-	-----	User string #7
user8				u8	str	u8	-		-	-----	User string #8
user9				u9	str	u9	-		-	-----	User string #9
#
# SVr4 added these capabilities to support color
#
orig_pair			op	str	op	-		-	-----	Set default pair to its original value
orig_colors			oc	str	oc	-		-	-----	Set all color pairs to the original ones
initialize_color		initc	str	Ic	-		-	-----	initialize color #1 to (#2,#3,#4)
initialize_pair			initp	str	Ip	-		-	-----	Initialize color pair #1 to fg=(#2,#3,#4), bg=(#5,#6,#7)
set_color_pair			scp	str	sp	-		-	-----	Set current color pair to #1
set_foreground			setf	str	Sf	-		-	-----	Set foreground color #1
set_background			setb	str	Sb	-		-	-----	Set background color #1
#
# SVr4 added these capabilities to support printers
#
change_char_pitch		cpi	str	ZA	-		-	-----	Change number of characters per inch to #1
change_line_pitch		lpi	str	ZB	-		-	-----	Change number of lines per inch to #1
change_res_horz			chr	str	ZC	-		-	-----	Change horizontal resolution to #1
change_res_vert			cvr	str	ZD	-		-	-----	Change vertical resolution to #1
define_char			defc	str	ZE	-		-	-----	Define a character #1, #2 dots wide, descender #3
enter_doublewide_mode		swidm	str	ZF	-		-	-----	Enter double-wide mode
enter_draft_quality		sdrfq	str	ZG	-		-	-----	Enter draft-quality mode
enter_italics_mode		sitm	str	ZH	-		-	-----	Enter italic mode
enter_leftward_mode		slm	str	ZI	-		-	-----	Start leftward carriage motion
enter_micro_mode		smicm	str	ZJ	-		-	-----	Start micro-motion mode
enter_near_letter_quality	snlq	str	ZK	-		-	-----	Enter NLQ mode
enter_normal_quality		snrmq	str	ZL	-		-	-----	Enter normal-quality mode
enter_shadow_mode		sshm	str	ZM	-		-	-----	Enter shadow-print mode
enter_subscript_mode		ssubm	str	ZN	-		-	-----	Enter subscript mode
enter_superscript_mode		ssupm	str	ZO	-		-	-----	Enter superscript mode
enter_upward_mode		sum	str	ZP	-		-	-----	Start upward carriage motion
exit_doublewide_mode		rwidm	str	ZQ	-		-	-----	End double-wide mode
exit_italics_mode		ritm	str	ZR	-		-	-----	End italic mode
exit_leftward_mode		rlm	str	ZS	-		-	-----	End left-motion mode
exit_micro_mode			rmicm	str	ZT	-		-	-----	End micro-motion mode
exit_shadow_mode		rshm	str	ZU	-		-	-----	End shadow-print mode
exit_subscript_mode		rsubm	str	ZV	-		-	-----	End subscript mode
exit_superscript_mode		rsupm	str	ZW	-		-	-----	End superscript mode
exit_upward_mode		rum	str	ZX	-		-	-----	End reverse character motion
micro_column_address		mhpa	str	ZY	-		-	-----	Like column_address in micro mode
micro_down			mcud1	str	ZZ	-		-	-----	Like cursor_down in micro mode
micro_left			mcub1	str	Za	-		-	-----	Like cursor_left in micro mode
micro_right			mcuf1	str	Zb	-		-	-----	Like cursor_right in micro mode
micro_row_address		mvpa	str	Zc	-		-	-----	Like row_address #1 in micro mode
micro_up			mcuu1	str	Zd	-		-	-----	Like cursor_up in micro mode
order_of_pins			porder	str	Ze	-		-	-----	Match software bits to print-head pins
parm_down_micro			mcud	str	Zf	-		-	-----	Like parm_down_cursor in micro mode
parm_left_micro			mcub	str	Zg	-		-	-----	Like parm_left_cursor in micro mode
parm_right_micro		mcuf	str	Zh	-		-	-----	Like parm_right_cursor in micro mode
parm_up_micro			mcuu	str	Zi	-		-	-----	Like parm_up_cursor in micro mode
select_char_set			scs	str	Zj	-		-	-----	Select character set, #1
set_bottom_margin		smgb	str	Zk	-		-	-----	Set bottom margin at current line
set_bottom_margin_parm		smgbp	str	Zl	-		-	-----	Set bottom margin at line #1 or (if smgtp is not given) #2 lines from bottom
set_left_margin_parm		smglp	str	Zm	-		-	-----	Set left (right) margin at column #1
set_right_margin_parm		smgrp	str	Zn	-		-	-----	Set right margin at column #1
set_top_margin			smgt	str	Zo	-		-	-----	Set top margin at current line
set_top_margin_parm		smgtp	str	Zp	-		-	-----	Set top (bottom) margin at row #1
start_bit_image			sbim	str	Zq	-		-	-----	Start printing bit image graphics
start_char_set_def		scsd	str	Zr	-		-	-----	Start character set definition #1, with #2 characters in the set
stop_bit_image			rbim	str	Zs	-		-	-----	Stop printing bit image graphics
stop_char_set_def		rcsd	str	Zt	-		-	-----	End definition of character set #1
subscript_characters		subcs	str	Zu	-		-	-----	List of subscriptable characters
superscript_characters		supcs	str	Zv	-		-	-----	List of superscriptable characters
these_cause_cr			docr	str	Zw	-		-	-----	Printing any of these characters causes CR
zero_motion			zerom	str	Zx	-		-	-----	No motion for subsequent character
#%.TE
#%.ad
#%
#%The following string capabilities are present in the SVr4.0 term structure,
#%but were originally not documented in the man page.
#%
#%.na
#%.TS H
#%center expand;
#%c l l c
#%c l l c
#%lw25 lw6 lw2 lw18.
#%\fBVariable	Cap-	TCap	Description\fR
#%\fBString	name	Code\fR
char_set_names			csnm	str	Zy	-		-	-----	Produce #1'th item from list of character set names
key_mouse			kmous	str	Km	KEY_MOUSE	0631	-----	Mouse event has occurred
mouse_info			minfo	str	Mi	-		-	-----	Mouse status information
req_mouse_pos			reqmp	str	RQ	-		-	-----	Request mouse position
get_mouse			getm	str	Gm	-		-	-----	Curses should get button events, parameter #1 not documented.
set_a_foreground		setaf	str	AF	-		-	-----	Set foreground color to #1, using ANSI escape
set_a_background		setab	str	AB	-		-	-----	Set background color to #1, using ANSI escape
pkey_plab			pfxl	str	xl	-		-	-----	Program function key #1 to type string #2 and show string #3
device_type			devt	str	dv	-		-	-----	Indicate language/codeset support
code_set_init			csin	str	ci	-		-	-----	Init sequence for multiple codesets
set0_des_seq			s0ds	str	s0	-		-	-----	Shift to codeset 0 (EUC set 0, ASCII)
set1_des_seq			s1ds	str	s1	-		-	-----	Shift to codeset 1
set2_des_seq			s2ds	str	s2	-		-	-----	Shift to codeset 2
set3_des_seq			s3ds	str	s3	-		-	-----	Shift to codeset 3
set_lr_margin			smglr	str	ML	-		-	-----	Set both left and right margins to #1, #2.  (ML is not in BSD termcap).
set_tb_margin			smgtb	str	MT	-		-	-----	Sets both top and bottom margins to #1, #2
bit_image_repeat		birep	str	Xy	-		-	-----	Repeat bit image cell #1 #2 times
bit_image_newline		binel	str	Zz	-		-	-----	Move to next row of the bit image
bit_image_carriage_return	bicr	str	Yv	-		-	-----	Move to beginning of same row
color_names			colornm	str	Yw	-		-	-----	Give name for color #1
define_bit_image_region		defbi	str	Yx	-		-	-----	Define rectangualar bit image region
end_bit_image_region		endbi	str	Yy	-		-	-----	End a bit-image region
set_color_band		setcolor	str	Yz	-		-	-----	Change to ribbon color #1
set_page_length			slines	str	YZ	-		-	-----	Set page length to #1 lines
#
# SVr4 added these capabilities for direct PC-clone support
#
display_pc_char			dispc	str	S1	-		-	-----	Display PC character #1
enter_pc_charset_mode		smpch	str	S2	-		-	-----	Enter PC character display mode
exit_pc_charset_mode		rmpch	str	S3	-		-	-----	Exit PC character display mode
enter_scancode_mode		smsc	str	S4	-		-	-----	Enter PC scancode mode
exit_scancode_mode		rmsc	str	S5	-		-	-----	Exit PC scancode mode
pc_term_options			pctrm	str	S6	-		-	-----	PC terminal options
scancode_escape			scesc	str	S7	-		-	-----	Escape for scancode emulation
alt_scancode_esc		scesa	str	S8	-		-	-----	Alternate escape for scancode emulation
#%.TE
#%.ad
#%
#%.in .8i
#%The XSI Curses standard added these.  They are some post-4.1 
#%versions of System V curses, e.g., Solaris 2.5 and IRIX 6.x.
#%The \fBncurses\fR termcap names for them are invented; according to the
#%XSI Curses standard, they have no termcap names.  If your compiled terminfo
#%entries use these, they may not be binary-compatible with System V terminfo
#%entries after SVr4.1; beware!
#%
#%.na
#%.TS H
#%center expand;
#%c l l c
#%c l l c
#%lw25 lw6 lw2 lw20.
#%\fBVariable	Cap-	TCap	Description\fR
#%\fBString	name	Code\fR
enter_horizontal_hl_mode	ehhlm	str	Xh	-		-	-----	Enter horizontal highlight mode
enter_left_hl_mode		elhlm	str	Xl	-		-	-----	Enter left highlight mode
enter_low_hl_mode		elohlm	str	Xo	-		-	-----	Enter low highlight mode
enter_right_hl_mode		erhlm	str	Xr	-		-	-----	Enter right highlight mode
enter_top_hl_mode		ethlm	str	Xt	-		-	-----	Enter top highlight mode
enter_vertical_hl_mode		evhlm	str	Xv	-		-	-----	Enter vertical highlight mode
set_a_attributes		sgr1	str	sA	-		-	-----	Define second set of video attributes #1-#6
set_pglen_inch			slength	str	sL	-		-	-----	YI Set page length to #1 hundredth of an inch
#%.TE
#%.ad
#
# The magic token below tells the tic compiler-generator code that all the caps
# past it should be ignored (not written out) when dumping terminfo objects. It
# also tells the man page table generator not to pass through following lines
# This means we can have obsolete capabilities and pseudo-capabilities that are
# recognized for termcap or terminfo compilation, but not output.
#
# %%-STOP-HERE-%%
#
# Don't move this casually!  In fact, don't move it at all unless you're
# either doing it to add System V or XPG4 extensions, or have decided you
# don't care about SVr4 binary compatibility.
#
#############################################################################
#
# TERMCAP EXTENSION CAPABILITIES
#
# The capabilities below are either obsolete or extensions on certain systems.
# They are not used by SVR4 terminfo.  Some are used by captoinfo to translate
# termcap sources; the rest are listed for completeness, and in case somebody
# cares about them enough to hack in code that will translate them into
# terminfo capabilities.
#
# The first part of the list is from Ross Ridge's `mytinfo' package
# (comp.sources.unix, volume 26); the variable names and terminfo names (as
# well as the termcap codes) match his list.
#
# This group of codes is not marked obsolete in 4.4BSD, but have no direct
# terminfo equivalents.  The rs capability is specially translated to terminfo
# r2, and vice versa, if an entry does not already have an r2.  Similarly,
# i2 is translated to r3 if there is no r3 (because SV terminfo maps is to i2).
# The ug capability is thrown away, but assumed to be whatever sg is if the
# latter is nonzero and we're dumping in termcap format.
#
termcap_init2			OTi2	str	i2	-		-	YB---	secondary initialization string
termcap_reset			OTrs	str	rs	-		-	YB-G-	terminal reset string
magic_cookie_glitch_ul		OTug	num	ug	-		-	YBCGE	number of blanks left by ul
#
# Obsolete termcap capabilities.  Some are used for termcap translation.  The
# code uses the 'OT' prefix we put on obsolete capabilities to suppress
# printing them in terminfo source dumps of compiled entries.
#
backspaces_with_bs		OTbs	bool	bs	-		-	YBCGE	uses ^H to move left
crt_no_scrolling		OTns	bool	ns	-		-	YBCG-	crt cannot scroll
no_correctly_working_cr		OTnc	bool	nc	-		-	YBCG-	no way to go to start of line
carriage_return_delay		OTdC	num	dC	-		-	YB-G-	pad needed for CR
new_line_delay			OTdN	num	dN	-		-	YB-G-	pad needed for LF
linefeed_if_not_lf		OTnl	str	nl	-		-	YBCGE	use to move down
backspace_if_not_bs		OTbc	str	bc	-		-	YBCGE	move left, if not ^H
#
# GNU termcap library extensions.  The GNU termcap file distributed with
# Emacs no longer uses these, but MT showed up in pre-9.0 versions of the
# BSD termcap file.  The name clash with terminfo MT is resolved by type
# info; MT is converted to km.
#
gnu_has_meta_key		OTMT	bool	MT	-		-	----E	has meta key
# gnu_tab_width			OTtw	num	tw	-		-	----E	tab width in spaces
#
# GNU termcap *does* include the following extended capability,  Only the
# now-obsolete Ann Arbor terminals used it.
#
# gnu_change_scroll_region	OTcS	str	cS	-		-	---GE	alternate set scrolling region 
#
# The following comments describe capnames so ancient that I believe no
# software uses them any longer.  Some of these have to go because they
# clash with terminfo names in ways that cannot be resolved by type
# information.
#
# These mytinfo codes are not used in the 4.4BSD curses code.  They are
# marked obsolete in the 4.4BSD manual pages.
#
# There is one conflict with terminfo; ma is in both.  This conflict is
# resolved by type information.
#
# The `ko' capability is translated by special code.  It should contain a
# comma-separated list of capabilities for which there are corresponding keys.
# The `kn' code is accepted but ignored.
#
# The `ma' capability seems to have been designed to map between the rogue(2)
# motion keys (including jkhl) and characters emitted by arrow keys on some
# primitive pre-ANSI terminals.  It's so obsolete it's fossilized...
#
# Here is a description of memory_lock_above and memory_unlock:
# "You can 'freeze' data on the screen by turning on Memory Lock in a line of
# text.  All lines above the cursor's current line become locked in place on
# the screen.  Then enter data normally.  When the screen fills up, any
# further data entered forces the first line of unfrozen line text to scroll
# under the frozen data.  Lines scrolled off the screen are inserted into
# memory immediately preceding the first frozen line." (from the HP 700/96
# User's manual).  VT100/ANSI memory lock set is \E[>2h, reset is \E[>2l.
#
# Applications that use terminfo are supposed to behave as though xr is
# always true.
#
linefeed_is_newline		OTNL	bool	NL	-		-	YB---	move down with \n
# even_parity			OTEP	bool	EP	-		-	-B---	terminal requires even parity
# odd_parity			OTOP	bool	OP	-		-	-B---	terminal requires odd parity
# half_duplex			OTHD	bool	HD	-		-	-B---	terminal is half-duplex
# lower_case_only		OTLC	bool	LC	-		-	-B---	terminal has only lower case
# upper_case_only		OTUC	bool	UC	-		-	-B---	terminal has only upper case
backspace_delay			OTdB	num	dB	-		-	YB-G-	padding required for ^H
# form_feed_delay		OTdF	num	dF	-		-	-B-G-	padding required for ^L
horizontal_tab_delay		OTdT	num	dT	-		-	YB-G-	padding required for ^I
# vertical_tab_delay		OTdV	num	dV	-		-	-B---	padding required for ^V
number_of_function_keys		OTkn	num	kn	-		-	-B-G-	count of function keys
other_non_function_keys		OTko	str	ko	-		-	-B-G-	list of self-mapped keycaps
arrow_key_map			OTma	str	ma	-		-	YBC--	map arrow keys rogue(1) motion keys
# memory_lock_above		OTml	str	ml	-		-	-B---	lock visible screen memory above the current line
# memory_unlock			OTmu	str	mu	-		-	-B---	unlock visible screen memory above the current line
has_hardware_tabs		OTpt	bool	pt	-		-	YB---	has 8-char tabs invoked with ^I
return_does_clr_eol		OTxr	bool	xr	-		-	YB---	return clears the line
# tek_4025_insert_line		OTxx	bool	xx	-		-	-BC--	Tektronix 4025 insert-line glitch
#
# mytinfo described this as a termcap capability, but it's not listed in the
# 4.4BSD man pages, and not found in the 4.4BSD termcap file.  The ncurses
# package, like System V, behaves as though it is always true.
#
# rind_only_at_top		OTxq	bool	xq	-		-	-----	reverse index only works from top line
#
# University of Waterloo termcap extensions (as described in mytinfo).
# The `xl' termcap file clashes with a terminfo name; this ambiguity cannot
# be resolved by a type check.  The descriptions are guesses from what was
# in the mytinfo tables. 
#
# key_interrupt_char		OTki	str	ki	-		-	-----	string set by interrupt key (?)
# key_kill_char			OTkk	str	kk	-		-	-----	string set by kill key (?)
# key_suspend_char		OTkz	str	kz	-		-	-----	string set by suspend key (?)
# initialization_messy		OTxc	bool	xc	-		-	-----	initialization leaves garbage on the screen (?)
# ind_at_bottom_does_cr		OTxl	bool	xl	-		-	-----	index does a carriage return
#
# Nonstandard capabilities unique to Ross Ridge's `mytinfo' package.
# SR clashes with a terminfo name; this ambiguity cannot be resolved by a type
# check.
#
# scroll_left			OTsl1	str	Sl	-		-	-----	scroll screen leftward
# scroll_right			OTsr1	str	Sr	-		-	-----	scroll screen rightward
# parm_scroll_left		OTsl	str	SL	-		-	-----	scroll screen leftward #1 characters
# parm_scroll_right		OTsr	str	SR	-		-	-----	scroll screen rightward #1 characters
#
# The mytinfo capabilities end here.
#
# XENIX extensions:
#
# Xenix defined its own set of forms-drawing capabilities:
#
# cap	IBM ASCII	description             ACS         	ASCII
# ---	-----------	--------------------    -------------	------
# G1	191 \277 M-?	single upper right   	ACS_URCORNER
# G2	218 \332 M-Z	single upper left	ACS_ULCORNER
# G3	192 \300 M-@	single lower left	ACS_LLCORNER
# G4	217 \331 M-Y	single lower right	ACS_LRCORNER
# G5	187 \273 M-;	double upper right
# G6	201 \311 M-I	double upper left
# G7	200 \310 M-H	double lower left
# G8	188 \274 M-<	double lower right
# GC	197 \305 M-E	single intersection	ACS_PLUS	_ _
# GD	194 \302 M-B	single down-tick	ACS_TTEE	 |
# GH	196 \304 M-D	single horizontal line	ACS_HLINE
# GL	180 \264 M-4	single left tick	ACS_RTEE	-|
# GR	195 \303 M-C	single right tick	ACS_LTEE	|-
# GU	193 \301 M-A	single up tick		ACS_BTEE	_|_
# GV	179 \263 M-3	single vertical line	ACS_VLINE
# Gc	206 \316 M-N	double intersection
# Gd	203 \313 M-K	double down tick
# Gh	205 \315 M-M	double horizontal line
# Gl	204 \204 M-L	double left tick
# Gr	185 \271 M-9	double right tick
# Gu	202 \312 M-J	double up tick
# Gv	186 \272 M-:	double vertical line
#
# The compiler will translate the single-line caps and discard the others
# (via IGNORE aliases further down).  We don't want to do normal pad 
# translation on these, they're often single-character printable ASCII
# strings that happen to be numerics.  There's awk code in parametrized.sh
# that detects the acs_ prefix and uses it to suppress pad translation.
# These terminfo names are invented.
#
acs_ulcorner			OTG2	str	G2	-		-	-----	single upper left
acs_llcorner			OTG3	str	G3	-		-	-----	single lower left
acs_urcorner			OTG1	str	G1	-		-	-----	single upper right
acs_lrcorner			OTG4	str	G4	-		-	-----	single lower right
acs_ltee			OTGR	str	GR	-		-	-----	tee pointing right
acs_rtee			OTGL	str	GL	-		-	-----	tee pointing left
acs_btee			OTGU	str	GU	-		-	-----	tee pointing up
acs_ttee			OTGD	str	GD	-		-	-----	tee pointing down
acs_hline			OTGH	str	GH	-		-	-----	single horizontal line
acs_vline			OTGV	str	GV	-		-	-----	single vertical line
acs_plus			OTGC	str	GC	-		-	-----	single intersection
#
#############################################################################
#
# TERMINFO EXTENSION CAPABILITIES
#
# This section is almost all comments.  What it's mainly for is to describe
# what capabilities need to be squeezed out to get down to the XSI Curses
# standard set.  They are flagged with K.
#
# HP extensions
#
# These extensions follow ptr_non (replacing everything after it) in HP
# terminfo files.  Except for memory_lock and memory_unlock, they are
# functionally identical to SVr4 extensions, but they make the binary format
# different.  Grrr....
#
memory_lock			meml	str	ml	-		-	----K	lock memory above cursor
memory_unlock			memu	str	mu	-		-	----K	unlock memory
#plab_norm			pln	str	pn	-		-	-----	program label #1 to show string #2
#label_on			smln	str	LO	-		-	-----	turn on soft labels
#label_off			rmln	str	LF	-		-	-----	turn off soft labels
#key_f11			kf11	str	F1	-		-	-----	F11 function key
#key_f12			kf12	str	F2	-		-	-----	F12 function key
#key_f13			kf13	str	F3	-		-	-----	F13 function key
#key_f14			kf14	str	F4	-		-	-----	F14 function key
#key_f15			kf15	str	F5	-		-	-----	F15 function key
#key_f16			kf16	str	F6	-		-	-----	F16 function key
#key_f17			kf17	str	F7	-		-	-----	F17 function key
#key_f18			kf18	str	F8	-		-	-----	F18 function key
#key_f19			kf19	str	F9	-		-	-----	F19 function key
#key_f20			kf20	str	FA	-		-	-----	F20 function key
#key_f21			kf21	str	FB	-		-	-----	F21 function key
#key_f22			kf22	str	FC	-		-	-----	F22 function key
#key_f23			kf23	str	FD	-		-	-----	F23 function key
#key_f24			kf24	str	FE	-		-	-----	F24 function key
#key_f25			kf25	str	FF	-		-	-----	F25 function key
#key_f26			kf26	str	FG	-		-	-----	F26 function key
#key_f27			kf27	str	FH	-		-	-----	F27 function key
#key_f28			kf28	str	FI	-		-	-----	F28 function key
#key_f29			kf29	str	FJ	-		-	-----	F29 function key
#key_f30			kf30	str	FK	-		-	-----	F30 function key
#key_f31			kf31	str	FL	-		-	-----	F31 function key
#key_f32			kf32	str	FM	-		-	-----	F32 function key
#key_f33			kf33	str	FN	-		-	-----	F33 function key
#key_f34			kf34	str	FO	-		-	-----	F34 function key
#key_f35			kf35	str	FP	-		-	-----	F35 function key
#key_f36			kf36	str	FQ	-		-	-----	F36 function key
#key_f37			kf37	str	FR	-		-	-----	F37 function key
#key_f38			kf38	str	FS	-		-	-----	F38 function key
#key_f39			kf39	str	FT	-		-	-----	F39 function key
#key_f40			kf40	str	FU	-		-	-----	F40 function key
#key_f41			kf41	str	FV	-		-	-----	F41 function key
#key_f42			kf42	str	FW	-		-	-----	F42 function key
#key_f43			kf43	str	FX	-		-	-----	F43 function key
#key_f44			kf44	str	FY	-		-	-----	F44 function key
#key_f45			kf45	str	FZ	-		-	-----	F45 function key
#key_f46			kf46	str	Fa	-		-	-----	F46 function key
#key_f47			kf47	str	Fb	-		-	-----	F47 function key
#key_f48			kf48	str	Fc	-		-	-----	F48 function key
#key_f49			kf49	str	Fd	-		-	-----	F49 function key
#key_f50			kf50	str	Fe	-		-	-----	F50 function key
#key_f51			kf51	str	Ff	-		-	-----	F51 function key
#key_f52			kf52	str	Fg	-		-	-----	F52 function key
#key_f53			kf53	str	Fh	-		-	-----	F53 function key
#key_f54			kf54	str	Fi	-		-	-----	F54 function key
#key_f55			kf55	str	Fj	-		-	-----	F55 function key
#key_f56			kf56	str	Fk	-		-	-----	F56 function key
#key_f57			kf57	str	Fl	-		-	-----	F57 function key
#key_f58			kf58	str	Fm	-		-	-----	F58 function key
#key_f59			kf59	str	Fn	-		-	-----	F59 function key
#key_f60			kf60	str	Fo	-		-	-----	F60 function key
#key_f61			kf61	str	Fp	-		-	-----	F61 function key
#key_f62			kf62	str	Fq	-		-	-----	F62 function key
#key_f63			kf63	str	Fr	-		-	-----	F63 function key
#
# IBM extensions
#
# These extensions follow ptr_non (replacing everything after it) in IBM
# terminfo files.
#
# The places in the box[12] capabilities correspond to acsc characters, here is
# the mapping:
#
#	box1[0]  = ACS_ULCORNER
#	box1[1]  = ACS_HLINE	
#	box1[2]  = ACS_URCORNER
#	box1[3]  = ACS_VLINE
#	box1[4]  = ACS_LRCORNER
#	box1[5]  = ACS_LLCORNER
#	box1[6]  = ACS_TTEE
#	box1[7]  = ACS_RTEE
#	box1[8]  = ACS_BTEE
#	box1[9]  = ACS_LTEE
#	box1[10] = ACS_PLUS
#
# The box2 characters are the double-line versions of these forms graphics.
#
box_chars_1			box1	str	bx	-		-	----K	box characters primary set
#box_chars_2			box2	str	by	-		-	----K	box characters secondary set
#box_attr_1			batt1	str	Bx	-		-	----K	attributes for box1
#box_attr_2			batt2	str	By	-		-	----K	attributes for box2
#color_bg_0			colb0	str	d0	-		-	----K	background color 0
#color_bg_1			colb1	str	d1	-		-	----K	background color 1
#color_bg_2			colb2	str	d2	-		-	----K	background color 2
#color_bg_3			colb3	str	d3	-		-	----K	background color 3
#color_bg_4			colb4	str	d4	-		-	----K	background color 4
#color_bg_5			colb5	str	d5	-		-	----K	background color 5
#color_bg_6			colb6	str	d6	-		-	----K	background color 6
#color_bg_7			colb7	str	d7	-		-	----K	background color 7
#color_fg_0			colf0	str	c0	-		-	----K	foreground color 0
#color_fg_1			colf1	str	c1	-		-	----K	foreground color 1
#color_fg_2			colf2	str	c2	-		-	----K	foreground color 2
#color_fg_3			colf3	str	c3	-		-	----K	foreground color 3
#color_fg_4			colf4	str	c4	-		-	----K	foreground color 4
#color_fg_5			colf5	str	c5	-		-	----K	foreground color 5
#color_fg_6			colf6	str	c6	-		-	----K	foreground color 6
#color_fg_7			colf7	str	c7	-		-	----K	foreground color 7
#font_0				font0	str	f0	-		-	-----	select font 0
#font_1				font1	str	f1	-		-	-----	select font 1
#font_2				font2	str	f2	-		-	-----	select font 2
#font_3				font3	str	f3	-		-	-----	select font 3
#font_4				font4	str	f4	-		-	----K	select font 4
#font_5				font5	str	f5	-		-	----K	select font 5
#font_6				font6	str	f6	-		-	----K	select font 6
#font_7				font7	str	f7	-		-	----K	select font 7
#key_back_tab			kbtab	str	k0	-		-	-----	backtab key
#key_do				kdo	str	ki	-		-	----K	do request key
#key_command			kcmd	str	kd	-		-	----K	command-request key
#key_command_pane		kcpn	str	kW	-		-	----K	command-pane key
#key_end			kend	str	kw	-		-	-----	end key
#key_help			khlp	str	kq	-		-	-----	help key
#key_newline			knl	str	nl	-		-	----K	newline key
#key_next_pane			knpn	str	kv	-		-	----K	next-pane key
#key_prev_cmd			kppn	str	kp	-		-	----K	previous-command key
#key_prev_pane			kppn	str	kV	-		-	----K	previous-pane key
#key_quit			kquit	str	kQ	-		-	----K	quit key
#key_select			ksel	str	kU	-		-	-----	select key
#key_scroll_left		kscl	str	kz	-		-	----K	scroll left
#key_scroll_right		kscr	str	kZ	-		-	----K	scroll right
#key_tab			ktab	str	ko	-		-	----K	tab key
#key_smap_in1			kmpf1	str	Kv	-		-	----K	special mapped key 1 input
#key_smap_out1			kmpt1	str	KV	-		-	----K	special mapped key 1 output
#key_smap_in2			kmpf2	str	Kw	-		-	----K	special mapped key 2 input
#key_smap_out2			kmpt2	str	KW	-		-	----K	special mapped key 2 output
#key_smap_in3			kmpf3	str	Kx	-		-	----K	special mapped key 3 input
#key_smap_out3			kmpt3	str	KX	-		-	----K	special mapped key 3 output
#key_smap_in4			kmpf4	str	Ky	-		-	----K	special mapped key 4 input
#key_smap_out4			kmpt4	str	KY	-		-	----K	special mapped key 4 output
#key_smap_in5			kmpf5	str	Kz	-		-	----K	special mapped key 5 input
#key_smap_out5			kmpt5	str	KZ	-		-	----K	special mapped key 5 output
#appl_defined_str		apstr	str	za	-		-	----K	application-defined string
# The key_smap_in[6789] and key_smap_out[6789] capabilities aren't described in
# the IBM manual pages, so the cap name strings are guesses.  The terminfo
# names are almost certainly right, the termcap ones almost certainly wrong.
#key_smap_in6			kmpf6	str	k!	-		-	----K	special mapped key 6 input
#key_smap_out6			kmpt6	str	K@	-		-	----K	special mapped key 6 output
#key_smap_in7			kmpf7	str	k#	-		-	----K	special mapped key 7 input
#key_smap_out7			kmpt7	str	K$	-		-	----K	special mapped key 7 output
#key_smap_in8			kmpf8	str	k%	-		-	----K	special mapped key 8 input
#key_smap_out8			kmpt8	str	K^	-		-	----K	special mapped key 8 output
#key_smap_in9			kmpf9	str	k&	-		-	----K	special mapped key 9 input
#key_smap_out9			kmpt9	str	K*	-		-	----K	special mapped key 9 output
# Undocumented capabilities end here
#key_sf1			ksf1	str	S1	-		-	----K	special function key 1
#key_sf2			ksf2	str	S2	-		-	----K	special function key 2
#key_sf3			ksf3	str	S3	-		-	----K	special function key 3
#key_sf4			ksf4	str	S4	-		-	----K	special function key 4
#key_sf5			ksf5	str	S5	-		-	----K	special function key 5
#key_sf6			ksf6	str	S6	-		-	----K	special function key 6
#key_sf7			ksf7	str	S7	-		-	----K	special function key 7
#key_sf8			ksf8	str	S8	-		-	----K	special function key 8
#key_sf9			ksf9	str	S9	-		-	----K	special function key 9
#key_sf10			ksf10	str	SA	-		-	----K	special function key 10
# AIX version 3 documents different codes for F11, F12 and does not mention
# F13-F64.  AIX version 4 uses the same naming for F0-F63 as above.
#key_f11			kf11	str	k<	-		-	-----	function key 11
#key_f12			kf12	str	k>	-		-	-----	function key 12
# Undocumented capabilities end here.
#key_action			kact	str	kJ	-		-	----K	sent by action key
# The IBM docs say these capabilities are for table-drawing, and are
# valid only for aixterm descriptions.
#enter_topline_mode		topl	str	tp	-		-	----K	start top-line mode
#enter_bottom_mode		btml	str	bm	-		-	----K	start bottom-line mode
#enter_rvert_mode		rvert	str	rv	-		-	----K	start right-vertical mode
#enter_lvert_mode		lvert	str	lv	-		-	----K	start left-vertical mode
#
#############################################################################
#
# ALIAS DECLARATIONS
#
# Here we set up aliases for translating extensions into standard terminfo.
#
#---------------------------------- Termcap aliases -------------------------
#
# BSD aliases:
#
# This is a common error in many termcap files.  We'll get notified during
# translation when this (or any other alias) fires.
#
capalias	sb	sr	BSD	scroll text down
#
# AT&T extensions:
#
# The old AT&T 5410, 5420, 5425, pc6300plus, 610, and s4 entries used a set of
# nonstandard capabilities.  Its signature is the KM capability, used to name
# some sort of keymap file.  EE, BO, CI, CV, XS, DS, FL and FE are in this
# set.  Comments in the original, and a little cross-checking with other AT&T
# documentation, seem to establish the following mappings:
#
capalias	BO	mr	AT&T	enter_reverse_mode
capalias	CI	vi	AT&T	cursor_invisible
capalias	CV	ve	AT&T	cursor_normal
capalias	DS	mh	AT&T	enter_dim_mode
#capalias	EE	me	AT&T	exit_attribute_mode	
capalias	FE	LF	AT&T	label_on
capalias	FL	LO	AT&T	label_off
capalias	XS	mk	AT&T	enter_secure_mode
#
# We comment out EE because the conflicting XENIX EE is more common in 
# old entries.
#
# XENIX extensions:
#
# These are the ones we know how to translate directly:
#
capalias	EE	mh	XENIX	exit_attribute_mode	
capalias	GE	ae	XENIX	exit_alt_charset_mode
capalias	GS	as	XENIX	enter_alt_charset_mode
capalias	CF	vi	XENIX	cursor_invis
capalias	CO	ve	XENIX	cursor_normal
capalias	EN	@7	XENIX	key_end
capalias	HM	kh	XENIX	key_home
capalias	LD	kL	XENIX	key_dl
capalias	PD	kN	XENIX	key_npage
capalias	PN	po	XENIX	prtr_off
capalias	PS	pf	XENIX	prtr_on
capalias	PU	kP	XENIX	key_ppage
capalias	RT	@8	XENIX	kent
capalias	UP	ku	XENIX	kcuu1
capalias	G6	IGNORE	XENIX	double-ACS_ULCORNER
capalias	G7	IGNORE	XENIX	double-ACS_LLCORNER
capalias	G5	IGNORE	XENIX	double-ACS_URCORNER
capalias	G8	IGNORE	XENIX	double-ACS_LRCORNER
capalias	Gr	IGNORE	XENIX	double-ACS_LTEE
capalias	Gr	IGNORE	XENIX	double-ACS_RTEE
capalias	Gu	IGNORE	XENIX	double-ACS_BTEE
capalias	Gd	IGNORE	XENIX	double ACS_TTEE
capalias	Gh	IGNORE	XENIX	double-ACS_HLINE
capalias	Gv	IGNORE	XENIX	double-ACS_VLINE
capalias	Gc	IGNORE	XENIX	double-ACS_PLUS
capalias	GG	IGNORE	XENIX	acs-glitch
#
# IBM extensions:
#
capalias	kq	%1	IBM	key_help
#
# Iris extensions:
#
capalias	HS	mh	IRIS	enter_dim_mode
#
# Tektronix extensions:
#
capalias	KA	k;	Tek	key_f10
capalias	KB	F1	Tek	key_f11
capalias	KC	F2	Tek	key_f12
capalias	KD	F3	Tek	key_f13
capalias	KE	F4	Tek	key_f14
capalias	KF	F5	Tek	key_f15
capalias	BC	Sb	Tek	set_background
capalias	FC	Sf	Tek	set_foreground
#
# There are also the following:
#
#	XENIX	XENIX variable name	name clash with terminfo?
#	-----	-------------------	-------------------------
#	CL	key_char_left
#	CR	key_char_right
#	CW	key_change_window
#	HP	??
#	LF	key_linefeed 		label_off
#	NU	key_next_unlocked_cell
#	PL	??
#	PR	??
#	RC	key_recalc		remove_clock
#	RF	key_toggle_ref		req_for_input
#	WL	key_word_left
#	WR	key_word_right
#
# If you know what any of the question-marked ones mean, please tell us.
#
#--------------------------------- Terminfo aliases ------------------------
#
# IBM extensions:
#
infoalias	font0	s0ds	IBM	set0_des_seq
infoalias	font1	s1ds	IBM	set1_des_seq
infoalias	font2	s2ds	IBM	set2_des_seq
infoalias	font3	s3ds	IBM	set3_des_seq
infoalias	kbtab	kcbt	IBM	key_backtab
infoalias	ksel	kslt	IBM	key_select
#
# Some others are identical to SVr4/XPG4 capabilities, in particular:
# kcmd, kend, khlp, and kf11...kf63.
#
#############################################################################
#
# The following sets edit modes for GNU EMACS
# Local Variables:
# case-fold-search:nil
# truncate-lines:t
# End:
