#!/usr/bin/env sh
# script to automate extracting blobs from an existing vendor bios

# SPDX-FileCopyrightText: 2022 Caleb La Grange <thonkpeasant@protonmail.com>
# SPDX-License-Identifier: GPL-3.0-only

board="${1}"
vendor_rom="${2}"

Print_help(){
	printf "Usage: ./blobutil extract {boardname} {path/to/vendor_rom}\n"
	printf "Example: ./blobutil extract x230 12mb_flash.bin\n"
	printf "\nYou need to specify exactly 2 arguments\n"
}

Fail(){
	printf "\nERROR: $@\n"
	exit 1
}

Build_deps(){
	if [ ! -d me_cleaner ]; then
		printf "downloading me_cleaner\n"
		./download me_cleaner || Fail 'could not download me_cleaner'
	else
		printf "me_cleaner already downloaded. Skipping.\n"
		printf "run ./download me_cleaner to manually overwrite\n"
	fi

	if [ ! -d coreboot/default ]; then
		printf "downloading coreboot\n"
		./download coreboot default || Fail 'could not download coreboot'
	else
		printf "coreboot already downloaded. Skipping.\n"
		printf "run ./download coreboot to manually overwrite\n"
	fi

	if ! [ -f coreboot/default/util/ifdtool/ifdtool ]; then
		printf "building ifdtool from coreboot\n"
		make -C coreboot/default/util/ifdtool || Fail 'could not build ifdtool'
	fi
}


Extract_blobs(){
	# TODO: find a better way to know which coreboot config to source
	set -- "resources/coreboot/${board}/config/*"
	. ${1} 2>/dev/null
	. "resources/coreboot/${board}/board.cfg"

	if [ "$CONFIG_HAVE_MRC" = "y" ]; then
		printf 'haswell board detected, downloading mrc\n'
		./download mrc || Fail 'could not download mrc, check network connection'
	fi

	_me_destination=${CONFIG_ME_BIN_PATH#../../}
	_gbe_destination=${CONFIG_GBE_BIN_PATH#../../}
	_ifd_destination=${CONFIG_IFD_BIN_PATH#../../}

	printf "extracting clean ime and modified ifd\n"
	./me_cleaner/me_cleaner.py -D ${_ifd_destination} -M ${_me_destination} ${vendor_rom} -t -r -S \
	|| ./resources/blobs/me7_update_parser.py -O ${_me_destination} ${vendor_rom} \
	|| Fail 'me_cleaner failed to extract blobs from rom'

	printf "extracting gigabit ethernet firmware"
	./coreboot/default/util/ifdtool/ifdtool -x ${vendor_rom}
	mv flashregion*gbe.bin ${_gbe_destination} || Fail 'could not extract gbe'
	
	# Cleans up other files extracted with ifdtool
	rm flashregion*.bin 2> /dev/null

	if [ -f ${_ifd_destination} ]; then
		printf "gbe, ifd, and me extracted to ${_me_destination%/*}\n"
	else
		printf "WARNING: Intel firmware descriptor could not be extracted with modified me\n"
	fi
}

if [ ! -f "${vendor_rom}" ] ; then
	Print_help
	exit 1
fi

if [ ! -d "resources/coreboot/${board}" ]; then
	Print_help
        printf "build/roms: Target %s does not exist in the %s build system. Skipping build.\n" "${projectname}" "${board}"
        exit 1
fi

if [ ! -f "resources/coreboot/${board}/board.cfg" ]; then
	Print_help
        printf "build/roms: Target %s does not have a board.cfg. Skipping build.\n" "${board}"
        exit 1
fi

printf "extracting blobs for ${board} from ${vendor_rom}\n"
Build_deps
Extract_blobs
