# samo_a1.map
# FLASH SIZE  = 64kB
# SECTOR SIZE =  4kB

0x1     mbr
0x0300  menu
0x02f0  version
0x1fe0  serial.header

0x2000  file-loader.header
0x2300  file-loader

0x4000  memory-test.header
0x4300  memory-test

0x6000  hw-test.header
0x6300  hw-test

# additional examples
# choose either:
#  1. the two *ERASE lines to remove a program
#     (*ERASE erases a 4 kByte sector)
#  2. the program.header and program lines
#     The program will remain in FLASH until it
#     is erased

#0x8000  *ERASE
#0x9000  *ERASE
#0x8000  a-test.header
#0x8300  a-test

#0xa000  *ERASE
#0xb000  *ERASE
#0xa000  other-test.header
#0xa300  other-test

# sample application
#0xc000  *ERASE
#0xd000  *ERASE
#0xc000  hello.header
#0xc300  hello

# for developers
#0xe000  *ERASE
#0xf000  *ERASE
#0xe000  rs232-loader.header
#0xe300  rs232-loader
