From ad812d008d570c1655bff13a9026f39a9efdcbc9 Mon Sep 17 00:00:00 2001
From: Leah Rowe <leah@libreboot.org>
Date: Tue, 31 Oct 2023 18:24:39 +0000
Subject: [PATCH 23/30] crank up vram allocation on more intel boards

these were added to libreboot, and it's a policy of
libreboot to max out the vram settings. this was
overlooked, in prior revisions and releases.

Signed-off-by: Leah Rowe <leah@libreboot.org>
---
 src/mainboard/dell/e6400/cmos.default                | 2 +-
 src/mainboard/dell/snb_ivb_workstations/cmos.default | 2 +-
 src/mainboard/hp/compaq_8200_elite_sff/cmos.default  | 2 +-
 src/mainboard/hp/compaq_elite_8300_usdt/cmos.default | 2 +-
 src/mainboard/hp/snb_ivb_laptops/cmos.default        | 1 +
 src/mainboard/lenovo/t420/cmos.default               | 1 +
 src/mainboard/lenovo/t420s/cmos.default              | 1 +
 src/mainboard/lenovo/t430/cmos.default               | 1 +
 src/mainboard/lenovo/t520/cmos.default               | 1 +
 src/mainboard/lenovo/t530/cmos.default               | 1 +
 src/mainboard/lenovo/x201/cmos.default               | 1 +
 src/mainboard/lenovo/x220/cmos.default               | 1 +
 12 files changed, 12 insertions(+), 4 deletions(-)

diff --git a/src/mainboard/dell/e6400/cmos.default b/src/mainboard/dell/e6400/cmos.default
index eeb6f47364..25dfa38cb5 100644
--- a/src/mainboard/dell/e6400/cmos.default
+++ b/src/mainboard/dell/e6400/cmos.default
@@ -2,4 +2,4 @@ boot_option=Fallback
 debug_level=Debug
 power_on_after_fail=Disable
 sata_mode=AHCI
-gfx_uma_size=32M
+gfx_uma_size=256M
diff --git a/src/mainboard/dell/snb_ivb_workstations/cmos.default b/src/mainboard/dell/snb_ivb_workstations/cmos.default
index ccc7e64625..7c97b84baf 100644
--- a/src/mainboard/dell/snb_ivb_workstations/cmos.default
+++ b/src/mainboard/dell/snb_ivb_workstations/cmos.default
@@ -3,5 +3,5 @@ debug_level=Debug
 power_on_after_fail=Disable
 nmi=Enable
 sata_mode=AHCI
-gfx_uma_size=128M
+gfx_uma_size=224M
 fan_full_speed=Disable
diff --git a/src/mainboard/hp/compaq_8200_elite_sff/cmos.default b/src/mainboard/hp/compaq_8200_elite_sff/cmos.default
index 6d27a79c66..4517ffc7c2 100644
--- a/src/mainboard/hp/compaq_8200_elite_sff/cmos.default
+++ b/src/mainboard/hp/compaq_8200_elite_sff/cmos.default
@@ -3,5 +3,5 @@ debug_level=Debug
 power_on_after_fail=Enable
 nmi=Enable
 sata_mode=AHCI
-gfx_uma_size=32M
+gfx_uma_size=224M
 psu_fan_lvl=3
diff --git a/src/mainboard/hp/compaq_elite_8300_usdt/cmos.default b/src/mainboard/hp/compaq_elite_8300_usdt/cmos.default
index 6f3cec735e..9fc4db2990 100644
--- a/src/mainboard/hp/compaq_elite_8300_usdt/cmos.default
+++ b/src/mainboard/hp/compaq_elite_8300_usdt/cmos.default
@@ -3,4 +3,4 @@ debug_level=Debug
 power_on_after_fail=Enable
 nmi=Enable
 sata_mode=AHCI
-gfx_uma_size=32M
+gfx_uma_size=224M
diff --git a/src/mainboard/hp/snb_ivb_laptops/cmos.default b/src/mainboard/hp/snb_ivb_laptops/cmos.default
index ad822d5043..89418a4cfc 100644
--- a/src/mainboard/hp/snb_ivb_laptops/cmos.default
+++ b/src/mainboard/hp/snb_ivb_laptops/cmos.default
@@ -3,3 +3,4 @@ debug_level=Debug
 power_on_after_fail=Disable
 nmi=Enable
 sata_mode=AHCI
+gfx_uma_size=224M
diff --git a/src/mainboard/lenovo/t420/cmos.default b/src/mainboard/lenovo/t420/cmos.default
index c011867916..83f590d39d 100644
--- a/src/mainboard/lenovo/t420/cmos.default
+++ b/src/mainboard/lenovo/t420/cmos.default
@@ -15,3 +15,4 @@ trackpoint=Enable
 hybrid_graphics_mode=Integrated Only
 usb_always_on=Disable
 me_state=Disabled
+gfx_uma_size=224M
diff --git a/src/mainboard/lenovo/t420s/cmos.default b/src/mainboard/lenovo/t420s/cmos.default
index c011867916..83f590d39d 100644
--- a/src/mainboard/lenovo/t420s/cmos.default
+++ b/src/mainboard/lenovo/t420s/cmos.default
@@ -15,3 +15,4 @@ trackpoint=Enable
 hybrid_graphics_mode=Integrated Only
 usb_always_on=Disable
 me_state=Disabled
+gfx_uma_size=224M
diff --git a/src/mainboard/lenovo/t430/cmos.default b/src/mainboard/lenovo/t430/cmos.default
index 55e1e6c04e..a72108f47e 100644
--- a/src/mainboard/lenovo/t430/cmos.default
+++ b/src/mainboard/lenovo/t430/cmos.default
@@ -16,3 +16,4 @@ backlight=Both
 usb_always_on=Disable
 hybrid_graphics_mode=Integrated Only
 me_state=Disabled
+gfx_uma_size=224M
diff --git a/src/mainboard/lenovo/t520/cmos.default b/src/mainboard/lenovo/t520/cmos.default
index b66f7034dc..a73ea6e9ee 100644
--- a/src/mainboard/lenovo/t520/cmos.default
+++ b/src/mainboard/lenovo/t520/cmos.default
@@ -16,3 +16,4 @@ backlight=Both
 hybrid_graphics_mode=Integrated Only
 usb_always_on=Disable
 me_state=Disabled
+gfx_uma_size=224M
diff --git a/src/mainboard/lenovo/t530/cmos.default b/src/mainboard/lenovo/t530/cmos.default
index b66f7034dc..a73ea6e9ee 100644
--- a/src/mainboard/lenovo/t530/cmos.default
+++ b/src/mainboard/lenovo/t530/cmos.default
@@ -16,3 +16,4 @@ backlight=Both
 hybrid_graphics_mode=Integrated Only
 usb_always_on=Disable
 me_state=Disabled
+gfx_uma_size=224M
diff --git a/src/mainboard/lenovo/x201/cmos.default b/src/mainboard/lenovo/x201/cmos.default
index 2cf484fd5a..46294d91ca 100644
--- a/src/mainboard/lenovo/x201/cmos.default
+++ b/src/mainboard/lenovo/x201/cmos.default
@@ -15,3 +15,4 @@ power_management_beeps=Enable
 low_battery_beep=Enable
 sata_mode=AHCI
 usb_always_on=Disable
+gfx_uma_size=128M
diff --git a/src/mainboard/lenovo/x220/cmos.default b/src/mainboard/lenovo/x220/cmos.default
index 52f303dfdb..92a2026542 100644
--- a/src/mainboard/lenovo/x220/cmos.default
+++ b/src/mainboard/lenovo/x220/cmos.default
@@ -14,3 +14,4 @@ fn_ctrl_swap=Disable
 sticky_fn=Disable
 trackpoint=Enable
 me_state=Disabled
+gfx_uma_size=224M
-- 
2.39.2

