(module Transformer_Ethernet_Bourns_SM51589PEL (layer F.Cu) (tedit 5E9997F2)
  (descr "350µH LAN 10/100/1000 Base-T Pulse Transformer 1CT:1CT")
  (tags "Transformer Ethernet Single Center-Tap")
  (attr smd)
  (fp_text reference REF** (at 0 -3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Transformer_Ethernet_Bourns_SM51589PEL (at 0 -1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 -3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6.6 -8.1) (end 6.6 -9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.4 -8.1) (end 6.6 -8.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.4 7.2) (end 8.4 -8.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.4 7.2) (end 8.4 7.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.4 8.75) (end 6.4 7.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.4 8.75) (end 6.4 8.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.4 7.2) (end -6.4 8.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.4 7.2) (end -6.4 7.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.6 -9.65) (end 6.6 -9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.6 -8.1) (end -6.6 -9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.6 -8.1) (end -8.4 -8.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.4 -8.1) (end -8.4 7.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.3 8.65) (end 6.3 7.125) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.3 8.65) (end 6.3 8.65) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.3 7.125) (end -6.3 8.65) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.5 -9.55) (end 6.5 -8.025) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.5 -9.55) (end 6.5 -9.55) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.5 -8.025) (end -6.5 -9.55) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.1 -8.025) (end -6.5 -8.025) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.15 -9.4) (end -5.35 -9.4) (layer F.Fab) (width 0.1))
  (fp_line (start 6.15 8.5) (end 6.15 -9.4) (layer F.Fab) (width 0.1))
  (fp_line (start -6.15 8.5) (end 6.15 8.5) (layer F.Fab) (width 0.1))
  (fp_line (start -6.15 -8.4) (end -6.15 8.5) (layer F.Fab) (width 0.1))
  (fp_line (start -6.15 -8.4) (end -5.35 -9.4) (layer F.Fab) (width 0.1))
  (pad 13 smd rect (at 7.3 6.525) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 7.3 5.255) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 7.3 3.985) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 7.3 2.715) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -7.3 6.525) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -7.3 5.255) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -7.3 3.985) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -7.3 2.715) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 7.3 -2.365) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 7.3 -7.445) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 7.3 -3.635) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 7.3 0.175) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 7.3 -6.175) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 7.3 1.445) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 7.3 -1.095) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 7.3 -4.905) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -7.3 1.445) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -7.3 -1.095) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -7.3 -2.365) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -7.3 0.175) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -7.3 -3.635) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -7.3 -4.905) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -7.3 -6.175) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -7.3 -7.445) (size 1.9 0.64) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Transformer_SMD.3dshapes/Transformer_Ethernet_Bourns_PT61017PEL.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
