(module USB3_B_XKB_U235-091N-4BLRC16-4-5 (layer F.Cu) (tedit 60F39768)
  (descr "USB3 B receptacle, Horizontal, through-hole, https://atta.szlcsc.com/upload/public/pdf/source/20190429/C388654_7F81AB876ECA2125365CFB417AE259C8.pdf")
  (tags "USB3-B receptacle horizontal through-hole")
  (fp_text reference REF** (at 0 -8.001) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB3_B_XKB_U235-091N-4BLRC16-4-5 (at -2.921 10.668) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 -8.001) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5 9.5) (end 5 -7) (layer F.CrtYd) (width 0.12))
  (fp_line (start -13.01 9.5) (end 5 9.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start -13.01 -7) (end 5 -7) (layer F.CrtYd) (width 0.12))
  (fp_line (start -13.01 -7) (end -13.01 9.5) (layer F.CrtYd) (width 0.12))
  (pad 3 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 2.5) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 2 2.5) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2 0) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at -2.71 -4.77) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at -2.71 7.27) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 4 1.25) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 4 -1.25) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 4 -3) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 4 5.5) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 4 3.75) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_B_OST_USB-B1HSxx_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
