(module USB3_A_Receptacle_XKB_U231-091N-4BLRA00-S-1 (layer F.Cu) (tedit 60DB53BD)
  (descr "USB3 type A Receptacle, Horizontal")
  (tags "usb A plug horizontal")
  (attr smd)
  (fp_text reference REF** (at 0 -8.382) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB3_A_Receptacle_XKB_U231-091N-4BLRA00-S-1 (at 0 8.89) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.175 7.85) (end 12.573 7.85) (layer F.CrtYd) (width 0.1))
  (fp_line (start -1.425 -4.61) (end -1.425 -5.29) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.425 4.61) (end -1.425 5.29) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.935 4.318) (end -2.935 3.718) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.175 -7.62) (end -3.175 7.85) (layer F.CrtYd) (width 0.1))
  (fp_line (start 12.573 -7.62) (end -3.175 -7.62) (layer F.CrtYd) (width 0.1))
  (fp_line (start 12.573 7.85) (end 12.573 -7.62) (layer F.CrtYd) (width 0.1))
  (fp_text user %R (at 9.075 0 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 5 smd rect (at -1.775 -4) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.775 -3 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.775 -2 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.775 -1 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -1.775 0 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.775 1 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.775 2 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.775 3 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.775 4 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 10 thru_hole oval (at 0.175 -6.4 90) (size 1.6 4) (drill oval 0.6 2.5) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 0.175 6.4 90) (size 1.6 4) (drill oval 0.6 2.5) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB3_A_Plug_Wuerth_692112030100_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
