[define]
DEVICE="V-Solution OLT V1600D_L"

[signal]
SIGNALMODE="HAL"
COLLECTORNAME="PONVsol"

SIGINDEX=".1.3.6.1.4.1.37950.1.1.5.12.2.1.8.1"

;OID below returns MACs for both active and non active ONUs
;which were registered on a PON port whenever
;if you'll decide to use it - comment the other MACINDEX OID and
;make sure to set GETACTIVEONUMACONLY to 0 in [misc] section
;but be aware - that may produce(unlikely, but...) duplicates in caches and unknown ONUs list
;recommended to use
MACINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.25.1.5"

;OID below returns MACs only for active ONUs 
;and an empty string for non active ONUs
;if you'll decide to use it
;make sure to set GETACTIVEONUMACONLY to 1 in [misc] section
;but be aware - that may put only active ONUs in caches and unknown ONUs list
;and LLID ifaces and deregistration reasons will probably not be shown
;MACINDEX=".1.3.6.1.4.1.37950.1.1.5.12.2.1.2.1.5"

SIGVALUE="STRING:"
MACVALUE="STRING:"
OFFSET="0"
OFFSETMODE="none"
DOWNVALUE=""

[system]
CPULOAD=".1.3.6.1.4.1.37950.1.1.5.10.12.3.0"
UPTIME=".1.3.6.1.2.1.1.3.0"
MEMLOAD=".1.3.6.1.4.1.37950.1.1.5.10.12.4.0"
TEMPERATURE=".1.3.6.1.4.1.37950.1.1.5.10.12.5.9.0"

[onu]
CONTROLMODE="VSOL_1600D"
DELETEPONINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.8.1.0"
DELETEONUINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.8.2.0"
DEREGPONINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.14.1.0"
DEREGONUINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.14.2.0"
RELOADPONINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.15.1.0"
RELOADONUINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.15.2.0"
DESCRPONINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.16.1.0"
DESCRONUINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.16.2.0"
DESCRSTRING=".1.3.6.1.4.1.37950.1.1.5.12.1.16.3.0"
DESCRCOMMIT=".1.3.6.1.4.1.37950.1.1.5.12.1.16.4.0"
DESCRIPTIONGET=".1.3.6.1.4.1.37950.1.1.5.12.1.25.1.9"
DESCRVALUE="STRING:"

[misc]
GETACTIVEONUMACONLY=0
DISTINDEX=".1.3.6.1.4.1.37950.1.1.5.12.1.25.1.17"
IFACEDESCR=".1.3.6.1.4.1.37950.1.1.5.10.1.2.1.1.2"
IFACECUSTOMDESCR=".1.3.6.1.4.1.37950.1.1.5.10.1.2.1.1.14"
DEREGREASON=".1.3.6.1.4.1.37950.1.1.5.12.1.25.1.15"
DISTVALUE="Gauge32:"
IFACEVALUE="STRING:"
DEREGVALUE="INTEGER:"
; FDBINDEX + DEC FDB MAC = pon port num + LLID num, aka "EPON0/1:18"
FDBINDEX=".1.3.6.1.4.1.37950.1.1.5.10.3.2.1.5"
FDBVALUE="EPON0/"
; DEC FDBINDEX = HEX FDB MAC
FDBMACINDEX=".1.3.6.1.4.1.37950.1.1.5.10.3.2.1.3"
FDBMACVALUE="Hex-STRING:"
; DEC FDBINDEX = VLAN ID
FDBVLANINDEX=".1.3.6.1.4.1.37950.1.1.5.10.3.2.1.2"
FDBVLANVALUE="INTEGER:"
LASTREGTIME=".1.3.6.1.4.1.37950.1.1.5.12.1.25.1.18"
LASTREGTIMEVAL="STRING:"
LASTDEREGTIME=".1.3.6.1.4.1.37950.1.1.5.12.1.25.1.19"
LASTDEREGTIMEVAL="STRING:"
LASTALIVETIME=".1.3.6.1.4.1.37950.1.1.5.12.1.25.1.20"
LASTALIVETIMEVAL="STRING:"
ONUTXSIGNAL=SIGINDEX=".1.3.6.1.4.1.37950.1.1.5.12.2.1.8.1.6"
ONUTXSIGNALVAL="STRING:"
ONURXSIGNAL=SIGINDEX=".1.3.6.1.4.1.37950.1.1.5.12.2.1.8.1.7"
ONURXSIGNALVAL="STRING:"
ONU_RENDER_MODE="mac"