Submitted By: Bruce Dubbs (bdubbs at liinuxfromscratch dot com)
Date: 2014-03-01
Initial Package Version: CVS_20101030
Origin: Self
Tanım: Removes ifconfig and hostname from the build
             due to duplication in inetutils

diff -Naur a/Makefile b/Makefile
--- a/Makefile	2009-12-31 14:38:02.000000000 -0600
+++ b/Makefile	2014-02-28 23:19:11.000000000 -0600
@@ -228,8 +228,8 @@
 	install -m 0755 -d ${BASEDIR}/sbin
 	install -m 0755 -d ${BASEDIR}/bin
 	install -m 0755 arp        ${BASEDIR}/sbin
-	install -m 0755 hostname   ${BASEDIR}/bin
-	install -m 0755 ifconfig   ${BASEDIR}/sbin
+#	install -m 0755 hostname   ${BASEDIR}/bin
+#	install -m 0755 ifconfig   ${BASEDIR}/sbin
 	install -m 0755 nameif     ${BASEDIR}/sbin
 	install -m 0755 netstat    ${BASEDIR}/bin
 	install -m 0755 plipconfig $(BASEDIR)/sbin
@@ -243,14 +243,6 @@
 ifeq ($(HAVE_MII),1)
 	install -m 0755 mii-tool   $(BASEDIR)/sbin
 endif
-	ln -fs hostname $(BASEDIR)/bin/dnsdomainname
-	ln -fs hostname $(BASEDIR)/bin/ypdomainname
-	ln -fs hostname $(BASEDIR)/bin/nisdomainname
-	ln -fs hostname $(BASEDIR)/bin/domainname
-ifeq ($(HAVE_AFDECnet),1)
-	ln -fs hostname $(BASEDIR)/bin/nodename
-endif
-
 savebin:
 	@for i in ${BASEDIR}/sbin/arp ${BASEDIR}/sbin/ifconfig \
                  ${BASEDIR}/bin/netstat \
diff -Naur a/config.in b/config.in
--- a/config.in	2008-10-02 21:09:57.000000000 -0500
+++ b/config.in	2014-02-28 23:18:31.000000000 -0600
@@ -68,8 +68,8 @@
 bool 'SLIP (serial line) support' HAVE_HWSLIP y
 bool 'PPP (serial line) support' HAVE_HWPPP y
 bool 'IPIP Tunnel support' HAVE_HWTUNNEL y
-bool 'STRIP (Metricom radio) support' HAVE_HWSTRIP y
-bool 'Token ring (generic) support' HAVE_HWTR y
+bool 'STRIP (Metricom radio) support' HAVE_HWSTRIP n
+bool 'Token ring (generic) support' HAVE_HWTR n
 bool 'AX25 (packet radio) support' HAVE_HWAX25 y
 bool 'Rose (packet radio) support' HAVE_HWROSE y
 bool 'NET/ROM (packet radio) support' HAVE_HWNETROM y
diff -Naur a/man/en_US/dnsdomainname.1 b/man/en_US/dnsdomainname.1
--- a/man/en_US/dnsdomainname.1	1998-08-10 15:51:04.000000000 -0500
+++ b/man/en_US/dnsdomainname.1	1969-12-31 18:00:00.000000000 -0600
@@ -1 +0,0 @@
-.so man1/hostname.1
diff -Naur a/man/en_US/domainname.1 b/man/en_US/domainname.1
--- a/man/en_US/domainname.1	1998-08-10 15:51:05.000000000 -0500
+++ b/man/en_US/domainname.1	1969-12-31 18:00:00.000000000 -0600
@@ -1 +0,0 @@
-.so man1/hostname.1
diff -Naur a/man/en_US/hostname.1 b/man/en_US/hostname.1
--- a/man/en_US/hostname.1	2008-10-02 18:16:59.000000000 -0500
+++ b/man/en_US/hostname.1	1969-12-31 18:00:00.000000000 -0600
@@ -1,213 +0,0 @@
-.TH HOSTNAME 1 "2008\-10\-03" "net\-tools" "Linux System Administrator's Manual"
-
-.SH NAME
-hostname \- show or set the system's host name
-.br
-domainname \- show or set the system's NIS/YP domain name
-.br
-dnsdomainname \- show the system's DNS domain name
-.br
-nisdomainname \- show or set system's NIS/YP domain name
-.br
-ypdomainname \- show or set the system's NIS/YP domain name
-.br
-nodename \- show or set the system's DECnet node name
-
-.SH SYNOPSIS
-.B hostname
-.RB [ \-v ]
-.RB [ \-a ]
-.RB [ \-\-alias ]
-.RB [ \-d ]
-.RB [ \-\-domain ]
-.RB [ \-f ]
-.RB [ \-\-fqdn ]
-.RB [ \-i ]
-.RB [ \-\-ip\-address ]
-.RB [ \-\-long ]
-.RB [ \-s ]
-.RB [ \-\-short ]
-.RB [ \-y ]
-.RB [ \-\-yp ]
-.RB [ \-\-nis ]
-.RB [ \-n ]
-.RB [ \-\-node ]
-
-.PP
-.B hostname 
-.RB [ \-v ]
-.RB [ \-F\ filename ]
-.RB [ \-\-file\ filename ]
-.RB [ hostname ]
-
-.PP
-.B domainname
-.RB [ \-v ]
-.RB [ \-F\ filename ]
-.RB [ \-\-file\ filename ]
-.RB [ name ]
-
-.PP 
-.B nodename
-.RB [ \-v ]
-.RB [ \-F\ filename ]
-.RB [ \-\-file\ filename ]
-.RB [ name ]
-
-.PP
-.B hostname
-.RB [ \-v ]
-.RB [ \-h ]
-.RB [ \-\-help ]
-.RB [ \-V ]
-.RB [ \-\-version ]
-
-.PP
-.B dnsdomainname
-.RB [ \-v ]
-.br
-.B nisdomainname
-.RB [ \-v ]
-.br
-.B ypdomainname
-.RB [ \-v ]
-
-.SH DESCRIPTION
-.B Hostname
-is the program that is used to either set or display
-the current host, domain or node name of the system.  These names are used
-by many of the networking programs to identify the machine. The domain 
-name is also used by NIS/YP.
-
-.SS "GET NAME"
-When called without any arguments, the program displays the current
-names:
-
-.LP
-.B hostname
-will print the name of the system as returned by the
-.BR gethostname (2)
-function.
-
-.LP
-.B "domainname, nisdomainname, ypdomainname"
-will print the name of the system as returned by the
-.BR getdomainname (2)
-function. This is also known as the YP/NIS domain name of the system.
-
-.LP
-.B nodename
-will print the DECnet node name of the system as returned by the
-.BR getnodename (2)
-function.
-
-.LP
-.B dnsdomainname
-will print the domain part of the FQDN (Fully Qualified Domain Name). The
-complete FQDN of the system is returned with
-.BR "hostname \-\-fqdn" .
-
-.SS "SET NAME"
-When called with one argument or with the 
-.B \-\-file
-option, the commands set the host name, the NIS/YP domain name or
-the node name. 
-
-.LP
-Note, that only the super-user can change the names. 
-
-.LP
-It is not possible to set the FQDN or the DNS domain name with the 
-.B dnsdomainname 
-command (see 
-.B "THE FQDN"
-below).
-
-.LP
-The host name is usually set once at system startup in
-.I /etc/rc.d/rc.inet1
-or
-.I /etc/init.d/boot
-(normally by reading the contents of a file which contains
-the host name, e.g. 
-.IR /etc/hostname ).
-
-.SS THE FQDN
-You can't change the FQDN (as returned by 
-.BR "hostname \-\-fqdn" ) 
-or the DNS domain name (as returned by
-.BR "dnsdomainname" ) 
-with this command. The FQDN of the system is the name that the
-.BR resolver (3)
-returns for the host name. 
-
-.LP
-Technically: The FQDN is the name
-.BR gethostbyname (2)
-returns for the host name returned by
-.BR gethostname (2).
-The DNS domain name is the part after the first dot.
-.LP
-Therefore it depends on the configuration (usually in 
-.IR /etc/host.conf )
-how you can change it. Usually (if the hosts file is parsed before DNS or 
-NIS) you can change it in 
-.IR /etc/hosts .
-
-
-.SH OPTIONS
-.TP
-.I "\-a, \-\-alias"
-Display the alias name of the host (if used).
-.TP
-.I "\-d, \-\-domain"
-Display the name of the DNS domain. Don't use the command
-.B domainname
-to get the DNS domain name because it will show the NIS domain name and
-not the DNS domain name. Use
-.B dnsdomainname 
-instead.
-.TP
-.I "\-F, \-\-file filename"
-Read the host name from the specified file. Comments (lines starting with
-a `#') are ignored.
-.TP
-.I "\-f, \-\-fqdn, \-\-long"
-Display the FQDN (Fully Qualified Domain Name). A FQDN consists of a
-short host name and the DNS domain name. Unless you are using bind or NIS
-for host lookups you can change the FQDN and the DNS domain name (which is
-part of the FQDN) in the \fI/etc/hosts\fR file.
-.TP
-.I "\-h, \-\-help"
-Print a usage message and exit.
-.TP
-.I "\-i, \-\-ip\-address"
-Display the IP address(es) of the host.
-.TP
-.I "\-n, \-\-node"
-Display the DECnet node name. If a parameter is given (or
-.B \-\-file name
-) the root can also set a new node name.
-.TP
-.I "\-s, \-\-short"
-Display the short host name. This is the host name cut at the first dot.
-.TP
-.I "\-V, \-\-version"
-Print version information on standard output and exit successfully.
-.TP
-.I "\-v, \-\-verbose"
-Be verbose and tell what's going on.
-.TP
-.I "\-y, \-\-yp, \-\-nis"
-Display the NIS domain name. If a parameter is given (or 
-.B \-\-file name
-) then root can also set a new NIS domain.
-.SH FILES
-.B /etc/hosts
-.SH AUTHOR
-Peter Tobias, <tobias@et\-inf.fho\-emden.de>
-.br
-Bernd Eckenfels, <net\-tools@lina.inka.de> (NIS and manpage).
-.br
-Steve Whitehouse, <SteveW@ACM.org> (DECnet support and manpage).
-
diff -Naur a/man/en_US/ifconfig.8 b/man/en_US/ifconfig.8
--- a/man/en_US/ifconfig.8	2008-10-02 18:16:59.000000000 -0500
+++ b/man/en_US/ifconfig.8	1969-12-31 18:00:00.000000000 -0600
@@ -1,229 +0,0 @@
-.TH IFCONFIG 8 "2008\-10\-03" "net\-tools" "Linux System Administrator's Manual"
-.SH NAME
-ifconfig \- configure a network interface
-.SH SYNOPSIS
-.B "ifconfig [-v] [-a] [-s] [interface]"
-.br
-.B "ifconfig [-v] interface [aftype] options | address ..."
-.SH DESCRIPTION
-.B Ifconfig
-is used to configure the kernel-resident network interfaces.  It is
-used at boot time to set up interfaces as necessary.  After that, it
-is usually only needed when debugging or when system tuning is needed.
-.LP
-If no arguments are given,
-.B ifconfig
-displays the status of the currently active interfaces.  If
-a single
-.B interface
-argument is given, it displays the status of the given interface
-only; if a single
-.B \-a
-argument is given, it displays the status of all interfaces, even
-those that are down.  Otherwise, it configures an interface.
-
-.SH Address Families
-If the first argument after the interface name is recognized as
-the name of a supported address family, that address family is
-used for decoding and displaying all protocol addresses.  Currently
-supported address families include
-.B inet
-(TCP/IP, default), 
-.B inet6
-(IPv6),
-.B ax25
-(AMPR Packet Radio),
-.B ddp
-(Appletalk Phase 2),
-.B ipx
-(Novell IPX) and
-.B netrom
-(AMPR Packet radio).
-.SH OPTIONS
-.TP
-.B -a
-display all interfaces which are currently available, even if down
-.TP
-.B -s
-display a short list (like netstat -i)
-.TP
-.B -v
-be more verbose for some error conditions
-.TP
-.B interface
-The name of the interface.  This is usually a driver name followed by
-a unit number, for example
-.B eth0
-for the first Ethernet interface. If your kernel supports alias interfaces,
-you can specify them with 
-.B eth0:0
-for the first alias of eth0. You can use them to assign a second address. To
-delete an alias interface use
-.BR "ifconfig eth0:0 down" .
-Note: for every scope (i.e. same net with address/netmask combination) all
-aliases are deleted, if you delete the first (primary).
-.TP
-.B up
-This flag causes the interface to be activated.  It is implicitly
-specified if an address is assigned to the interface.
-.TP
-.B down
-This flag causes the driver for this interface to be shut down.
-.TP
-.B "[\-]arp"
-Enable or disable the use of the ARP protocol on this interface.
-.TP
-.B "[\-]promisc"
-Enable or disable the
-.B promiscuous
-mode of the interface.  If selected, all packets on the network will
-be received by the interface.
-.TP
-.B "[\-]allmulti"
-Enable or disable 
-.B all-multicast
-mode.  If selected, all multicast packets on the network will be
-received by the interface.
-.TP
-.B "metric N"
-This parameter sets the interface metric.
-.TP
-.B "mtu N"
-This parameter sets the Maximum Transfer Unit (MTU) of an interface.
-.TP
-.B "dstaddr addr"
-Set the remote IP address for a point-to-point link (such as
-PPP).  This keyword is now obsolete; use the
-.B pointopoint
-keyword instead.
-.TP
-.B "netmask addr"
-Set the IP network mask for this interface.  This value defaults to the
-usual class A, B or C network mask (as derived from the interface IP
-address), but it can be set to any value.
-.TP
-.B "add addr/prefixlen"
-Add an IPv6 address to an interface. 
-.TP
-.B "del addr/prefixlen"
-Remove an IPv6 address from an interface.
-.TP
-.B "tunnel aa.bb.cc.dd"
-Create a new SIT (IPv6-in-IPv4) device, tunnelling to the given destination.
-.TP
-.B "irq addr"
-Set the interrupt line used by this device.  Not all devices can
-dynamically change their IRQ setting.
-.TP
-.B "io_addr addr"
-Set the start address in I/O space for this device. 
-.TP
-.B "mem_start addr"
-Set the start address for shared memory used by this device.  Only a
-few devices need this.
-.TP
-.B "media type"
-Set the physical port or medium type to be used by the device.  Not
-all devices can change this setting, and those that can vary in what
-values they support.  Typical values for
-.B type
-are 
-.B 10base2
-(thin Ethernet),
-.B 10baseT
-(twisted-pair 10Mbps Ethernet),
-.B AUI 
-(external transceiver) and so on.  The special medium type of
-.B auto
-can be used to tell the driver to auto-sense the media.  Again, not
-all drivers can do this.
-.TP
-.B "[\-]broadcast [addr]"
-If the address argument is given, set the protocol broadcast
-address for this interface.  Otherwise, set (or clear) the
-.B IFF_BROADCAST
-flag for the interface.
-.TP
-.B "[\-]pointopoint [addr]"
-This keyword enables the
-.B point-to-point
-mode of an interface, meaning that it is a direct link between two
-machines with nobody else listening on it.
-.br
-If the address argument is also given, set the protocol address of
-the other side of the link, just like the obsolete
-.B dstaddr
-keyword does.  Otherwise, set or clear the
-.B IFF_POINTOPOINT
-flag for the interface. 
-.TP
-.B hw class address
-Set the hardware address of this interface, if the device driver
-supports this operation.  The keyword must be followed by the
-name of the hardware class and the printable ASCII equivalent of
-the hardware address.  Hardware classes currently supported include
-.B ether
-(Ethernet),
-.B ax25
-(AMPR AX.25),
-.B ARCnet
-and
-.B netrom
-(AMPR NET/ROM).
-.TP
-.B multicast
-Set the multicast flag on the interface. This should not normally be needed
-as the drivers set the flag correctly themselves.
-.TP
-.B address
-The IP address to be assigned to this interface.
-.TP
-.B txqueuelen length
-Set the length of the transmit queue of the device. It is useful to set this
-to small values for slower devices with a high latency (modem links, ISDN)
-to prevent fast bulk transfers from disturbing interactive traffic like
-telnet too much. 
-.SH NOTES
-Since kernel release 2.2 there are no explicit interface statistics for
-alias interfaces anymore. The statistics printed for the original address
-are shared with all alias addresses on the same device. If you want per-address
-statistics you should add explicit accounting
-rules for the address using the 
-.BR ipchains (8)
-or
-.BR iptables (8)
-command.
-.LP
-Since net\-tools 1.60\-4 ifconfig is printing byte counters and human readable
-counters with IEC 60027-2 units. So 1 KiB are 2^10 byte. Note, the numbers 
-are truncated to one decimal (which can by quite a large error if you 
-consider 0.1 PiB is 112.589.990.684.262 bytes :)
-.LP
-Interrupt problems with Ethernet device drivers fail with EAGAIN
-.I (SIOCSIIFLAGS: Resource temporarily unavailable)
-it is most likely a interrupt conflict. See
-.I http://www.scyld.com/expert/irq\-conflict.html
-for more information.
-.SH FILES
-.I /proc/net/socket 
-.br
-.I /proc/net/dev
-.br
-.I /proc/net/if_inet6
-.SH BUGS
-While appletalk DDP and IPX addresses will be displayed they cannot be
-altered by this command.
-.SH SEE ALSO
-route(8), netstat(8), arp(8), rarp(8), ipchains(8), iptables(8), ifup(8), interfaces(5).
-.br
-http://physics.nist.gov/cuu/Units/binary.html - Prefixes for binary multiples
-.SH AUTHORS
-Fred N. van Kempen, <waltje@uwalt.nl.mugnet.org>
-.br
-Alan Cox, <Alan.Cox@linux.org>
-.br
-Phil Blundell, <Philip.Blundell@pobox.com>
-.br
-Andi Kleen
-.br
-Bernd Eckenfels, <net\-tools@lina.inka.de>
diff -Naur a/man/en_US/nisdomainname.1 b/man/en_US/nisdomainname.1
--- a/man/en_US/nisdomainname.1	1998-08-10 15:51:12.000000000 -0500
+++ b/man/en_US/nisdomainname.1	1969-12-31 18:00:00.000000000 -0600
@@ -1 +0,0 @@
-.so man1/hostname.1
diff -Naur a/man/en_US/ypdomainname.1 b/man/en_US/ypdomainname.1
--- a/man/en_US/ypdomainname.1	1998-08-10 15:51:16.000000000 -0500
+++ b/man/en_US/ypdomainname.1	1969-12-31 18:00:00.000000000 -0600
@@ -1 +0,0 @@
-.so man1/hostname.1
