# Architecture
BR2_arm=y
BR2_cortex_a17=y
BR2_ARM_FPU_NEON_VFPV4=y

# Linux headers same as kernel, a 4.12 series
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_4_12=y

# Bootloader
BR2_TARGET_UBOOT=y
BR2_TARGET_UBOOT_BUILD_SYSTEM_KCONFIG=y
BR2_TARGET_UBOOT_CUSTOM_VERSION=y
BR2_TARGET_UBOOT_CUSTOM_VERSION_VALUE="2017.11"
BR2_TARGET_UBOOT_BOARD_DEFCONFIG="tinker-rk3288"
BR2_TARGET_UBOOT_NEEDS_DTC=y
BR2_TARGET_UBOOT_NEEDS_OPENSSL=y
BR2_TARGET_UBOOT_FORMAT_DTB_IMG=y
BR2_TARGET_UBOOT_FORMAT_DTB_BIN=y
BR2_TARGET_UBOOT_SPL=y
BR2_TARGET_UBOOT_SPL_NAME="spl/u-boot-spl-dtb.bin"

# Kernel
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_VERSION=y
BR2_LINUX_KERNEL_CUSTOM_VERSION_VALUE="4.12"
BR2_LINUX_KERNEL_DEFCONFIG="multi_v7"
BR2_LINUX_KERNEL_UIMAGE=y
BR2_LINUX_KERNEL_UIMAGE_LOADADDR="0x02000000"
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="rk3288-tinker"
BR2_LINUX_KERNEL_INSTALL_TARGET=y

# Filesystem
BR2_TARGET_GENERIC_HOSTNAME="tinker-rk3288"
BR2_TARGET_GENERIC_ISSUE="Welcome to TINKER RK3288!"
BR2_TARGET_ROOTFS_EXT2=y
BR2_TARGET_ROOTFS_EXT2_4=y
BR2_TARGET_ROOTFS_EXT2_SIZE="512M"
BR2_PACKAGE_HOST_DOSFSTOOLS=y
BR2_PACKAGE_HOST_GENIMAGE=y
BR2_PACKAGE_HOST_MTOOLS=y
BR2_PACKAGE_HOST_UBOOT_TOOLS=y
BR2_ROOTFS_POST_IMAGE_SCRIPT="support/scripts/genimage.sh"
BR2_ROOTFS_POST_SCRIPT_ARGS="-c board/asus/tinker/genimage.cfg"
BR2_ROOTFS_POST_BUILD_SCRIPT="board/asus/tinker/post-build.sh"
