From 7030ea600d560026b91726f2eb79c856b813afa9 Mon Sep 17 00:00:00 2001
From: Dan Haab <dhaab@luxul.com>
Date: Mon, 9 Oct 2017 09:47:00 -0600
Subject: [PATCH] ARM: dts: BCM53573: Add DT for Luxul XAP-1440
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This is BCM53573 WiSoC based outdoor access point with an extra BCM43217
chipset used for 2.4 GHz.

Signed-off-by: Dan Haab <dhaab@luxul.com>
Acked-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/Makefile                    |  1 +
 arch/arm/boot/dts/bcm47189-luxul-xap-1440.dts | 50 +++++++++++++++++++++++++++
 2 files changed, 51 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm47189-luxul-xap-1440.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -95,6 +95,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm953012hr.dtb \
 	bcm953012k.dtb
 dtb-$(CONFIG_ARCH_BCM_53573) += \
+	bcm47189-luxul-xap-1440.dtb \
 	bcm47189-luxul-xap-810.dtb \
 	bcm47189-tenda-ac9.dtb \
 	bcm947189acdbmr.dtb
--- /dev/null
+++ b/arch/arm/boot/dts/bcm47189-luxul-xap-1440.dts
@@ -0,0 +1,50 @@
+/*
+ * Copyright 2017 Luxul Inc.
+ *
+ * Licensed under the ISC license.
+ */
+
+/dts-v1/;
+
+#include "bcm53573.dtsi"
+
+/ {
+	compatible = "luxul,xap-1440-v1", "brcm,bcm47189", "brcm,bcm53573";
+	model = "Luxul XAP-1440 V1";
+
+	chosen {
+		bootargs = "earlycon";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		wlan {
+			label = "bcm53xx:blue:wlan";
+			gpios = <&chipcommon 10 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+
+		system {
+			label = "bcm53xx:green:system";
+			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "timer";
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 7 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
