From 89b3b66aa955fed15585a4ba7120cf63f9e92aba Mon Sep 17 00:00:00 2001
From: Zhao Qiang <qiang.zhao@nxp.com>
Date: Thu, 13 Oct 2016 10:19:08 +0800
Subject: [PATCH 141/141] caam: add caam node for ls1088a

Signed-off-by: Zhao Qiang <qiang.zhao@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi |   43 ++++++++++++++++++++++++
 1 file changed, 43 insertions(+)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi
@@ -485,6 +485,49 @@
 			     <1 10 0x1>; /*Hypervisor PPI, edge triggered */
 	};
 
+	crypto: crypto@8000000 {
+		compatible = "fsl,sec-v5.4", "fsl,sec-v5.0",
+			     "fsl,sec-v4.0";
+		fsl,sec-era = <8>;
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges = <0x0 0x00 0x8000000 0x100000>;
+		reg = <0x00 0x8000000 0x0 0x100000>;
+		interrupts = <0 139 0x4>;
+
+		sec_jr0: jr@10000 {
+			compatible = "fsl,sec-v5.4-job-ring",
+				     "fsl,sec-v5.0-job-ring",
+				     "fsl,sec-v4.0-job-ring";
+			reg	   = <0x10000 0x10000>;
+			interrupts = <0 140 0x4>;
+		};
+
+		sec_jr1: jr@20000 {
+			compatible = "fsl,sec-v5.4-job-ring",
+				     "fsl,sec-v5.0-job-ring",
+				     "fsl,sec-v4.0-job-ring";
+			reg	   = <0x20000 0x10000>;
+			interrupts = <0 141 0x4>;
+		};
+
+		sec_jr2: jr@30000 {
+			compatible = "fsl,sec-v5.4-job-ring",
+				     "fsl,sec-v5.0-job-ring",
+				     "fsl,sec-v4.0-job-ring";
+			reg	   = <0x30000 0x10000>;
+			interrupts = <0 142 0x4>;
+		};
+
+		sec_jr3: jr@40000 {
+			compatible = "fsl,sec-v5.4-job-ring",
+				     "fsl,sec-v5.0-job-ring",
+				     "fsl,sec-v4.0-job-ring";
+			reg	   = <0x40000 0x10000>;
+			interrupts = <0 143 0x4>;
+		};
+	};
+
 	fsl_mc: fsl-mc@80c000000 {
 		compatible = "fsl,qoriq-mc";
 		#stream-id-cells = <2>;
