From caaab508dc2ba749d8394b5934353b1c47f37d75 Mon Sep 17 00:00:00 2001
From: Zhao Qiang <qiang.zhao@nxp.com>
Date: Sun, 9 Oct 2016 15:14:16 +0800
Subject: [PATCH 139/141] ls1088ardb: add ITS file

Signed-off-by: Zhao Qiang <qiang.zhao@nxp.com>
---
 kernel-ls1088a-rdb.its |   55 ++++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 55 insertions(+)
 create mode 100644 kernel-ls1088a-rdb.its

--- /dev/null
+++ b/kernel-ls1088a-rdb.its
@@ -0,0 +1,55 @@
+/*
+ * Copyright (C) 2015, Freescale Semiconductor
+ *
+ * Raghav Dogra	 <raghav@freescale.com>
+ *
+ * This file is licensed under the terms of the GNU General Public
+ * License version 2.  This program is licensed "as is" without any
+ * warranty of any kind, whether express or implied.
+ */
+
+/dts-v1/;
+
+/ {
+	description = "Simulator Image file for the LS1088A Linux Kernel";
+	#address-cells = <1>;
+
+	images {
+		kernel@1 {
+			description = "ARM64 Linux kernel";
+			data = /incbin/("./arch/arm64/boot/Image.gz");
+			type = "kernel";
+			arch = "arm64";
+			os = "linux";
+			compression = "gzip";
+			load = <0x80080000>;
+			entry = <0x80080000>;
+		};
+		fdt@1 {
+			description = "Flattened Device Tree blob";
+			data = /incbin/("./arch/arm64/boot/dts/freescale/fsl-ls1088a-rdb.dtb");
+			type = "flat_dt";
+			arch = "arm64";
+			compression = "none";
+			load = <0x90000000>;
+		};
+		ramdisk@1 {
+			description = "LS2 Ramdisk";
+			data = /incbin/("./fsl-image-core-ls1088ardb-be.ext2.gz");
+			type = "ramdisk";
+			arch = "arm64";
+			os = "linux";
+			compression = "none";
+		};
+	};
+
+	configurations {
+		default = "config@1";
+		config@1 {
+			description = "Boot Linux kernel";
+			kernel = "kernel@1";
+			fdt = "fdt@1";
+			ramdisk = "ramdisk@1";
+		};
+	};
+};
