From 32b74f9dc3caa9d3422ffa735db0ecf088dbffbe Mon Sep 17 00:00:00 2001
From: Georgii Staroselskii <gosha371@gmail.com>
Date: Wed, 7 Dec 2016 15:10:27 +0300
Subject: [PATCH] BCM270X_DT: overlays/*-overlay.dtb -> overlays/*.dtbo (#1752)

We now create overlays as .dtbo files.
---
 arch/arm/boot/dts/overlays/README | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -61,7 +61,7 @@ this becomes a line in config.txt:
 
     dtoverlay=lirc-rpi
 
-This causes the file /boot/overlays/lirc-rpi-overlay.dtb to be loaded. By
+This causes the file /boot/overlays/lirc-rpi.dtbo to be loaded. By
 default it will use GPIOs 17 (out) and 18 (in), but this can be modified using
 DT parameters:
 
