From: Gregory CLEMENT <gregory.clement@free-electrons.com>
Date: Thu, 4 Feb 2016 22:09:27 +0100
Subject: [PATCH] net: mvneta: Modify the queue related fields from each cpu

In the MVNETA_INTR_* registers, the queues related fields are per cpu,
according to the datasheet (comment in [] are added by me):
"In a multi-CPU system, bits of RX[or TX] queues for which the access by
the reading[or writing] CPU is disabled are read as 0, and cannot be
cleared[or written]."

That means that each time we want to manipulate these bits we had to do
it on each cpu and not only on the current cpu.

Signed-off-by: Gregory CLEMENT <gregory.clement@free-electrons.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -1041,6 +1041,43 @@ static void mvneta_set_autoneg(struct mv
 	}
 }
 
+static void mvneta_percpu_unmask_interrupt(void *arg)
+{
+	struct mvneta_port *pp = arg;
+
+	/* All the queue are unmasked, but actually only the ones
+	 * mapped to this CPU will be unmasked
+	 */
+	mvreg_write(pp, MVNETA_INTR_NEW_MASK,
+		    MVNETA_RX_INTR_MASK_ALL |
+		    MVNETA_TX_INTR_MASK_ALL |
+		    MVNETA_MISCINTR_INTR_MASK);
+}
+
+static void mvneta_percpu_mask_interrupt(void *arg)
+{
+	struct mvneta_port *pp = arg;
+
+	/* All the queue are masked, but actually only the ones
+	 * mapped to this CPU will be masked
+	 */
+	mvreg_write(pp, MVNETA_INTR_NEW_MASK, 0);
+	mvreg_write(pp, MVNETA_INTR_OLD_MASK, 0);
+	mvreg_write(pp, MVNETA_INTR_MISC_MASK, 0);
+}
+
+static void mvneta_percpu_clear_intr_cause(void *arg)
+{
+	struct mvneta_port *pp = arg;
+
+	/* All the queue are cleared, but actually only the ones
+	 * mapped to this CPU will be cleared
+	 */
+	mvreg_write(pp, MVNETA_INTR_NEW_CAUSE, 0);
+	mvreg_write(pp, MVNETA_INTR_MISC_CAUSE, 0);
+	mvreg_write(pp, MVNETA_INTR_OLD_CAUSE, 0);
+}
+
 /* This method sets defaults to the NETA port:
  *	Clears interrupt Cause and Mask registers.
  *	Clears all MAC tables.
@@ -1058,14 +1095,10 @@ static void mvneta_defaults_set(struct m
 	int max_cpu = num_present_cpus();
 
 	/* Clear all Cause registers */
-	mvreg_write(pp, MVNETA_INTR_NEW_CAUSE, 0);
-	mvreg_write(pp, MVNETA_INTR_OLD_CAUSE, 0);
-	mvreg_write(pp, MVNETA_INTR_MISC_CAUSE, 0);
+	on_each_cpu(mvneta_percpu_clear_intr_cause, pp, true);
 
 	/* Mask all interrupts */
-	mvreg_write(pp, MVNETA_INTR_NEW_MASK, 0);
-	mvreg_write(pp, MVNETA_INTR_OLD_MASK, 0);
-	mvreg_write(pp, MVNETA_INTR_MISC_MASK, 0);
+	on_each_cpu(mvneta_percpu_mask_interrupt, pp, true);
 	mvreg_write(pp, MVNETA_INTR_ENABLE, 0);
 
 	/* Enable MBUS Retry bit16 */
@@ -2531,31 +2564,6 @@ static int mvneta_setup_txqs(struct mvne
 	return 0;
 }
 
-static void mvneta_percpu_unmask_interrupt(void *arg)
-{
-	struct mvneta_port *pp = arg;
-
-	/* All the queue are unmasked, but actually only the ones
-	 * maped to this CPU will be unmasked
-	 */
-	mvreg_write(pp, MVNETA_INTR_NEW_MASK,
-		    MVNETA_RX_INTR_MASK_ALL |
-		    MVNETA_TX_INTR_MASK_ALL |
-		    MVNETA_MISCINTR_INTR_MASK);
-}
-
-static void mvneta_percpu_mask_interrupt(void *arg)
-{
-	struct mvneta_port *pp = arg;
-
-	/* All the queue are masked, but actually only the ones
-	 * maped to this CPU will be masked
-	 */
-	mvreg_write(pp, MVNETA_INTR_NEW_MASK, 0);
-	mvreg_write(pp, MVNETA_INTR_OLD_MASK, 0);
-	mvreg_write(pp, MVNETA_INTR_MISC_MASK, 0);
-}
-
 static void mvneta_start_dev(struct mvneta_port *pp)
 {
 	int cpu;
@@ -2606,13 +2614,10 @@ static void mvneta_stop_dev(struct mvnet
 	mvneta_port_disable(pp);
 
 	/* Clear all ethernet port interrupts */
-	mvreg_write(pp, MVNETA_INTR_MISC_CAUSE, 0);
-	mvreg_write(pp, MVNETA_INTR_OLD_CAUSE, 0);
+	on_each_cpu(mvneta_percpu_clear_intr_cause, pp, true);
 
 	/* Mask all ethernet port interrupts */
-	mvreg_write(pp, MVNETA_INTR_NEW_MASK, 0);
-	mvreg_write(pp, MVNETA_INTR_OLD_MASK, 0);
-	mvreg_write(pp, MVNETA_INTR_MISC_MASK, 0);
+	on_each_cpu(mvneta_percpu_mask_interrupt, pp, true);
 
 	mvneta_tx_reset(pp);
 	mvneta_rx_reset(pp);
@@ -2924,9 +2929,7 @@ static int mvneta_percpu_notifier(struct
 		}
 
 		/* Mask all ethernet port interrupts */
-		mvreg_write(pp, MVNETA_INTR_NEW_MASK, 0);
-		mvreg_write(pp, MVNETA_INTR_OLD_MASK, 0);
-		mvreg_write(pp, MVNETA_INTR_MISC_MASK, 0);
+		on_each_cpu(mvneta_percpu_mask_interrupt, pp, true);
 		napi_enable(&port->napi);
 
 
@@ -2941,14 +2944,8 @@ static int mvneta_percpu_notifier(struct
 		 */
 		mvneta_percpu_elect(pp);
 
-		/* Unmask all ethernet port interrupts, as this
-		 * notifier is called for each CPU then the CPU to
-		 * Queue mapping is applied
-		 */
-		mvreg_write(pp, MVNETA_INTR_NEW_MASK,
-			MVNETA_RX_INTR_MASK(rxq_number) |
-			MVNETA_TX_INTR_MASK(txq_number) |
-			MVNETA_MISCINTR_INTR_MASK);
+		/* Unmask all ethernet port interrupts */
+		on_each_cpu(mvneta_percpu_unmask_interrupt, pp, true);
 		mvreg_write(pp, MVNETA_INTR_MISC_MASK,
 			MVNETA_CAUSE_PHY_STATUS_CHANGE |
 			MVNETA_CAUSE_LINK_CHANGE |
@@ -2959,9 +2956,7 @@ static int mvneta_percpu_notifier(struct
 	case CPU_DOWN_PREPARE_FROZEN:
 		netif_tx_stop_all_queues(pp->dev);
 		/* Mask all ethernet port interrupts */
-		mvreg_write(pp, MVNETA_INTR_NEW_MASK, 0);
-		mvreg_write(pp, MVNETA_INTR_OLD_MASK, 0);
-		mvreg_write(pp, MVNETA_INTR_MISC_MASK, 0);
+		on_each_cpu(mvneta_percpu_mask_interrupt, pp, true);
 
 		napi_synchronize(&port->napi);
 		napi_disable(&port->napi);
@@ -2977,10 +2972,7 @@ static int mvneta_percpu_notifier(struct
 		/* Check if a new CPU must be elected now this on is down */
 		mvneta_percpu_elect(pp);
 		/* Unmask all ethernet port interrupts */
-		mvreg_write(pp, MVNETA_INTR_NEW_MASK,
-			MVNETA_RX_INTR_MASK(rxq_number) |
-			MVNETA_TX_INTR_MASK(txq_number) |
-			MVNETA_MISCINTR_INTR_MASK);
+		on_each_cpu(mvneta_percpu_unmask_interrupt, pp, true);
 		mvreg_write(pp, MVNETA_INTR_MISC_MASK,
 			MVNETA_CAUSE_PHY_STATUS_CHANGE |
 			MVNETA_CAUSE_LINK_CHANGE |
