/dts-v1/;

#include "vr9.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "FRITZ3370 - Fritz!Box WLAN 3370";

	chosen {
		bootargs = "console=ttyLTQ0,115200 ubi.mtd=1,512 root=/dev/mtdblock9";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;

		led-dsl = &dsl;
		led-internet = &info_green;
		led-wifi = &wifi;
	};

	memory@0 {
		reg = <0x0 0x8000000>;
	};

	fpi@10000000 {
		localbus@0 {
			nand-parts@0 {
				compatible = "gen_nand", "lantiq,nand-xway";
				bank-width = <2>;
				reg = <1 0x0 0x2000000>;
				#address-cells = <1>;
				#size-cells = <1>;

				partitions {
					compatible = "fixed-partitions";
					#address-cells = <1>;
					#size-cells = <1>;

					partition@0 {
						label = "kernel";
						reg = <0x0 0x400000>;
					};

					partition@400000 {
						label = "rootfs_ubi";
						reg = <0x400000 0x3000000>;
					};

					partition@3400000 {
						label = "vr9_firmware";
						reg = <0x3400000 0x400000>;
					};
					partition@3800000 {
						label = "reserved";
						reg = <0x3800000 0x3000000>;
					};
					partition@6800000 {
						label = "config";
						reg = <0x6800000 0x200000>;
					};
					partition@6a00000 {
						label = "nand-filesystem";
						reg = <0x6a00000 0x1600000>;
					};
				};
			};
		};

		gpio: pinmux@E100B10 {
			pinctrl-names = "default";
			pinctrl-0 = <&state_default>;

			state_default: pinmux {
				mdio {
					lantiq,groups = "mdio";
					lantiq,function = "mdio";
				};
				nand {
					lantiq,groups = "nand cle", "nand ale",
							"nand rd", "nand cs1", "nand rdy";
					lantiq,function = "ebu";
					lantiq,pull = <1>;
				};
				phy-rst {
					lantiq,pins = "io37", "io44";
					lantiq,pull = <0>;
					lantiq,open-drain = <0>;
					lantiq,output = <1>;
				};
				pcie-rst {
					lantiq,pins = "io38";
					lantiq,pull = <0>;
					lantiq,output = <1>;
				};
			};
			pins_spi_default: pins_spi_default {
				spi_in {
					lantiq,groups = "spi_di";
					lantiq,function = "spi";
				};
				spi_out {
					lantiq,groups = "spi_do", "spi_clk",
						"spi_cs4";
					lantiq,function = "spi";
					lantiq,output = <1>;
				};
			};
		};

		ifxhcd@E101000 {
			status = "okay";
			gpios = <&gpio 5 GPIO_ACTIVE_HIGH
				&gpio 14 GPIO_ACTIVE_HIGH>;
			lantiq,portmask = <0x3>;
		};
	};

	gphy-xrx200 {
		compatible = "lantiq,phy-xrx200";
		firmware = "lantiq/vr9_phy11g_a1x.bin";
		phys = [ 00 01 ];
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;
		power {
			label = "power";
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_POWER>;
		};
/*		wifi {
			label = "wifi";
			gpios = <&gpio 29 GPIO_ACTIVE_HIGH>;
			linux,code = <BTN_1>;
		};*/
	};

	gpio-leds {
		compatible = "gpio-leds";

		power_green: power {
			label = "fritz3370:green:power";
			gpios = <&gpio 32 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_red: power2 {
			label = "fritz3370:red:power";
			gpios = <&gpio 33 GPIO_ACTIVE_LOW>;
		};
		info_red {
			label = "fritz3370:red:info";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "fritz3370:green:wlan";
			gpios = <&gpio 35 GPIO_ACTIVE_LOW>;
		};
		dsl: dsl {
			label = "fritz3370:green:dsl";
			gpios = <&gpio 36 GPIO_ACTIVE_LOW>;
		};
		lan {
			label = "fritz3370:green:lan";
			gpios = <&gpio 38 GPIO_ACTIVE_LOW>;
		};
		info_green: info_green {
			label = "fritz3370:green:info";
			gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi {
	pinctrl-names = "default";
	pinctrl-0 = <&pins_spi_default>;

	status = "ok";

	m25p80@4 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <4 0>;
		spi-max-frequency = <1000000>;

		urlader: partition@0 {
			reg = <0x0 0x20000>;
			label = "urlader";
			read-only;
		};

		partition@20000 {
			reg = <0x20000 0x10000>;
			label = "tffs (1)";
			read-only;
		};

		partition@30000 {
			reg = <0x30000 0x10000>;
			label = "tffs (2)";
			read-only;
		};
	};
};

&eth0 {
	lan: interface@0 {
		compatible = "lantiq,xrx200-pdi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;
		mtd-mac-address = <&urlader 0x987>;
		mtd-mac-address-increment = <(-2)>;
		lantiq,switch;

		ethernet@0 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <0>;
			phy-mode = "rgmii";
			phy-handle = <&phy0>;
			gpios = <&gpio 37 GPIO_ACTIVE_HIGH>;
		};
		ethernet@1 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <1>;
			phy-mode = "rgmii";
			phy-handle = <&phy1>;
			gpios = <&gpio 44 GPIO_ACTIVE_HIGH>;
		};
		ethernet@2 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <2>;
			phy-mode = "gmii";
			phy-handle = <&phy11>;
		};
		ethernet@3 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <4>;
			phy-mode = "gmii";
			phy-handle = <&phy13>;
		};
	};

	mdio@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "lantiq,xrx200-mdio";
		phy0: ethernet-phy@0 {
			reg = <0x0>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy1: ethernet-phy@1 {
			reg = <0x1>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy11: ethernet-phy@11 {
			reg = <0x11>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy13: ethernet-phy@13 {
			reg = <0x13>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
	};
};

&pcie0 {
	pcie@0 {
		reg = <0 0 0 0 0>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		device_type = "pci";

		wifi@0,0 {
			compatible = "pci0,0";
			reg = <0 0 0 0 0>;
			qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:01:00.0.bin */
		};
	};
};
