From 6d665e736d0418ad5ffbfc49fc09aff30148b7a4 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 27 Apr 2016 12:01:41 +0100
Subject: [PATCH] BCM270X_DT: Fix codec use in hifiberry-dac overlay

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts
+++ b/arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts
@@ -13,7 +13,7 @@
 	};
 
 	fragment@1 {
-		target = <&soc>;
+		target-path = "/";
 		__overlay__ {
 			pcm5102a-codec {
 				#sound-dai-cells = <0>;
