From 1aeb63c52ade1219032161fcdb923aa4c62b3796 Mon Sep 17 00:00:00 2001
From: Prabhakar Kushwaha <prabhakar.kushwaha@nxp.com>
Date: Sun, 9 Oct 2016 14:52:49 +0800
Subject: [PATCH 137/141] armv8: ls1088a: Add PCIe compatible

commit: 1a089a382b187c80390f022d1e3f3749b2adcc64
[don't apply dtsi]

Signed-off-by: Prabhakar Kushwaha <prabhakar.kushwaha@nxp.com>
Integrated-by: Zhao Qiang <qiang.zhao@nxp.com>
---
 drivers/pci/host/pci-layerscape.c |    8 ++++++++
 1 file changed, 8 insertions(+)

--- a/drivers/pci/host/pci-layerscape.c
+++ b/drivers/pci/host/pci-layerscape.c
@@ -215,6 +215,13 @@ static struct ls_pcie_drvdata ls1046_drv
 	.ops = &ls_pcie_host_ops,
 };
 
+static struct ls_pcie_drvdata ls1088_drvdata = {
+	.lut_offset = 0x80000,
+	.ltssm_shift = 0,
+	.lut_dbg = 0x407fc,
+	.ops = &ls_pcie_host_ops,
+};
+
 static struct ls_pcie_drvdata ls2080_drvdata = {
 	.lut_offset = 0x80000,
 	.ltssm_shift = 0,
@@ -227,6 +234,7 @@ static const struct of_device_id ls_pcie
 	{ .compatible = "fsl,ls1021a-pcie", .data = &ls1021_drvdata },
 	{ .compatible = "fsl,ls1043a-pcie", .data = &ls1043_drvdata },
 	{ .compatible = "fsl,ls1046a-pcie", .data = &ls1046_drvdata },
+	{ .compatible = "fsl,ls1088a-pcie", .data = &ls1088_drvdata },
 	{ .compatible = "fsl,ls2080a-pcie", .data = &ls2080_drvdata },
 	{ .compatible = "fsl,ls2085a-pcie", .data = &ls2080_drvdata },
 	{ },
