From 9e4e6206c67ae11d68fc96882256f37c237087d4 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Mon, 22 Feb 2016 22:51:13 +0100
Subject: [PATCH] bgmac: support Ethernet device on BCM47094 SoC
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

It needs very similar workarounds to the one on BCM4707. It was tested
on D-Link DIR-885L home router.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/broadcom/bgmac.c | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/broadcom/bgmac.c
+++ b/drivers/net/ethernet/broadcom/bgmac.c
@@ -30,6 +30,7 @@ static inline bool bgmac_is_bcm4707_fami
 {
 	switch (bgmac->core->bus->chipinfo.id) {
 	case BCMA_CHIP_ID_BCM4707:
+	case BCMA_CHIP_ID_BCM47094:
 	case BCMA_CHIP_ID_BCM53018:
 		return true;
 	default:
@@ -1057,8 +1058,9 @@ static void bgmac_chip_reset(struct bgma
 	    (ci->id == BCMA_CHIP_ID_BCM53572 && ci->pkg == BCMA_PKG_ID_BCM47188))
 		iost &= ~BGMAC_BCMA_IOST_ATTACHED;
 
-	/* 3GMAC: for BCM4707, only do core reset at bgmac_probe() */
-	if (ci->id != BCMA_CHIP_ID_BCM4707) {
+	/* 3GMAC: for BCM4707 & BCM47094, only do core reset at bgmac_probe() */
+	if (ci->id != BCMA_CHIP_ID_BCM4707 &&
+	    ci->id != BCMA_CHIP_ID_BCM47094) {
 		flags = 0;
 		if (iost & BGMAC_BCMA_IOST_ATTACHED) {
 			flags = BGMAC_BCMA_IOCTL_SW_CLKEN;
