From 762eec4d6e09623bb5dad09a469a626a5d18ec98 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 19 May 2016 14:40:28 +0100
Subject: [PATCH] mmc: Apply QUIRK_BROKEN_ERASE to other capacities

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/mmc/card/block.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/mmc/card/block.c
+++ b/drivers/mmc/card/block.c
@@ -2559,6 +2559,10 @@ static const struct mmc_fixup blk_fixups
 	 */
 	MMC_FIXUP("SD16G", 0x41, 0x3432, add_quirk_mmc,
 		  MMC_QUIRK_ERASE_BROKEN),
+	MMC_FIXUP("SD32G", 0x41, 0x3432, add_quirk_mmc,
+		  MMC_QUIRK_ERASE_BROKEN),
+	MMC_FIXUP("SD64G", 0x41, 0x3432, add_quirk_mmc,
+		  MMC_QUIRK_ERASE_BROKEN),
 
 	END_FIXUP
 };
