/* This file is released into the public domain */

/dts-v1/;

#include "mt7620a.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "ralink,mt7620a-soc";
	model = "Netgear WN3000RPv3";

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	gpio-leds {
		compatible = "gpio-leds";

		power_g {
			label = "wn3000rpv3:green:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		power_r {
			label = "wn3000rpv3:red:power";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		client_g {
			label = "wn3000rpv3:green:client";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};

		client_r {
			label = "wn3000rpv3:red:client";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};

		router_g {
			label = "wn3000rpv3:green:router";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		router_r {
			label = "wn3000rpv3:red:router";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "wn3000rpv3:green:wps";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
		};

		l_arrow {
			label = "wn3000rpv3:blue:leftarrow";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};

		r_arrow {
			label = "wn3000rpv3:blue:rightarrow";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&spi0 {
	status = "okay";

	m25p80@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x30000>;
			read-only;
		};

		partition@30000 {
			label = "u-boot-env";
			reg = <0x30000 0x10000>;
			read-only;
		};

		partition@40000 {
			label = "firmware";
			reg = <0x40000 0x7b0000>;
		};

		art: partition@7f0000 {
			label = "art";
			reg = <0x7f0000 0x10000>;
			read-only;
		};
	};
};

&ethernet {
	mtd-mac-address = <&art 0x0>;
};

&wmac {
	mtd-mac-address = <&art 0x6>;
	ralink,mtd-eeprom = <&art 0x1000>;
};

&pinctrl {
	state_default: pinctrl0 {
		default {
			ralink,group = "i2c", "uartf", "spi refclk";
			ralink,function = "gpio";
		};
	};
};
