From 399409ff2196eb6d3f758579b63a1091fff93870 Mon Sep 17 00:00:00 2001
From: Jes Sorensen <Jes.Sorensen@redhat.com>
Date: Thu, 21 Jul 2016 15:23:16 -0400
Subject: [PATCH] rtl8xxxu: 8188eu use same ADDA on parameters as 8723au/8192cu

For ADDA setup the 8188eu looks to match the gen1 parts.

Signed-off-by: Jes Sorensen <Jes.Sorensen@redhat.com>
---
 drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8188e.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8188e.c
+++ b/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8188e.c
@@ -526,6 +526,10 @@ struct rtl8xxxu_fileops rtl8188eu_fops =
 	.rx_desc_size = sizeof(struct rtl8xxxu_rxdesc16),
 	.tx_desc_size = sizeof(struct rtl8xxxu_txdesc32),
 	.has_tx_report = 1,
+	.adda_1t_init = 0x0b1b25a0,
+	.adda_1t_path_on = 0x0bdb25a0,
+	.adda_2t_path_on_a = 0x04db25a4,
+	.adda_2t_path_on_b = 0x0b1b25a4,
 	/*
 	 * Use 9K for 8188e normal chip
 	 * Max RX buffer = 10K - max(TxReportSize(64*8), WOLPattern(16*24))
