From 514dc56068291b52b6f8bb2fe29d8755d6126283 Mon Sep 17 00:00:00 2001
From: Boris Brezillon <boris.brezillon@free-electrons.com>
Date: Tue, 22 Nov 2016 12:45:28 -0800
Subject: [PATCH] clk: bcm2835: Fix ->fixed_divider of pllh_aux

There is no fixed divider on pllh_aux.

Signed-off-by: Boris Brezillon <boris.brezillon@free-electrons.com>
Signed-off-by: Eric Anholt <eric@anholt.net>
Reviewed-by: Eric Anholt <eric@anholt.net>
Signed-off-by: Stephen Boyd <sboyd@codeaurora.org>
(cherry picked from commit f2a46926aba1f0c33944901d2420a6a887455ddc)
---
 drivers/clk/bcm/clk-bcm2835.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/clk/bcm/clk-bcm2835.c
+++ b/drivers/clk/bcm/clk-bcm2835.c
@@ -1663,7 +1663,7 @@ static const struct bcm2835_clk_desc clk
 		.a2w_reg = A2W_PLLH_AUX,
 		.load_mask = CM_PLLH_LOADAUX,
 		.hold_mask = 0,
-		.fixed_divider = 10),
+		.fixed_divider = 1),
 	[BCM2835_PLLH_PIX]	= REGISTER_PLL_DIV(
 		.name = "pllh_pix",
 		.source_pll = "pllh",
