From 2e2105a1578172eaf61e3b59a2c10c4fe04c21b9 Mon Sep 17 00:00:00 2001
From: Dan Haab <riproute@gmail.com>
Date: Fri, 4 May 2018 10:08:43 -0600
Subject: [PATCH] ARM: dts: BCM5301X: Add DT for Luxul XWR-3150 V1
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Luxul XWR-3150 is a wireless router similar to the XWR-3100 except:
1) It has more RAM
2) Its NAND controller in running in BCH8 mode
3) LAN ports LEDs are hardware controlled

Signed-off-by: Dan Haab <dan.haab@luxul.com>
Acked-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/Makefile                       |  1 +
 arch/arm/boot/dts/bcm47094-luxul-xwr-3150-v1.dts | 77 ++++++++++++++++++++++++
 2 files changed, 78 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm47094-luxul-xwr-3150-v1.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -88,6 +88,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm47094-luxul-abr-4500.dtb \
 	bcm47094-luxul-xbr-4500.dtb \
 	bcm47094-luxul-xwr-3100.dtb \
+	bcm47094-luxul-xwr-3150-v1.dtb \
 	bcm47094-netgear-r8500.dtb \
 	bcm94708.dtb \
 	bcm94709.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/bcm47094-luxul-xwr-3150-v1.dts
@@ -0,0 +1,77 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+/*
+ * Copyright 2018 Luxul Inc.
+ */
+
+/dts-v1/;
+
+#include "bcm47094.dtsi"
+#include "bcm5301x-nand-cs0-bch8.dtsi"
+
+/ {
+	compatible = "luxul,xwr-3150-v1", "brcm,bcm47094", "brcm,bcm4708";
+	model = "Luxul XWR-3150 V1";
+
+	chosen {
+		bootargs = "earlycon";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000
+		       0x88000000 0x18000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		power	{
+			label = "bcm53xx:green:power";
+			gpios = <&chipcommon 0 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-on";
+		};
+
+		usb3	{
+			label = "bcm53xx:green:usb3";
+			gpios = <&chipcommon 8 GPIO_ACTIVE_LOW>;
+			trigger-sources = <&ohci_port1>, <&ehci_port1>,
+					  <&xhci_port1>;
+			linux,default-trigger = "usbport";
+		};
+
+		status	{
+			label = "bcm53xx:green:status";
+			gpios = <&chipcommon 10 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "timer";
+		};
+
+		2ghz {
+			label = "bcm53xx:green:2ghz";
+			gpios = <&chipcommon 13 GPIO_ACTIVE_LOW>;
+		};
+
+		5ghz {
+			label = "bcm53xx:green:5ghz";
+			gpios = <&chipcommon 14 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 17 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&usb3 {
+	vcc-gpio = <&chipcommon 18 GPIO_ACTIVE_HIGH>;
+};
+
+&spi_nor {
+	status = "okay";
+};
