Description="my static bridge"
Interface=br0
Connection=bridge
BindsToInterfaces=(ens9 tap0)
## Use the MAC address of eth1 (may also be set to a literal MAC address)
MACAddress=ens9
IP=static
Address=('10.0.1.111/24')
Gateway='10.0.1.1'
DNS=('10.0.1.1')
## Ignore (R)STP and immediately activate the bridge
SkipForwardingDelay=yes
SkipNoCarrier=yes
