# Load firmware into the Xorcom Astribank device:
SUBSYSTEM=="usb", ACTION=="add", \
ENV{PRODUCT}=="e4e4/11[3456][013]/*", ENV{DEVTYPE}!="usb_interface", \
	RUN+="/usr/share/dahdi/xpp_fxloader udev $env{PRODUCT}"

# Hotplug hook for Astribank up/down
# If you need this functionality, copy the astribank_hook.sample
# to $XPP_INIT_DIR/astribank_hook
#
# By default XPP_INIT_DIR="/usr/share/dahdi"
KERNEL=="xbus*", RUN+="%E{XPP_INIT_DIR}/astribank_hook udev $kernel $sysfs{status} $sysfs{connector}"
