From de507dbe4db754f09905800e4d1629bd933d16f5 Mon Sep 17 00:00:00 2001
From: Kevin Mihelich <kevin@archlinuxarm.org>
Date: Sun, 7 May 2017 13:32:25 -0600
Subject: [PATCH 8/9] ARM: dove: enable ethernet on D3Plug

Signed-off-by: Kevin Mihelich <kevin@archlinuxarm.org>
---
 arch/arm/boot/dts/dove-d3plug.dts | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/arch/arm/boot/dts/dove-d3plug.dts b/arch/arm/boot/dts/dove-d3plug.dts
index 826026c28f90..a4c9963e1261 100644
--- a/arch/arm/boot/dts/dove-d3plug.dts
+++ b/arch/arm/boot/dts/dove-d3plug.dts
@@ -61,6 +61,13 @@ usb_power: regulator@1 {
 &uart0 { status = "okay"; };
 &sata0 { status = "okay"; };
 &i2c0 { status = "okay"; };
+&mdio { status = "okay"; };
+&eth { status = "okay"; };
+
+&ethphy {
+	compatible = "marvell,88e1310";
+	reg = <1>;
+};
 
 /* Samsung M8G2F eMMC */
 &sdio0 {
-- 
2.30.0

