From: "Jan Alexander Steffens (heftig)" <jan.steffens@gmail.com>
Date: Tue, 6 Mar 2018 23:39:47 +0100
Subject: [PATCH] Use Arch Linux' device access groups

  cdrom   → optical
  dialout → uucp
  tape    → storage
---
 rules.d/50-udev-default.rules.in | 14 +++++++-------
 sysusers.d/basic.conf.in       |  6 +++---
 2 files changed, 10 insertions(+), 10 deletions(-)

diff --git a/rules.d/50-udev-default.rules.in b/rules.d/50-udev-default.rules.in
index 191f56f42..f81c4d0fc 100644
--- a/rules.d/50-udev-default.rules.in
+++ b/rules.d/50-udev-default.rules.in
@@ -22,7 +22,7 @@ SUBSYSTEM=="tty", KERNEL=="sclp_line[0-9]*", GROUP="tty", MODE="0620"
 SUBSYSTEM=="tty", KERNEL=="ttysclp[0-9]*", GROUP="tty", MODE="0620"
 SUBSYSTEM=="tty", KERNEL=="3270/tty[0-9]*", GROUP="tty", MODE="0620"
 SUBSYSTEM=="vc", KERNEL=="vcs*|vcsa*", GROUP="tty"
-KERNEL=="tty[A-Z]*[0-9]|ttymxc[0-9]*|pppox[0-9]*|ircomm[0-9]*|noz[0-9]*|rfcomm[0-9]*", GROUP="dialout"
+KERNEL=="tty[A-Z]*[0-9]|ttymxc[0-9]*|pppox[0-9]*|ircomm[0-9]*|noz[0-9]*|rfcomm[0-9]*", GROUP="uucp"
 
 SUBSYSTEM=="mem", KERNEL=="mem|kmem|port", GROUP="kmem", MODE="0640"
 
@@ -57,13 +57,13 @@ KERNEL=="irlpt[0-9]*", GROUP="lp"
 SUBSYSTEM=="usb", ENV{DEVTYPE}=="usb_device", ENV{ID_USB_INTERFACES}=="*:0701??:*", GROUP="lp"
 
 SUBSYSTEM=="block", GROUP="disk"
-SUBSYSTEM=="block", KERNEL=="sr[0-9]*", GROUP="cdrom"
-SUBSYSTEM=="scsi_generic", SUBSYSTEMS=="scsi", ATTRS{type}=="4|5", GROUP="cdrom"
-KERNEL=="sch[0-9]*", GROUP="cdrom"
-KERNEL=="pktcdvd[0-9]*", GROUP="cdrom"
-KERNEL=="pktcdvd", GROUP="cdrom"
+SUBSYSTEM=="block", KERNEL=="sr[0-9]*", GROUP="optical"
+SUBSYSTEM=="scsi_generic", SUBSYSTEMS=="scsi", ATTRS{type}=="4|5", GROUP="optical"
+KERNEL=="sch[0-9]*", GROUP="optical"
+KERNEL=="pktcdvd[0-9]*", GROUP="optical"
+KERNEL=="pktcdvd", GROUP="optical"
 
-SUBSYSTEM=="scsi_generic|scsi_tape", SUBSYSTEMS=="scsi", ATTRS{type}=="1|8", GROUP="tape"
+SUBSYSTEM=="scsi_generic|scsi_tape", SUBSYSTEMS=="scsi", ATTRS{type}=="1|8", GROUP="storage"
 SUBSYSTEM=="scsi_generic", SUBSYSTEMS=="scsi", ATTRS{type}=="0", GROUP="disk"
 KERNEL=="qft[0-9]*|nqft[0-9]*|zqft[0-9]*|nzqft[0-9]*|rawqft[0-9]*|nrawqft[0-9]*", GROUP="disk"
 KERNEL=="loop-control", GROUP="disk", OPTIONS+="static_node=loop-control"
diff --git a/sysusers.d/basic.conf.in b/sysusers.d/basic.conf.in
index 8e358c02d..33e513a36 100644
--- a/sysusers.d/basic.conf.in
+++ b/sysusers.d/basic.conf.in
@@ -24,14 +24,14 @@ g utmp    -     -            -
 
 # Hardware access groups
 g audio   -     -            -
-g cdrom   -     -            -
-g dialout -     -            -
 g disk    -     -            -
 g input   -     -            -
 g kvm     -     -            -
 g lp      -     -            -
+g optical -     -            -
 g render  -     -            -
-g tape    -     -            -
+g storage -     -            -
+g uucp    -     -            -
 g video   -     -            -
 
 # Default group for normal users
