From d555bd69e792e42d94bd909b30d9bfef01db4e25 Mon Sep 17 00:00:00 2001
From: Eloi BAIL <eloi.bail@savoirfairelinux.com>
Date: Tue, 15 Sep 2015 11:38:22 -0400
Subject: [PATCH 2/3] rtpdec: inform jitter buffer size
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This commit print as AV_LOG_VERBOSE the jitter buffer
size. It might be the default value or the value set by application.

Signed-off-by: Eloi BAIL <eloi.bail@savoirfairelinux.com>
Signed-off-by: Martin Storsjö <martin@martin.st>
---
 libavformat/rtpdec.c | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/libavformat/rtpdec.c b/libavformat/rtpdec.c
index 5706f16..34c77f8 100644
--- a/libavformat/rtpdec.c
+++ b/libavformat/rtpdec.c
@@ -513,6 +513,10 @@ RTPDemuxContext *ff_rtp_parse_open(AVFormatContext *s1, AVStream *st,
     s->ic                  = s1;
     s->st                  = st;
     s->queue_size          = queue_size;
+
+    av_log(s->st ? s->st->codec : NULL, AV_LOG_VERBOSE,
+            "setting jitter buffer size to %d\n", s->queue_size);
+
     rtp_init_statistics(&s->statistics, 0);
     if (st) {
         switch (st->codec->codec_id) {
2.1.4
