ORGANIZATION_BLOCK OB 1
TITLE ="Main Program Sweep (Cycle)"
VERSION : 0.1


VAR_TEMP
  OB1_EV_CLASS : BYTE ;	//Bits 0-3 = 1 (Coming event), Bits 4-7 = 1 (Event class 1)
  OB1_SCAN_1 : BYTE ;	//1 (Cold restart scan 1 of OB 1), 3 (Scan 2-n of OB 1)
  OB1_PRIORITY : BYTE ;	//Priority of OB Execution
  OB1_OB_NUMBR : BYTE ;	//1 (Organization block 1, OB1)
  OB1_RESERVED_1 : BYTE ;	//Reserved for system
  OB1_RESERVED_2 : BYTE ;	//Reserved for system
  OB1_PREV_CYCLE : INT ;	//Cycle time of previous OB1 scan (milliseconds)
  OB1_MIN_CYCLE : INT ;	//Minimum cycle time of OB1 (milliseconds)
  OB1_MAX_CYCLE : INT ;	//Maximum cycle time of OB1 (milliseconds)
  OB1_DATE_TIME : DATE_AND_TIME ;	//Date and time OB1 started
END_VAR
BEGIN
NETWORK
TITLE =

      L     'ä'; 
      __ASSERT==	__ACCU 1, DW#16#E4
      L     'Ä'; 
      __ASSERT==	__ACCU 1, DW#16#C4
      L     'ö'; 
      __ASSERT==	__ACCU 1, DW#16#F6
      L     'Ö'; 
      __ASSERT==	__ACCU 1, DW#16#D6
      L     'ü'; 
      __ASSERT==	__ACCU 1, DW#16#FC
      L     'Ü'; 
      __ASSERT==	__ACCU 1, DW#16#DC
      L     'ß'; 
      __ASSERT==	__ACCU 1, DW#16#DF

      CALL SFC 46 // STOP CPU
END_ORGANIZATION_BLOCK

