From 56e74338a535cbcc2f2da08b1ea1a92920194364 Mon Sep 17 00:00:00 2001
From: Alexandra Yates <alexandra.yates@linux.intel.com>
Date: Tue, 3 Nov 2015 14:14:18 -0800
Subject: [PATCH] ahci: add new Intel device IDs

Adding Intel codename Lewisburg platform device IDs for SATA.

Signed-off-by: Alexandra Yates <alexandra.yates@linux.intel.com>
Signed-off-by: Tejun Heo <tj@kernel.org>
---
 drivers/ata/ahci.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/drivers/ata/ahci.c b/drivers/ata/ahci.c
index ff343c4..ff02bb4 100644
--- a/drivers/ata/ahci.c
+++ b/drivers/ata/ahci.c
@@ -314,6 +314,16 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	{ PCI_VDEVICE(INTEL, 0x1f37), board_ahci_avn }, /* Avoton RAID */
 	{ PCI_VDEVICE(INTEL, 0x1f3e), board_ahci_avn }, /* Avoton RAID */
 	{ PCI_VDEVICE(INTEL, 0x1f3f), board_ahci_avn }, /* Avoton RAID */
+	{ PCI_VDEVICE(INTEL, 0xa182), board_ahci }, /* Lewisburg AHCI*/
+	{ PCI_VDEVICE(INTEL, 0xa202), board_ahci }, /* Lewisburg AHCI*/
+	{ PCI_VDEVICE(INTEL, 0xa184), board_ahci }, /* Lewisburg RAID*/
+	{ PCI_VDEVICE(INTEL, 0xa204), board_ahci }, /* Lewisburg RAID*/
+	{ PCI_VDEVICE(INTEL, 0xa186), board_ahci }, /* Lewisburg RAID*/
+	{ PCI_VDEVICE(INTEL, 0xa206), board_ahci }, /* Lewisburg RAID*/
+	{ PCI_VDEVICE(INTEL, 0x2822), board_ahci }, /* Lewisburg RAID*/
+	{ PCI_VDEVICE(INTEL, 0x2826), board_ahci }, /* Lewisburg RAID*/
+	{ PCI_VDEVICE(INTEL, 0xa18e), board_ahci }, /* Lewisburg RAID*/
+	{ PCI_VDEVICE(INTEL, 0xa20e), board_ahci }, /* Lewisburg RAID*/
 	{ PCI_VDEVICE(INTEL, 0x2823), board_ahci }, /* Wellsburg RAID */
 	{ PCI_VDEVICE(INTEL, 0x2827), board_ahci }, /* Wellsburg RAID */
 	{ PCI_VDEVICE(INTEL, 0x8d02), board_ahci }, /* Wellsburg AHCI */
-- 
2.3.10

