From afd81dfadb70b6b4357fab2842b0ac62e48623a1 Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Sun, 5 Apr 2015 17:58:01 -0500
Subject: [PATCH 02/17] mainboards/lenovo/t400: Enable serial debug option for
 use with dock

Change-Id: I93fcc8147586c7ca32d4805579f4185cad3d61db
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/mainboard/lenovo/t400/Kconfig | 1 -
 1 file changed, 1 deletion(-)

diff --git a/src/mainboard/lenovo/t400/Kconfig b/src/mainboard/lenovo/t400/Kconfig
index e410f20..a1d0652 100644
--- a/src/mainboard/lenovo/t400/Kconfig
+++ b/src/mainboard/lenovo/t400/Kconfig
@@ -8,7 +8,6 @@ config BOARD_SPECIFIC_OPTIONS # dummy
 	select SOUTHBRIDGE_INTEL_I82801IX
 	select EC_LENOVO_PMH7
 	select EC_LENOVO_H8
-	select NO_UART_ON_SUPERIO
 	select DRIVERS_ICS_954309
 	select BOARD_ROMSIZE_KB_8192
 	select DRIVERS_GENERIC_IOAPIC
-- 
1.9.1

